{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["INSP FORM WITH DROP DOWN","Sheet1","FORMTAB PREP","MAIN LIST APP A","latest table 9","INSP FORM V4","INSP FORM V3","INSP FORM V2","ORIG INSP FORM"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"INSP FORM WITH DROP DOWN","index":0,"n_rows":347,"n_cols":9,"rows_kept":347,"cut":false,"hidden":false,"merged":[[318,1,336,1],[318,2,336,2],[337,1,343,1],[337,2,343,2],[253,1,257,1],[253,2,257,2],[258,1,263,1],[258,2,263,2],[264,1,271,1],[264,2,271,2],[290,1,297,1],[290,2,297,2],[298,1,301,1],[298,2,301,2],[302,1,306,1],[302,2,306,2],[88,1,93,1],[88,2,93,2],[125,1,130,1],[125,2,130,2],[131,1,153,1],[131,2,153,2],[94,1,98,1],[94,2,98,2],[99,1,104,1],[99,2,104,2],[105,1,113,1],[105,2,113,2],[114,1,124,1],[114,2,124,2],[67,1,72,1],[67,2,72,2],[73,1,81,1],[73,2,81,2],[82,1,87,1],[82,2,87,2],[39,1,45,1],[39,2,45,2],[46,1,56,1],[46,2,56,2],[57,1,66,1],[57,2,66,2],[10,0,16,8],[23,1,23,8],[34,1,38,1],[26,1,33,1],[26,2,33,2],[34,2,38,2],[175,1,180,1],[175,2,180,2],[181,1,185,1],[181,2,185,2],[154,1,174,1],[154,2,174,2],[307,1,312,1],[307,2,312,2],[313,1,317,1],[313,2,317,2],[187,2,204,2],[272,1,283,1],[272,2,283,2],[284,1,289,1],[284,2,289,2],[187,1,204,1],[205,1,227,1],[205,2,227,2],[228,1,235,1],[228,2,235,2],[236,1,252,1],[236,2,252,2]]}
[]
[null,null,null,null,null,null,"Form",null,"RSI-100-05"]
[null,null,null,null,null,null,"Original Date",null,"2019-08-04"]
[null,null,null,null,"Incoming Material ",null,"Revision Level",null,"VER 01-04-2021"]
[]
[null,null,null,null,"Inspection  Form",null,"Revision Date",null,"2021-05-27"]
[null,null,null,null,null,null,"Revised By",null,"T. SISTO"]
[null,null,null,null,null,null,"Approved By ",null,"J. BYRNE"]
[]
[]
["The tank car facility receiving parts, materials, or components must ensure that the manufactures or distributor provides any requested certificates of conformance, compliance (measurement, testing or mill test reports) required by the purchasing documents that provides the objective evidence that the required inspection points noted in Appendix A of RSI-100 were in fact performed. Each facility is responsible to address the CTC characteristics/requirements identified in Appendix A."]
[]
[]
[]
[]
[]
[]
["Purchasing Document(s): "]
[]
["Brand and Model number:"]
[]
["Facility Part Number: "]
[]
[null,"Inspection Method\nD – Document Verification (certificates) , I – Inspection Verification (Marking),  M – Measurement Verification Criteria"]
[]
["SELECT","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria","Certificate \nProvided\nY/N","Inspection\nPerfromed\nY/N","Pass\nFail\nP/F","Measurement \nEquipment\nID#"]
["Bolts","Bolts",null,"D","Material Specification"]
["Bolts",null,null,"I","Marking"]
["Bolts",null,null,"D","Thread Specification"]
["Bolts",null,null,"M","Overall Length"]
["Bolts",null,null,"M","Length of Threads"]
["Bolts",null,null,"M","Length of Shoulder"]
["Bolts",null,null,"M","Diameter"]
["Bolts",null,null,"M","Head size across flats"]
["BOV SADDLE"," Tank Bottom Outlet Valve Mounting \nSaddle Flange ",null,"D","AAR Device Approval  (If Contractually Specified)"]
["BOV SADDLE",null,null,"D","Material Specification"]
["BOV SADDLE",null,null,"I","Marking"]
["BOV SADDLE",null,null," M","Dimensional"]
["BOV SADDLE",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Eduction Pipe Assembly\n","Eduction Pipe Assembly\n",null,"D","Material Specification"]
["Eduction Pipe Assembly\n",null,null,"M","Length Overall"]
["Eduction Pipe Assembly\n",null,null,"D & M","Thread Specification (If Applicable)"]
["Eduction Pipe Assembly\n",null,null,"M","Diameter"]
["Eduction Pipe Assembly\n",null,null,"M","Thickness"]
["Eduction Pipe Assembly\n",null,null,"I & M","Machined Characteristics"]
["Eduction Pipe Assembly\n",null,null,"I","Weld Size and Type"]
["Excess Flow Valves, (Includes Spring Loaded)","Excess Flow Valves, (Includes Spring Loaded)",null,"D","AAR Device Approval "]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D","Model"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D ","Manufacturing Facility"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"M","Connection – Flange Dimensions"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D & M","Connection – Thread Specification"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D","Flow Rated Capacity"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D","OEM test certificate"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,0,"Each device must be marked to indicate as following:"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"I","Station stencil of the C4a or C4m facility"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"I","Model number correlated to the AAR design approval"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"I","Unique serial number"]
["Eyebolts","Eyebolts",null,"D","Material Specification"]
["Eyebolts",null,null,"I","Marking"]
["Eyebolts",null,null,"D","Thread Specification"]
["Eyebolts",null,null,"M","Overall Length"]
["Eyebolts",null,null,"M","Length of Threads"]
["Eyebolts",null,null,"M","Length of Shoulder"]
["Eyebolts",null,null,"M","Diameter"]
["Eyebolts",null,null,"M","Nut length across flats and thickness"]
["Eyebolts",null,null,"M","Nut style square/hex"]
["Eyebolts",null,null,"M","Eyelet ID/OD"]
["Fittings Plate with no nozzles\n","Fittings Plate with no nozzles\n",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Fittings Plate with no nozzles\n",null,null,"D","Material Specification"]
["Fittings Plate with no nozzles\n",null,null,"D","Thickness"]
["Fittings Plate with no nozzles\n",null,null,"D","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with no nozzles\n",null,null,"M","Gauge tapped threads"]
["Fittings Plate with no nozzles\n",null,null,"I &M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes"]
["Fittings Plate with Welded Nozzle(s)","Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D ","Material Specification"]
["Fittings Plate with Welded Nozzle(s)",null,null," M","Inside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null," M","Outside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null,"M","Thickness"]
["Fittings Plate with Welded Nozzle(s)",null,null,"M","Nozzle Dimensions"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Weld Size and Type"]
["Flanged Nozzle","Flanged Nozzle",null,"D","Material Specification"]
["Flanged Nozzle",null,null," M","Length Overall"]
["Flanged Nozzle",null,null,"M","Diameter"]
["Flanged Nozzle",null,null,"M","Thickness"]
["Flanged Nozzle",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern"]
["Flanged Nozzle",null,null,"I","Weld Size and Type (Forged or Cast)"]
["Flanges","Flanges",null,"D","Material Specification"]
["Flanges",null,null,"M","Inside Diameter (if required)"]
["Flanges",null,null,"M","Outside Diameter"]
["Flanges",null,null,"M","Thickness"]
["Flanges",null,null,"I","Sealing Style (Flat Face, Raised, or Tongue and Groove)"]
["Flanges",null,null,"I","Machined Characteristics /Gasket Surface"]
["Gaskets and O-Rings","Gaskets and O-Rings",null,"D","Material Specification"]
["Gaskets and O-Rings",null,null,"I","Marking (if applicable)"]
["Gaskets and O-Rings",null,null,"M","Inside Diameter"]
["Gaskets and O-Rings",null,null,"M","Outside Diameter"]
["Gaskets and O-Rings",null,null," M","Thickness"]
["Heat and Pressure Sensors","Heat and Pressure Sensors",null,"D","AAR Device Approval "]
["Heat and Pressure Sensors",null,null,"D","Model"]
["Heat and Pressure Sensors",null,null,"D","Manufacturing Facility"]
["Heat and Pressure Sensors",null,null,"M","Connection – Flange Dimensions"]
["Heat and Pressure Sensors",null,null,"D & M","Connection – Thread Specification"]
["Heat and Pressure Sensors",null,null,"D","OEM test certificate"]
["Hinged and Bolted \nManway Covers\n(Cast)\n","Hinged and Bolted \nManway Covers\n(Cast)\n",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"D","Material Specification"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"D ","Structural Integrity – Pressure Test "]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"D","Casting Quality"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"I","Bolt Pattern"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"I","Hinge Position"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"M","Bolt Slot Opening Dimensions"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"M","Gasket Groove Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Material Specification"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Nozzle Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Bolt Pattern"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Hinge Position"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Bolt Slot Opening Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," I","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)"]
["Hinged and Bolted Nozzle Assembly","Hinged and Bolted Nozzle Assembly",null,"D","Material Specification"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Length Overall"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Thickness"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Hinge Position"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Eyebolt Lug Position"]
["Liquid Level and Gauging Devices","Liquid Level and Gauging Devices",null,"D","AAR Device Approval "]
["Liquid Level and Gauging Devices",null,null,"D","Model"]
["Liquid Level and Gauging Devices",null,null,"D ","Manufacturing Facility"]
["Liquid Level and Gauging Devices",null,null,"M","Connection – Flange Dimensions & Bolt Circle"]
["Liquid Level and Gauging Devices",null,null,"M","Gage Rod Housing Length"]
["Liquid Level and Gauging Devices",null,null,"I","Gage Rod Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Float Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Body Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Bottom Spring"]
["Liquid Level and Gauging Devices",null,null,"I","Guide Tube Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Installation Correction Nut"]
["Liquid Level and Gauging Devices",null,null,"I","Specific Gravity Adjustment Bushing (as applicable)"]
["Liquid Level and Gauging Devices",null,null,"I","Cover with Chain"]
["Liquid Level and Gauging Devices",null,null,"D","Seal/O-Ring Dimensions"]
["Liquid Level and Gauging Devices",null,null,"D","Seal/O-Ring Material"]
["Liquid Level and Gauging Devices",null,null,"D","Magnetic Strength per OEM Specifications"]
["Liquid Level and Gauging Devices",null,null,"D","Commodity(s)"]
["Liquid Level and Gauging Devices",null,null,"D","Specific Gravity(s)"]
["Liquid Level and Gauging Devices",null,null,null,"Each device must be marked on the body as follows:"]
["Liquid Level and Gauging Devices",null,null,"I","Station stencil of the C4a or C4m facility"]
["Liquid Level and Gauging Devices",null,null,"I","Model number correlated to the AAR design approval"]
["Liquid Level and Gauging Devices",null,null,"I","Unique serial number"]
["Liquid Level and Gauging Devices",null,null,"I","Pressure rating (PSIG)"]
["Liquid/Vapor, and Sample Valves","Liquid/Vapor, and Sample Valves",null,"D","AAR Device Approval "]
["Liquid/Vapor, and Sample Valves",null,null,"D","Model"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Manufacturing Facility"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Connection – Flange Dimensions"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Connection – Thread Specification"]
["Liquid/Vapor, and Sample Valves",null,null,"M","Body Length"]
["Liquid/Vapor, and Sample Valves",null,null,"M","Body Diameter"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Port Opening Size"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Body Material"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Lining Material (If Applicable)"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Seal/O-Ring Material"]
["Liquid/Vapor, and Sample Valves",null,null,"D","OEM test certificate"]
["Liquid/Vapor, and Sample Valves",null,null,null,"Each Valve with a port free flow diameter greater than 0.75 inches = net free-flow area of more than 1/2 in.2 (323 mm2) must be marked to indicate the following:"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Unique serial number"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Pressure and/or temperature rating"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Type of trim and body material"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Note:  All pressure-retaining valve body castings shall be marked in accordance with the appropriate ASTM specification, including material identification with the grade symbols (e.g., WCB, WC9, CF8M, etc.), heat numbers, or a lot number traceable to either a heat number or month poured."]
["Liquid/Vapor, and Sample Valves",null,null,null,"For valve bodies constructed with more than one pressure-retaining casting, each casting must comply with the applicable ASTM marking requirement. This does not apply to bonnets, yokes, or body inserts."]
["Nut","Nut",null,"D","Material Specification"]
["Nut",null,null,"I","Marking"]
["Nut",null,null,"D","Thread Specification"]
["Nut",null,null,"M","Length across flats"]
["Nut",null,null,"M","Thickness"]
["Nut",null,null,"I","Style (Square or Hex)"]
["Pipe Plugs","Plugs w/Chains",null,"D","Material Specification (plug)"]
["Pipe Plugs",null,null,"D","Material Specification (chain)"]
["Plugs w/Chains",null,null,"D & M","Thread Specification"]
["Plugs w/Chains",null,null,"M","Diameter"]
["Plugs w/Chains",null,null,"M","Chain size"]
["Plugs w/Chains Attached to Flanges","Plugs w/Chains Attached to Flanges",null,null,"Refer to “Plugs w/Chains” and “Flange” requirements"]
["Pressure Regulator Valves","Pressure Regulator Valves",null,"D","AAR Device Approval "]
["Pressure Regulator Valves",null,null,"D","Model"]
["Pressure Regulator Valves",null,null,"D","Manufacturing Facility"]
["Pressure Regulator Valves",null,null,"I","Connection – Flange Dimensions"]
["Pressure Regulator Valves",null,null,"I","Connection – Thread Specification"]
["Pressure Regulator Valves",null,null,"M","Body Length"]
["Pressure Regulator Valves",null,null,"M","Body Diameter"]
["Pressure Regulator Valves",null,null,"D","Port Opening Size"]
["Pressure Regulator Valves",null,null,"D","Body Material"]
["Pressure Regulator Valves",null,null,"I","Lining Material (If Applicable)"]
["Pressure Regulator Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Pressure Regulator Valves",null,null,"D","Seal/O-Ring Material"]
["Pressure Regulator Valves",null,null,"D","OEM test certificate "]
["Pressure Regulator Valves",null,null,0,"Pressure Regulator Valves must be marked to indicate the following:"]
["Pressure Regulator Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Pressure Regulator Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Pressure Regulator Valves",null,null,"I","Unique serial number"]
["Pressure Regulator Valves",null,null,"I","Nominal standard set pressure"]
["Pressure Relief Valves","Pressure Relief Valves",null,"D","AAR Device Approval "]
["Pressure Relief Valves",null,null,"D","Model"]
["Pressure Relief Valves",null,null,"D","Manufacturing Facility"]
["Pressure Relief Valves",null,null,"I","Connection – Flange Dimensions"]
["Pressure Relief Valves",null,null,"I","Connection – Thread Specification"]
["Pressure Relief Valves",null,null,"M","Length"]
["Pressure Relief Valves",null,null,"M","Body Diameter"]
["Pressure Relief Valves",null,null,"D","Body Material"]
["Pressure Relief Valves",null,null,"I","Lining Material (If Applicable)"]
["Pressure Relief Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Pressure Relief Valves",null,null,"D","Seal/O-Ring Material"]
["Pressure Relief Valves",null,null,"D","Start to Discharge Pressure"]
["Pressure Relief Valves",null,null,"D","Vapor Tight Pressure"]
["Pressure Relief Valves",null,null,"D","Flow Rated Capacity"]
["Pressure Relief Valves",null,null,"D","OEM Test Certificate"]
["Pressure Relief Valves",null,null,"D","AAR Certificate of Test"]
["Pressure Relief Valves",null,null,0,"Pressure Relief Valves must be marked as follows:"]
["Pressure Relief Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Pressure Relief Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Pressure Relief Valves",null,null,"I","Unique serial number"]
["Pressure Relief Valves",null,null,"I","Set pressure, psi (or psi and kPa)"]
["Pressure Relief Valves",null,null,"I","Official flow capacity"]
["Pressure Relief Valves",null,null,"I","Flow rating pressure, psi (or psi and kPa)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material","Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"D","After 7/1/2021 - CID tag from C4a, C4m, or C5 facility"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"D","Material Specification and Grade"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Thickness"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Radius (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Rolling Direction (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Inside Diameter (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Outside Diameter (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Material Marking"]
["Rupture Disc Housing/Devices","Rupture Disc Housing/Devices",null,"D","AAR Device Approval"]
["Rupture Disc Housing/Devices",null,null,"D","Model"]
["Rupture Disc Housing/Devices",null,null,"D","Manufacturing Facility"]
["Rupture Disc Housing/Devices",null,null,"I","Connection – Flange Dimensions"]
["Rupture Disc Housing/Devices",null,null,"I","Connection – Thread Specification"]
["Rupture Disc Housing/Devices",null,null,"M","Body Length"]
["Rupture Disc Housing/Devices",null,null,"M","Body Diameter"]
["Rupture Disc Housing/Devices",null,null,"D","Port Opening Size"]
["Rupture Disc Housing/Devices",null,null,"D","Body Material"]
["Rupture Disc Housing/Devices",null,null,"I","Lining Material (If Applicable)"]
["Rupture Disc Housing/Devices",null,null,"D","Vapor Tight Pressure"]
["Rupture Disc Housing/Devices",null,null,"D","OEM Test Certificate"]
["Rupture Disc Housing/Devices",null,null,"D","AAR Certificate of Test"]
["Rupture Disc Housing/Devices",null,null,0,"Marked on the flange or on a nameplate:"]
["Rupture Disc Housing/Devices",null,null,"I","Manufacturer marking;"]
["Rupture Disc Housing/Devices",null,null,"I","Manufacturer’s design or type number and serial number; and"]
["Rupture Disc Housing/Devices",null,null,"I","Flow rating pressure, (PSI and/or kPa)"]
["Rupture Discs","Rupture Discs",null,"D","Model"]
["Rupture Discs",null,null,"D","Burst Rating"]
["Rupture Discs",null,null,"I","Structural Integrity"]
["Rupture Discs",null,null,"D","Certificate of Test (Per Lot)"]
["Rupture Discs",null,null,"I","Mark “TOP” on discharge side."]
["Secondary Closures - Caps with w/o Camlocks ","Secondary Closures - Caps with w/o Camlocks \nPCP 1 \n(3 if requried)",null,"D","Material Specification"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"D & M","Thread Specification"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"M","Thread Depth"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"M","Diameter"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"D","Casting Quality (if required)"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"M","Overall Height"]
["Segment\nWasher\n(used on rubber lined cars)","Segment Washer\n\n(used on rubber lined fittings)",null,"D","Material Specification"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"I","Marking (if required)"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Inside Radius"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Outside Radius"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Thickness"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Flatness"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Bolt Circle"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Bolt Hole Diameter"]
["Socket Head Cap Screws","Socket Head Cap Screws",null,"D","Material Specification"]
["Socket Head Cap Screws",null,null,"I","Finish (plain, zinc, other)"]
["Socket Head Cap Screws",null,null,"I ","Marking (if specified)"]
["Socket Head Cap Screws",null,null,"D","Thread Specification"]
["Socket Head Cap Screws",null,null,"M","Overall Length"]
["Socket Head Cap Screws",null,null,"M","Minimum Thread Length"]
["Socket Head Cap Screws",null,null,"M","Head Diameter"]
["Socket Head Cap Screws",null,null,"M","Screw Diameter"]
["Socket Head Cap Screws",null,null,"I","Head Type (plain, knurled)"]
["Socket Head Cap Screws",null,null,"M","Head Chamfer angle (30 or 45 degrees)"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Size"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Depth"]
["Spool","Spool",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Spool",null,null,"D","Material Specification"]
["Spool",null,null," M","Length Overall"]
["Spool",null,null,"M","Flange Dimensions"]
["Spool",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Spool",null,null,"M","Pipe Dimensions"]
["Stud Bolts","Stud Bolts",null,"D","Material Specification"]
["Stud Bolts",null,null,"I","Marking"]
["Stud Bolts",null,null,"D","Thread Specification"]
["Stud Bolts",null,null,"M","Overall Length"]
["Stud Bolts",null,null,"M","Length of Threads"]
["Stud Bolts",null,null,"M","Length of Shoulder"]
["Stud Bolts",null,null,"D","Stud end chamfer and radius configuration"]
["Stud Bolts",null,null,"M","Diameter"]
["Tank Bottom Sump \nNo washout","Tank Bottom Sump \nNo washout",null,"D ","Material Specification"]
["Tank Bottom Sump \nNo washout",null,null,"I","Marking"]
["Tank Bottom Sump \nNo washout",null,null," M","Dimensional"]
["Tank Bottom Sump \nNo washout",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Tank Bottom Sump \nwith washout","Tank Bottom Sump \nwith washout",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Tank Bottom Sump \nwith washout",null,null,"D","Material Specification"]
["Tank Bottom Sump \nwith washout",null,null,"I","Marking"]
["Tank Bottom Sump \nwith washout",null,null," M","Dimensional"]
["Tank Bottom Sump \nwith washout",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Tank Shell and Manway Nozzles ","Tank Shell and Manway Nozzles ",null,"D","Certified Mill Test Report"]
["Tank Shell and Manway Nozzles ",null,null,"D","Material Specification and Grade"]
["Tank Shell and Manway Nozzles ",null,null,"M","Thickness "]
["Tank Shell and Manway Nozzles ",null,null,"M","Radius (If Applicable)"]
["Tank Shell and Manway Nozzles ",null,null,"I","Rolling Direction (If Applicable)"]
["Tank Shell and Manway Nozzles ",null,null,"I","Material Marking"]
["Thermowell","Thermowell",null,"D","Material Specification"]
["Thermowell",null,null,"D","AAR Device Approval "]
["Thermowell",null,null,"M","Length Overall"]
["Thermowell",null,null,"D & M","Thread Specification"]
["Thermowell",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Vacuum Relief Valves","Vacuum Relief Valves",null,"D","AAR Device Approval "]
["Vacuum Relief Valves",null,null,"D","Model"]
["Vacuum Relief Valves",null,null,"D","Manufacturing Facility"]
["Vacuum Relief Valves",null,null,"I","Connection – Flange Dimensions"]
["Vacuum Relief Valves",null,null,"I","Connection – Thread Specification"]
["Vacuum Relief Valves",null,null,"M","Length"]
["Vacuum Relief Valves",null,null,"M","Body Diameter"]
["Vacuum Relief Valves",null,null,"D","Body Material"]
["Vacuum Relief Valves",null,null,"I","Weld Size / Type (if applicable)"]
["Vacuum Relief Valves",null,null,"I","Lining Material (If Applicable)"]
["Vacuum Relief Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Vacuum Relief Valves",null,null,"D","Seal/O-Ring Material"]
["Vacuum Relief Valves",null,null,"D","OEM Test Certificate"]
["Vacuum Relief Valves",null,null,null,"Vacuum Relief Valves must be marked as following:"]
["Vacuum Relief Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Vacuum Relief Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Vacuum Relief Valves",null,null,"I","Unique serial number"]
["Vacuum Relief Valves",null,null,"I","Type of trim and body material"]
["Vacuum Relief Valves",null,null,"I","Vacuum start to open pressure (PSIG)"]
["Washer","Washer",null,"D","Material Specification"]
["Washer",null,null,"I","Marking"]
["Washer",null,null,"M","Inside Diameter"]
["Washer",null,null,"M","Outside Diameter"]
["Washer",null,null,"M","Thickness"]
["Washer",null,null,"M","Flatness"]
["Washer",null,null,"I","Style (Flat or Spring or Lock)"]
["A_None"]
[]
[null,"INPSECTOR NAME:",null,null,"   SIGNATURE:",null,null,"DATE:"]

{"sheet":"Sheet1","index":1,"n_rows":320,"n_cols":9,"rows_kept":320,"cut":false,"hidden":false,"merged":[[80,1,88,1],[80,2,88,2],[89,1,99,1],[89,2,99,2],[100,1,105,1],[100,2,105,2],[42,1,47,1],[42,2,47,2],[48,1,56,1],[48,2,56,2],[57,1,62,1],[57,2,62,2],[293,1,311,1],[293,2,311,2],[312,1,318,1],[312,2,318,2],[265,1,272,1],[265,2,272,2],[273,1,276,1],[273,2,276,2],[277,1,281,1],[277,2,281,2],[282,1,287,1],[282,2,287,2],[288,1,292,1],[288,2,292,2],[259,1,264,1],[259,2,264,2],[211,1,227,1],[211,2,227,2],[228,1,232,1],[228,2,232,2],[233,1,238,1],[233,2,238,2],[239,1,246,1],[239,2,246,2],[247,1,258,1],[247,2,258,2],[180,1,202,1],[180,2,202,2],[203,1,210,1],[203,2,210,2],[106,1,128,1],[106,2,128,2],[129,1,149,1],[162,1,179,1],[162,2,179,2],[129,2,149,2],[150,1,155,1],[150,2,155,2],[156,1,160,1],[156,2,160,2],[69,1,73,1],[69,2,73,2],[74,1,79,1],[74,2,79,2],[63,1,68,1],[63,2,68,2],[21,1,31,1],[21,2,31,2],[32,1,41,1],[32,2,41,2],[1,1,8,1],[1,2,8,2],[9,1,13,1],[9,2,13,2],[14,1,20,1],[14,2,20,2]]}
["SELECT","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria","Certificate \nProvided\nY/N","Inspection\nPerfromed\nY/N","Pass\nFail\nP/F","Measurement \nEquipment\nID#"]
["Bolts","Bolts",null,"D","Material Specification"]
["Bolts",null,null,"I","Marking"]
["Bolts",null,null,"D","Thread Specification"]
["Bolts",null,null,"M","Overall Length"]
["Bolts",null,null,"M","Length of Threads"]
["Bolts",null,null,"M","Length of Shoulder"]
["Bolts",null,null,"M","Diameter"]
["Bolts",null,null,"M","Head size across flats"]
["BOV SADDLE"," Tank Bottom Outlet Valve Mounting \nSaddle Flange ",null,"D","AAR Device Approval  (If Contractually Specified)"]
["BOV SADDLE",null,null,"D","Material Specification"]
["BOV SADDLE",null,null,"I","Marking"]
["BOV SADDLE",null,null," M","Dimensional"]
["BOV SADDLE",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Eduction Pipe Assembly\n","Eduction Pipe Assembly\n",null,"D","Material Specification"]
["Eduction Pipe Assembly\n",null,null,"M","Length Overall"]
["Eduction Pipe Assembly\n",null,null,"D & M","Thread Specification (If Applicable)"]
["Eduction Pipe Assembly\n",null,null,"M","Diameter"]
["Eduction Pipe Assembly\n",null,null,"M","Thickness"]
["Eduction Pipe Assembly\n",null,null,"I & M","Machined Characteristics"]
["Eduction Pipe Assembly\n",null,null,"I","Weld Size and Type"]
["Excess Flow Valves, (Includes Spring Loaded)","Excess Flow Valves, (Includes Spring Loaded)",null,"D","AAR Device Approval "]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D","Model"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D ","Manufacturing Facility"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"M","Connection – Flange Dimensions"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D & M","Connection – Thread Specification"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D","Flow Rated Capacity"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"D","OEM test certificate"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,0,"Each device must be marked to indicate as following:"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"I","Station stencil of the C4a or C4m facility"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"I","Model number correlated to the AAR design approval"]
["Excess Flow Valves, (Includes Spring Loaded)",null,null,"I","Unique serial number"]
["Eyebolts","Eyebolts",null,"D","Material Specification"]
["Eyebolts",null,null,"I","Marking"]
["Eyebolts",null,null,"D","Thread Specification"]
["Eyebolts",null,null,"M","Overall Length"]
["Eyebolts",null,null,"M","Length of Threads"]
["Eyebolts",null,null,"M","Length of Shoulder"]
["Eyebolts",null,null,"M","Diameter"]
["Eyebolts",null,null,"M","Nut length across flats and thickness"]
["Eyebolts",null,null,"M","Nut style square/hex"]
["Eyebolts",null,null,"M","Eyelet ID/OD"]
["Fittings Plate with no nozzles\n","Fittings Plate with no nozzles\n",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Fittings Plate with no nozzles\n",null,null,"D","Material Specification"]
["Fittings Plate with no nozzles\n",null,null,"D","Thickness"]
["Fittings Plate with no nozzles\n",null,null,"D","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with no nozzles\n",null,null,"M","Gauge tapped threads"]
["Fittings Plate with no nozzles\n",null,null,"I &M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes"]
["Fittings Plate with Welded Nozzle(s)","Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D ","Material Specification"]
["Fittings Plate with Welded Nozzle(s)",null,null," M","Inside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null," M","Outside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null,"M","Thickness"]
["Fittings Plate with Welded Nozzle(s)",null,null,"M","Nozzle Dimensions"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Weld Size and Type"]
["Flanged Nozzle","Flanged Nozzle",null,"D","Material Specification"]
["Flanged Nozzle",null,null," M","Length Overall"]
["Flanged Nozzle",null,null,"M","Diameter"]
["Flanged Nozzle",null,null,"M","Thickness"]
["Flanged Nozzle",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern"]
["Flanged Nozzle",null,null,"I","Weld Size and Type (Forged or Cast)"]
["Flanges","Flanges",null,"D","Material Specification"]
["Flanges",null,null,"M","Inside Diameter (if required)"]
["Flanges",null,null,"M","Outside Diameter"]
["Flanges",null,null,"M","Thickness"]
["Flanges",null,null,"I","Sealing Style (Flat Face, Raised, or Tongue and Groove)"]
["Flanges",null,null,"I","Machined Characteristics /Gasket Surface"]
["Gaskets and O-Rings","Gaskets and O-Rings",null,"D","Material Specification"]
["Gaskets and O-Rings",null,null,"I","Marking (if applicable)"]
["Gaskets and O-Rings",null,null,"M","Inside Diameter"]
["Gaskets and O-Rings",null,null,"M","Outside Diameter"]
["Gaskets and O-Rings",null,null," M","Thickness"]
["Heat and Pressure Sensors","Heat and Pressure Sensors",null,"D","AAR Device Approval "]
["Heat and Pressure Sensors",null,null,"D","Model"]
["Heat and Pressure Sensors",null,null,"D","Manufacturing Facility"]
["Heat and Pressure Sensors",null,null,"M","Connection – Flange Dimensions"]
["Heat and Pressure Sensors",null,null,"D & M","Connection – Thread Specification"]
["Heat and Pressure Sensors",null,null,"D","OEM test certificate"]
["Hinged and Bolted \nManway Covers\n(Cast)\n","Hinged and Bolted \nManway Covers\n(Cast)\n",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"D","Material Specification"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"D ","Structural Integrity – Pressure Test "]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"D","Casting Quality"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"I","Bolt Pattern"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"I","Hinge Position"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"M","Bolt Slot Opening Dimensions"]
["Hinged and Bolted \nManway Covers\n(Cast)\n",null,null,"M","Gasket Groove Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Material Specification"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Nozzle Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Bolt Pattern"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Hinge Position"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Bolt Slot Opening Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," I","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)"]
["Hinged and Bolted Nozzle Assembly","Hinged and Bolted Nozzle Assembly",null,"D","Material Specification"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Length Overall"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Thickness"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Hinge Position"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Eyebolt Lug Position"]
["Liquid Level and Gauging Devices","Liquid Level and Gauging Devices",null,"D","AAR Device Approval "]
["Liquid Level and Gauging Devices",null,null,"D","Model"]
["Liquid Level and Gauging Devices",null,null,"D ","Manufacturing Facility"]
["Liquid Level and Gauging Devices",null,null,"M","Connection – Flange Dimensions & Bolt Circle"]
["Liquid Level and Gauging Devices",null,null,"M","Gage Rod Housing Length"]
["Liquid Level and Gauging Devices",null,null,"I","Gage Rod Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Float Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Body Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Bottom Spring"]
["Liquid Level and Gauging Devices",null,null,"I","Guide Tube Assembly"]
["Liquid Level and Gauging Devices",null,null,"I","Installation Correction Nut"]
["Liquid Level and Gauging Devices",null,null,"I","Specific Gravity Adjustment Bushing (as applicable)"]
["Liquid Level and Gauging Devices",null,null,"I","Cover with Chain"]
["Liquid Level and Gauging Devices",null,null,"D","Seal/O-Ring Dimensions"]
["Liquid Level and Gauging Devices",null,null,"D","Seal/O-Ring Material"]
["Liquid Level and Gauging Devices",null,null,"D","Magnetic Strength per OEM Specifications"]
["Liquid Level and Gauging Devices",null,null,"D","Commodity(s)"]
["Liquid Level and Gauging Devices",null,null,"D","Specific Gravity(s)"]
["Liquid Level and Gauging Devices",null,null,null,"Each device must be marked on the body as follows:"]
["Liquid Level and Gauging Devices",null,null,"I","Station stencil of the C4a or C4m facility"]
["Liquid Level and Gauging Devices",null,null,"I","Model number correlated to the AAR design approval"]
["Liquid Level and Gauging Devices",null,null,"I","Unique serial number"]
["Liquid Level and Gauging Devices",null,null,"I","Pressure rating (PSIG)"]
["Liquid/Vapor, and Sample Valves","Liquid/Vapor, and Sample Valves",null,"D","Specific gravity for which it is intended"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Model"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Manufacturing Facility"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Connection – Flange Dimensions"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Connection – Thread Specification"]
["Liquid/Vapor, and Sample Valves",null,null,"M","Body Length"]
["Liquid/Vapor, and Sample Valves",null,null,"M","Body Diameter"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Port Opening Size"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Body Material"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Lining Material (If Applicable)"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Liquid/Vapor, and Sample Valves",null,null,"D","Seal/O-Ring Material"]
["Liquid/Vapor, and Sample Valves",null,null,"D","OEM test certificate"]
["Liquid/Vapor, and Sample Valves",null,null,null,"Each Valve with a port free flow diameter greater than 0.75 inches = net free-flow area of more than 1/2 in.2 (323 mm2) must be marked to indicate the following:"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Unique serial number"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Pressure and/or temperature rating"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Type of trim and body material"]
["Liquid/Vapor, and Sample Valves",null,null,"I","Note:  All pressure-retaining valve body castings shall be marked in accordance with the appropriate ASTM specification, including material identification with the grade symbols (e.g., WCB, WC9, CF8M, etc.), heat numbers, or a lot number traceable to either a heat number or month poured."]
["Liquid/Vapor, and Sample Valves",null,null,null,"For valve bodies constructed with more than one pressure-retaining casting, each casting must comply with the applicable ASTM marking requirement. This does not apply to bonnets, yokes, or body inserts."]
["Nut","Nut",null,"D","Material Specification"]
["Nut",null,null,"I","Marking"]
["Nut",null,null,"D","Thread Specification"]
["Nut",null,null,"M","Length across flats"]
["Nut",null,null,"M","Thickness"]
["Nut",null,null,"I","Style (Square or Hex)"]
["Pipe Plugs","Plugs w/Chains",null,"D","Material Specification (plug)"]
["Pipe Plugs",null,null,"D","Material Specification (chain)"]
["Plugs w/Chains",null,null,"D & M","Thread Specification"]
["Plugs w/Chains",null,null,"M","Diameter"]
["Plugs w/Chains",null,null,"M","Chain size"]
["Plugs w/Chains Attached to Flanges","Plugs w/Chains Attached to Flanges",null,null,"Refer to “Plugs w/Chains” and “Flange” requirements"]
["Pressure Regulator Valves","Pressure Regulator Valves",null,"D","AAR Device Approval "]
["Pressure Regulator Valves",null,null,"D","Model"]
["Pressure Regulator Valves",null,null,"D","Manufacturing Facility"]
["Pressure Regulator Valves",null,null,"I","Connection – Flange Dimensions"]
["Pressure Regulator Valves",null,null,"I","Connection – Thread Specification"]
["Pressure Regulator Valves",null,null,"M","Body Length"]
["Pressure Regulator Valves",null,null,"M","Body Diameter"]
["Pressure Regulator Valves",null,null,"D","Port Opening Size"]
["Pressure Regulator Valves",null,null,"D","Body Material"]
["Pressure Regulator Valves",null,null,"I","Lining Material (If Applicable)"]
["Pressure Regulator Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Pressure Regulator Valves",null,null,"D","Seal/O-Ring Material"]
["Pressure Regulator Valves",null,null,"D","OEM test certificate "]
["Pressure Regulator Valves",null,null,0,"Pressure Regulator Valves must be marked to indicate the following:"]
["Pressure Regulator Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Pressure Regulator Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Pressure Regulator Valves",null,null,"I","Unique serial number"]
["Pressure Regulator Valves",null,null,"I","Nominal standard set pressure"]
["Pressure Relief Valves","Pressure Relief Valves",null,"D","AAR Device Approval "]
["Pressure Relief Valves",null,null,"D","Model"]
["Pressure Relief Valves",null,null,"D","Manufacturing Facility"]
["Pressure Relief Valves",null,null,"I","Connection – Flange Dimensions"]
["Pressure Relief Valves",null,null,"I","Connection – Thread Specification"]
["Pressure Relief Valves",null,null,"M","Length"]
["Pressure Relief Valves",null,null,"M","Body Diameter"]
["Pressure Relief Valves",null,null,"D","Body Material"]
["Pressure Relief Valves",null,null,"I","Lining Material (If Applicable)"]
["Pressure Relief Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Pressure Relief Valves",null,null,"D","Seal/O-Ring Material"]
["Pressure Relief Valves",null,null,"D","Start to Discharge Pressure"]
["Pressure Relief Valves",null,null,"D","Vapor Tight Pressure"]
["Pressure Relief Valves",null,null,"D","Flow Rated Capacity"]
["Pressure Relief Valves",null,null,"D","OEM Test Certificate"]
["Pressure Relief Valves",null,null,"D","AAR Certificate of Test"]
["Pressure Relief Valves",null,null,0,"Pressure Relief Valves must be marked as follows:"]
["Pressure Relief Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Pressure Relief Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Pressure Relief Valves",null,null,"I","Unique serial number"]
["Pressure Relief Valves",null,null,"I","Set pressure, psi (or psi and kPa)"]
["Pressure Relief Valves",null,null,"I","Official flow capacity"]
["Pressure Relief Valves",null,null,"I","Flow rating pressure, psi (or psi and kPa)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material","Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"D","After 7/1/2021 - CID tag from C4a, C4m, or C5 facility"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"D","Material Specification and Grade"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Thickness"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Radius (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Rolling Direction (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Inside Diameter (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Outside Diameter (If Applicable)"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Material Marking"]
["Rupture Disc Housing/Devices","Rupture Disc Housing/Devices",null,"D","AAR Device Approval"]
["Rupture Disc Housing/Devices",null,null,"D","Model"]
["Rupture Disc Housing/Devices",null,null,"D","Manufacturing Facility"]
["Rupture Disc Housing/Devices",null,null,"I","Connection – Flange Dimensions"]
["Rupture Disc Housing/Devices",null,null,"I","Connection – Thread Specification"]
["Rupture Disc Housing/Devices",null,null,"M","Body Length"]
["Rupture Disc Housing/Devices",null,null,"M","Body Diameter"]
["Rupture Disc Housing/Devices",null,null,"D","Port Opening Size"]
["Rupture Disc Housing/Devices",null,null,"D","Body Material"]
["Rupture Disc Housing/Devices",null,null,"I","Lining Material (If Applicable)"]
["Rupture Disc Housing/Devices",null,null,"D","Vapor Tight Pressure"]
["Rupture Disc Housing/Devices",null,null,"D","OEM Test Certificate"]
["Rupture Disc Housing/Devices",null,null,"D","AAR Certificate of Test"]
["Rupture Disc Housing/Devices",null,null,0,"Marked on the flange or on a nameplate:"]
["Rupture Disc Housing/Devices",null,null,"I","Manufacturer marking;"]
["Rupture Disc Housing/Devices",null,null,"I","Manufacturer’s design or type number and serial number; and"]
["Rupture Disc Housing/Devices",null,null,"I","Flow rating pressure, (PSI and/or kPa)"]
["Rupture Discs","Rupture Discs",null,"D","Model"]
["Rupture Discs",null,null,"D","Burst Rating"]
["Rupture Discs",null,null,"I","Structural Integrity"]
["Rupture Discs",null,null,"D","Certificate of Test (Per Lot)"]
["Rupture Discs",null,null,"I","Mark “TOP” on discharge side."]
["Secondary Closures - Caps with w/o Camlocks ","Secondary Closures - Caps with w/o Camlocks \nPCP 1 \n(3 if requried)",null,"D","Material Specification"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"D & M","Thread Specification"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"M","Thread Depth"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"M","Diameter"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"D","Casting Quality (if required)"]
["Secondary Closures - Caps with w/o Camlocks ",null,null,"M","Overall Height"]
["Segment\nWasher\n(used on rubber lined cars)","Segment Washer\n\n(used on rubber lined fittings)",null,"D","Material Specification"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"I","Marking (if required)"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Inside Radius"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Outside Radius"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Thickness"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Flatness"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Bolt Circle"]
["Segment\nWasher\n(used on rubber lined cars)",null,null,"M","Bolt Hole Diameter"]
["Socket Head Cap Screws","Socket Head Cap Screws",null,"D","Material Specification"]
["Socket Head Cap Screws",null,null,"I","Finish (plain, zinc, other)"]
["Socket Head Cap Screws",null,null,"I ","Marking (if specified)"]
["Socket Head Cap Screws",null,null,"D","Thread Specification"]
["Socket Head Cap Screws",null,null,"M","Overall Length"]
["Socket Head Cap Screws",null,null,"M","Minimum Thread Length"]
["Socket Head Cap Screws",null,null,"M","Head Diameter"]
["Socket Head Cap Screws",null,null,"M","Screw Diameter"]
["Socket Head Cap Screws",null,null,"I","Head Type (plain, knurled)"]
["Socket Head Cap Screws",null,null,"M","Head Chamfer angle (30 or 45 degrees)"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Size"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Depth"]
["Spool","Spool",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Spool",null,null,"D","Material Specification"]
["Spool",null,null," M","Length Overall"]
["Spool",null,null,"M","Flange Dimensions"]
["Spool",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Spool",null,null,"M","Pipe Dimensions"]
["Stud Bolts","Stud Bolts",null,"D","Material Specification"]
["Stud Bolts",null,null,"I","Marking"]
["Stud Bolts",null,null,"D","Thread Specification"]
["Stud Bolts",null,null,"M","Overall Length"]
["Stud Bolts",null,null,"M","Length of Threads"]
["Stud Bolts",null,null,"M","Length of Shoulder"]
["Stud Bolts",null,null,"D","Stud end chamfer and radius configuration"]
["Stud Bolts",null,null,"M","Diameter"]
["Tank Bottom Sump \nNo washout","Tank Bottom Sump \nNo washout",null,"D ","Material Specification"]
["Tank Bottom Sump \nNo washout",null,null,"I","Marking"]
["Tank Bottom Sump \nNo washout",null,null," M","Dimensional"]
["Tank Bottom Sump \nNo washout",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Tank Bottom Sump \nwith washout","Tank Bottom Sump \nwith washout",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Tank Bottom Sump \nwith washout",null,null,"D","Material Specification"]
["Tank Bottom Sump \nwith washout",null,null,"I","Marking"]
["Tank Bottom Sump \nwith washout",null,null," M","Dimensional"]
["Tank Bottom Sump \nwith washout",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Tank Shell and Manway Nozzles ","Tank Shell and Manway Nozzles ",null,"D","Certified Mill Test Report"]
["Tank Shell and Manway Nozzles ",null,null,"D","Material Specification and Grade"]
["Tank Shell and Manway Nozzles ",null,null,"M","Thickness "]
["Tank Shell and Manway Nozzles ",null,null,"M","Radius (If Applicable)"]
["Tank Shell and Manway Nozzles ",null,null,"I","Rolling Direction (If Applicable)"]
["Tank Shell and Manway Nozzles ",null,null,"I","Material Marking"]
["Thermowell","Thermowell",null,"D","Material Specification"]
["Thermowell",null,null,"D","AAR Device Approval "]
["Thermowell",null,null,"M","Length Overall"]
["Thermowell",null,null,"D & M","Thread Specification"]
["Thermowell",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Vacuum Relief Valves","Vacuum Relief Valves",null,"D","AAR Device Approval "]
["Vacuum Relief Valves",null,null,"D","Model"]
["Vacuum Relief Valves",null,null,"D","Manufacturing Facility"]
["Vacuum Relief Valves",null,null,"I","Connection – Flange Dimensions"]
["Vacuum Relief Valves",null,null,"I","Connection – Thread Specification"]
["Vacuum Relief Valves",null,null,"M","Length"]
["Vacuum Relief Valves",null,null,"M","Body Diameter"]
["Vacuum Relief Valves",null,null,"D","Body Material"]
["Vacuum Relief Valves",null,null,"I","Weld Size / Type (if applicable)"]
["Vacuum Relief Valves",null,null,"I","Lining Material (If Applicable)"]
["Vacuum Relief Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Vacuum Relief Valves",null,null,"D","Seal/O-Ring Material"]
["Vacuum Relief Valves",null,null,"D","OEM Test Certificate"]
["Vacuum Relief Valves",null,null,null,"Vacuum Relief Valves must be marked as following:"]
["Vacuum Relief Valves",null,null,"I","Station stencil of the C4a or C4m facility"]
["Vacuum Relief Valves",null,null,"I","Model number correlated to the AAR design approval"]
["Vacuum Relief Valves",null,null,"I","Unique serial number"]
["Vacuum Relief Valves",null,null,"I","Type of trim and body material"]
["Vacuum Relief Valves",null,null,"I","Vacuum start to open pressure (PSIG)"]
["Washer","Washer",null,"D","Material Specification"]
["Washer",null,null,"I","Marking"]
["Washer",null,null,"M","Inside Diameter"]
["Washer",null,null,"M","Outside Diameter"]
["Washer",null,null,"M","Thickness"]
["Washer",null,null,"M","Flatness"]
["Washer",null,null,"I","Style (Flat or Spring or Lock)"]
["A_None"]

{"sheet":"FORMTAB PREP","index":2,"n_rows":307,"n_cols":17,"rows_kept":307,"cut":false,"hidden":true,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,4],[3,0,3,4],[90,2,90,3],[80,2,80,3],[81,2,81,3],[82,2,82,3],[83,2,83,3],[84,2,84,3],[85,2,85,3],[86,2,86,3],[87,2,87,3],[88,2,88,3],[89,2,89,3],[97,2,97,3],[91,2,91,3],[92,2,92,3],[93,2,93,3],[94,2,94,3],[95,2,95,3],[96,2,96,3],[138,1,139,1],[138,2,139,2],[138,3,139,3],[138,4,139,4],[106,2,106,3],[107,2,107,3],[108,2,108,3],[109,2,109,3],[110,2,112,3],[80,16,85,16],[86,16,97,16],[176,4,177,4],[62,2,62,3],[63,2,63,3],[64,2,64,3],[65,2,65,3],[176,2,177,2],[176,3,177,3],[105,2,105,3],[98,2,98,3],[99,2,99,3],[100,2,100,3],[101,2,101,3],[102,2,102,3],[103,2,104,3],[42,16,52,16],[53,16,55,16],[56,16,61,16],[62,16,69,16],[70,16,79,16],[5,16,11,16],[12,16,17,16],[18,16,26,16],[27,16,32,16],[33,16,41,16],[98,16,105,16],[106,16,112,16],[113,16,117,16],[118,16,121,16],[122,16,126,16],[127,16,132,16],[133,16,139,16],[140,16,145,16],[146,16,150,16],[151,16,156,16],[157,16,177,16],[178,16,196,16],[197,16,201,16],[202,16,218,16],[219,16,229,16],[230,16,234,16],[235,16,257,16],[258,16,275,16],[276,16,298,16],[299,16,306,16]]}
["CLOSURES and FITTINGS - CTQ INSPECTION CRITERIA"]
["D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
["M – Measurement Verification Criteria"]
[]
["Item","Inspection Criteria","Manufacturer","Distributor","Facility",null,"NAME","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria","Certificate \nProvided\nY/N","Inspection\nPerfromed\nY/N","Pass\nFail\nP/F","Measurement \nEquipment\nID#"]
["Eduction Pipe Assembly\n","Material Specification","D","D","D",null,null,"Bolts",null,"D","Material Specification",null,null,null,null,null,"Eduction Pipe Assembly\n"]
[null,"Length Overall","M","M","M",null,null,"Bolts",null,"I","Marking"]
[null,"Thread Specification (If Applicable)","M","M","D & M",null,null,"Bolts",null,"D","Thread Specification"]
[null,"Diameter","M","M","M",null,null,"Bolts",null,"M","Overall Length"]
[null,"Thickness","M","M","M",null,null,"Bolts",null,"M","Length of Threads"]
[null,"Machined Characteristics","M","M","I & M",null,null,"Bolts",null,"M","Length of Shoulder"]
[null,"Weld Size and Type","I","I","I",null,null,"Bolts",null,"M","Diameter"]
["Fittings Plate with no nozzles\n","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Bolts",null,"M","Head size across flats",null,null,null,null,null,"Fittings Plate with no nozzles\n"]
[null,"Material Specification","D","D","D",null,null,"Tank Bottom Sump with washout PCP 1 & 8 (4 if required)\n",null,"D","AAR Device Approval  (If Contractually Specified)"]
[null,"Thickness","M","M","D",null,null,"Tank Bottom Sump with washout PCP 1 & 8 (4 if required)\n",null,"D","Material Specification"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","M","M","D",null,null,"Tank Bottom Sump with washout PCP 1 & 8 (4 if required)\n",null,"I","Marking"]
[null,"Gauge tapped threads","M","M","M",null,null,"Tank Bottom Sump with washout PCP 1 & 8 (4 if required)\n",null," M","Dimensional"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes","M","M","I &M",null,null,"Tank Bottom Sump with washout PCP 1 & 8 (4 if required)\n",null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Fittings Plate with Welded Nozzle(s)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Tank Bottom Sump no washout\nPCP 1 & 8 (4 if required)\n",null,"D ","Material Specification",null,null,null,null,null,"Fittings Plate with Welded Nozzle(s)"]
[null,"Material Specification","D","D","D ",null,null,"Tank Bottom Sump no washout\nPCP 1 & 8 (4 if required)\n",null,"I","Marking"]
[null,"Inside Diameter","M","M"," M",null,null,"Tank Bottom Sump no washout\nPCP 1 & 8 (4 if required)\n",null," M","Dimensional"]
[null,"Outside Diameter","M","M"," M",null,null,"Tank Bottom Sump no washout\nPCP 1 & 8 (4 if required)\n",null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
[null,"Thickness","M","M","M",null,null,"Eduction Pipe Assembly\n",null,"D","Material Specification"]
[null,"Nozzle Dimensions","M","M","M",null,null,"Eduction Pipe Assembly\n",null,"M","Length Overall"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I",null,null,"Eduction Pipe Assembly\n",null,"D & M","Thread Specification (If Applicable)"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern","M","M","I & M",null,null,"Eduction Pipe Assembly\n",null,"M","Diameter"]
[null,"Weld Size and Type","I","I","I",null,null,"Eduction Pipe Assembly\n",null,"M","Thickness"]
["Flanges","Material Specification","D","D","D",null,null,"Eduction Pipe Assembly\n",null,"I & M","Machined Characteristics",null,null,null,null,null,"Flanges"]
[null,"Inside Diameter (if required)","M","M","M",null,null,"Eduction Pipe Assembly\n",null,"I","Weld Size and Type"]
[null,"Outside Diameter","M","M","M",null,null,"  Tank Bottom Outlet Valve Mounting Saddle Flange PCP 1 & 8 (4 if required)",null,"D","AAR Device Approval  (If Contractually Specified)"]
[null,"Thickness","M","M","M",null,null,"  Tank Bottom Outlet Valve Mounting Saddle Flange PCP 1 & 8 (4 if required)",null,"D","Material Specification"]
[null,"Sealing Style (Flat Face, Raised, or Tongue and Groove)","M","M","I",null,null,"  Tank Bottom Outlet Valve Mounting Saddle Flange PCP 1 & 8 (4 if required)",null,"I","Marking"]
[null,"Machined Characteristics /Gasket Surface","M","M","I",null,null,"  Tank Bottom Outlet Valve Mounting Saddle Flange PCP 1 & 8 (4 if required)",null," M","Dimensional"]
["Hinged and Bolted \nManway Covers\n(Cast)\n","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"  Tank Bottom Outlet Valve Mounting Saddle Flange PCP 1 & 8 (4 if required)",null,"I","Structural Integrity (Cracks or Excessive Porosity)",null,null,null,null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n"]
[null,"Material Specification","D","D","D",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"D","AAR Device Approval "]
[null,"Structural Integrity – Pressure Test ","M","M","D ",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"D","Model"]
[null,"Casting Quality","I","D","D",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"D ","Manufacturing Facility"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"M","Connection – Flange Dimensions"]
[null,"Bolt Pattern","M","M","I",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"D & M","Connection – Thread Specification"]
[null,"Hinge Position","M","M","I",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"D","Flow Rated Capacity"]
[null,"Bolt Slot Opening Dimensions","M","M","M",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"D","OEM test certificate"]
[null,"Gasket Groove Dimensions","M","M","M",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,0,"Each device must be marked to indicate as following:"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"I","• Manufacturer marking",null,null,null,null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)"]
[null,"Material Specification","D","D","D",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"I","• Manufacturer’s design or type number"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I",null,null,"Excess Flow Valves, (Includes Spring Loaded)",null,"I","• Serial number for threaded device (not welded to manway cover)"]
[null,"Nozzle Dimensions","M","M"," M",null,null,"Eyebolts",null,"D","Material Specification"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I",null,null,"Eyebolts",null,"I","Marking"]
[null,"Bolt Pattern","M","M","D",null,null,"Eyebolts",null,"D","Thread Specification"]
[null,"Weld Size and Type","I","I","I",null,null,"Eyebolts",null,"M","Overall Length"]
[null,"Hinge Position","M","M","I",null,null,"Eyebolts",null,"M","Length of Threads"]
[null,"Bolt Slot Opening Dimensions","M","M"," M",null,null,"Eyebolts",null,"M","Length of Shoulder"]
[null,"Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)","M","M"," M",null,null,"Eyebolts",null,"M","Diameter"]
[null,"Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)","M","M"," I",null,null,"Eyebolts",null,"M","Nut length across flats and thickness"]
["Pipe Plugs","Material Specification","D","D","D",null,null,"Eyebolts",null,"M","Nut style square/hex",null,null,null,null,null,"Pipe Plugs"]
[null,"Thread Specification ","M","M","D & M",null,null,"Eyebolts",null,"M","Eyelet ID/OD"]
[null,"Diameter","M","M","M",null,null,"Fittings Plate with no nozzles\n",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Spool","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Fittings Plate with no nozzles\n",null,"D","Material Specification",null,null,null,null,null,"Spool"]
[null,"Material Specification","D","D","D",null,null,"Fittings Plate with no nozzles\n",null,"D","Thickness"]
[null,"Length Overall","M","M"," M",null,null,"Fittings Plate with no nozzles\n",null,"D","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
[null,"Flange Dimensions","M","M","M",null,null,"Fittings Plate with no nozzles\n",null,"M","Gauge tapped threads"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I",null,null,"Fittings Plate with no nozzles\n",null,"I &M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes"]
[null,"Pipe Dimensions","M","M","M",null,null,"Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Bolts","Material Specification","Per ASME B18.18, Category 2, ",null,"D",null,null,"Fittings Plate with Welded Nozzle(s)",null,"D ","Material Specification",null,null,null,null,null,"Bolts"]
[null,"Marking","ASTM F1470",null,"I",null,null,"Fittings Plate with Welded Nozzle(s)",null," M","Inside Diameter"]
[null,"Thread Specification","ASTM 370",null,"D",null,null,"Fittings Plate with Welded Nozzle(s)",null," M","Outside Diameter"]
[null,"Overall Length","ASTM F788",null,"M",null,null,"Fittings Plate with Welded Nozzle(s)",null,"M","Thickness"]
[null,"Length of Threads",null,null,"M",null,null,"Fittings Plate with Welded Nozzle(s)",null,"M","Nozzle Dimensions"]
[null,"Length of Shoulder",null,null,"M",null,null,"Fittings Plate with Welded Nozzle(s)",null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
[null,"Diameter",null,null,"M",null,null,"Fittings Plate with Welded Nozzle(s)",null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern"]
[null,"Head size across flats",null,null,"M",null,null,"Fittings Plate with Welded Nozzle(s)",null,"I","Weld Size and Type"]
["Eyebolts","Material Specification","D","D","D",null,null,"Flanged Nozzle",null,"D","Material Specification",null,null,null,null,null,{"$f":"A71","v":"Eyebolts"}]
[null,"Marking","I","I","I",null,null,"Flanged Nozzle",null," M","Length Overall"]
[null,"Thread Specification","M","M","D",null,null,"Flanged Nozzle",null,"M","Diameter"]
[null,"Overall Length","M","M","M",null,null,"Flanged Nozzle",null,"M","Thickness"]
[null,"Length of Threads","M","M","M",null,null,"Flanged Nozzle",null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern"]
[null,"Length of Shoulder","M","M","M",null,null,"Flanged Nozzle",null,"I","Weld Size and Type (Forged or Cast)"]
[null,"Diameter","M","M","M",null,null,"Flanges",null,"D","Material Specification"]
[null,"Nut length across flats and thickness","M","M","M",null,null,"Flanges",null,"M","Inside Diameter (if required)"]
[null,"Nut style square/hex","M","M","M",null,null,"Flanges",null,"M","Outside Diameter"]
[null,"Eyelet ID/OD","M","M","M",null,null,"Flanges",null,"M","Thickness"]
["Nut","Material Specification","Per ASME B18.18, Category 2.",null,"D",null,null,"Flanges",null,"I","Sealing Style (Flat Face, Raised, or Tongue and Groove)",null,null,null,null,null,{"$f":"A81","v":"Nut"}]
[null,"Marking","ASTM F1470, ",null,"I",null,null,"Flanges",null,"I","Machined Characteristics /Gasket Surface"]
[null,"Thread Specification","ASTM 370",null,"D",null,null,"Gaskets and O-Rings",null,"D","Material Specification"]
[null,"Length across flats","ASTM F788",null,"M",null,null,"Gaskets and O-Rings",null,"I","Marking (if applicable)"]
[null,"Thickness",null,null,"M",null,null,"Gaskets and O-Rings",null,"M","Inside Diameter"]
[null,"Style (Square or Hex)",null,null,"I",null,null,"Gaskets and O-Rings",null,"M","Outside Diameter"]
["Socket Head Cap Screws","Material Specification","Per ASME B18.18, Category 2.",null,"D",null,null,"Gaskets and O-Rings",null," M","Thickness",null,null,null,null,null,{"$f":"A87","v":"Socket Head Cap Screws"}]
[null,"Finish (plain, zinc, other)","ASTM F1470",null,"I",null,null,"Heat and Pressure Sensors",null,"D","AAR Device Approval "]
[null,"Marking (if specified)","ASTM 370",null,"I ",null,null,"Heat and Pressure Sensors",null,"D","Model"]
[null,"Thread Specification","ASTM F788",null,"D",null,null,"Heat and Pressure Sensors",null,"D","Manufacturing Facility"]
[null,"Overall Length",null,null,"M",null,null,"Heat and Pressure Sensors",null,"M","Connection – Flange Dimensions"]
[null,"Minimum Thread Length",null,null,"M",null,null,"Heat and Pressure Sensors",null,"D & M","Connection – Thread Specification"]
[null,"Head Diameter",null,null,"M",null,null,"Heat and Pressure Sensors",null,"D","OEM test certificate"]
[null,"Screw Diameter",null,null,"M",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"D","AAR Device Approval  (If Contractually Specified)"]
[null,"Head Type (plain, knurled)",null,null,"I",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"D","Material Specification"]
[null,"Head Chamfer angle (30 or 45 degrees)",null,null,"M",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"D ","Structural Integrity – Pressure Test "]
[null,"Nominal Hex Socket Size",null,null,"M",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"D","Casting Quality"]
[null,"Nominal Hex Socket Depth",null,null,"M",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Stud Bolts","Material Specification","Per ASME B18.18, Category 2.",null,"D",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"I","Bolt Pattern",null,null,null,null,null,{"$f":"A99","v":"Stud Bolts"}]
[null,"Marking","ASTM F1470",null,"I",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"I","Hinge Position"]
[null,"Thread Specification","ASTM 370",null,"D",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"M","Bolt Slot Opening Dimensions"]
[null,"Overall Length","ASTM F788",null,"M",null,null,"Hinged and Bolted \nManway Covers\n(Cast)\n",null,"M","Gasket Groove Dimensions"]
[null,"Length of Threads",null,null,"M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","AAR Device Approval  (If Contractually Specified)"]
[null,"Length of Shoulder",null,null,"M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","Material Specification"]
[null,"Stud end chamfer and radius configuration",null,null,"D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"I","Thickness (Dished, Flanged, or Grooved)"]
[null,"Diameter",null,null,"M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null," M","Nozzle Dimensions"]
["Washer","Material Specification","Per ASME B18.18, Category 2.",null,"D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)",null,null,null,null,null,{"$f":"A107","v":"Washer"}]
[null,"Marking","ASTM F1470",null,"I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","Bolt Pattern"]
[null,"Inside Diameter","ASTM 370",null,"M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"I","Weld Size and Type"]
[null,"Outside Diameter","ASTM F788",null,"M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"I","Hinge Position"]
[null,"Thickness",null,null,"M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null," M","Bolt Slot Opening Dimensions"]
[null,"Flatness",null,null,"M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null," M","Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)"]
[null,"Style (Flat or Spring or Lock)",null,null,"I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null," I","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)"]
["Bottom Outlet Valve Saddle – Drain Opening","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Hinged and Bolted Nozzle Assembly",null,"D","Material Specification",null,null,null,null,null,{"$f":"A114","v":"Bottom Outlet Valve Saddle – Drain Opening"}]
[null,"Material Specification","D","D","D",null,null,"Hinged and Bolted Nozzle Assembly",null,"M","Length Overall"]
[null,"Marking","I","I","I",null,null,"Hinged and Bolted Nozzle Assembly",null,"M","Thickness"]
[null,"Dimensional","M","M"," M",null,null,"Hinged and Bolted Nozzle Assembly",null,"I","Weld Size and Type"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I",null,null,"Hinged and Bolted Nozzle Assembly",null,"I","Hinge Position"]
["Bottom Outlet Valve Sump – No Opening","Material Specification","D","D","D ",null,null,"Hinged and Bolted Nozzle Assembly",null,"M","Eyebolt Lug Position",null,null,null,null,null,{"$f":"A119","v":"Bottom Outlet Valve Sump – No Opening"}]
[null,"Marking","I","I","I",null,null,"Hinged and Bolted Nozzle Assembly",null,0,0]
[null,"Dimensional","M","M"," M",null,null,"Liquid Level and Gauging Devices",null,"D","AAR Device Approval "]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I",null,null,"Liquid Level and Gauging Devices",null,"D","Model"]
["Eduction Pipe Sump","Material Specification","D","D","D",null,null,"Liquid Level and Gauging Devices",null,"D ","Manufacturing Facility",null,null,null,null,null,{"$f":"A123","v":"Eduction Pipe Sump"}]
[null,"Marking (If Required)","I","I","I",null,null,"Liquid Level and Gauging Devices",null,"M","Connection – Flange Dimensions & Bolt Circle"]
[null,"Dimensions (O.D. and Depth)","M","M","M",null,null,"Liquid Level and Gauging Devices",null,"M","Gage Rod Housing Length"]
[null,"Structural Integrity – Pressure Test","M","M","D ",null,null,"Liquid Level and Gauging Devices",null,"I","Gage Rod Assembly"]
[null,"Thickness","M","M","M",null,null,"Liquid Level and Gauging Devices",null,"I","Float Assembly"]
["Flanged Nozzle","Material Specification","D","D","D",null,null,"Liquid Level and Gauging Devices",null,"I","Body Assembly",null,null,null,null,null,{"$f":"A128","v":"Flanged Nozzle"}]
[null,"Length Overall","M","M"," M",null,null,"Liquid Level and Gauging Devices",null,"I","Bottom Spring"]
[null,"Diameter","M","M","M",null,null,"Liquid Level and Gauging Devices",null,"I","Guide Tube Assembly"]
[null,"Thickness","M","M","M",null,null,"Liquid Level and Gauging Devices",null,"I","Installation Correction Nut"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern","M","M","I & M",null,null,"Liquid Level and Gauging Devices",null,"I","Specific Gravity Adjustment Bushing (as applicable)"]
[null,"Weld Size and Type (Forged or Cast)","I","I","I",null,null,"Liquid Level and Gauging Devices",null,"I","Cover with Chain"]
["Hinged and Bolted Nozzle Assembly","Material Specification","D","D","D",null,null,"Liquid Level and Gauging Devices",null,"D","Seal/O-Ring Dimensions",null,null,null,null,null,{"$f":"A134","v":"Hinged and Bolted Nozzle Assembly"}]
[null,"Length Overall","M","M","M",null,null,"Liquid Level and Gauging Devices",null,"D","Seal/O-Ring Material"]
[null,"Thickness","M","M","M",null,null,"Liquid Level and Gauging Devices",null,"D","Magnetic Strength per OEM Specifications"]
[null,"Weld Size and Type","I","I","I",null,null,"Liquid Level and Gauging Devices",null,"D","Commodity(s)"]
[null,"Hinge Position","M","M","I",null,null,"Liquid Level and Gauging Devices",null,"D","Specific Gravity(s)"]
[null,"Eyebolt Lug Position","M","M","M",null,null,"Liquid Level and Gauging Devices",null,0,"Each device must be marked as follows:"]
[null,null,null,null,null,null,null,"Liquid Level and Gauging Devices",null,"I","• Manufacturer marking"]
["Tank Shell and Manway Nozzles ","Certified Mill Test Report","I","D","D",null,null,"Liquid Level and Gauging Devices",null,"I","• Manufacturer’s design or type number",null,null,null,null,null,{"$f":"A141","v":"Tank Shell and Manway Nozzles "}]
[null,"Material Specification and Grade","D","D","D",null,null,"Liquid Level and Gauging Devices",null,"I","• Serial number"]
[null,"Thickness ","M","M","M",null,null,"Liquid Level and Gauging Devices",null,"I","• Pressure-temperature limitations"]
[null,"Radius (If Applicable)","M","M","M",null,null,"Liquid/Vapor, and Sample Valves",null,"D","AAR Device Approval "]
[null,"Rolling Direction (If Applicable)","M","I","I",null,null,"Liquid/Vapor, and Sample Valves",null,"D","Model"]
[null,"Material Marking","I","I","I",null,null,"Liquid/Vapor, and Sample Valves",null,"D","Manufacturing Facility"]
["Gaskets and O-Rings","Material Specification","D","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,"I","Connection – Flange Dimensions",null,null,null,null,null,{"$f":"A147","v":"Gaskets and O-Rings"}]
[null,"Marking (if applicable)","D","D","I",null,null,"Liquid/Vapor, and Sample Valves",null,"I","Connection – Thread Specification"]
[null,"Inside Diameter","M","M","M",null,null,"Liquid/Vapor, and Sample Valves",null,"M","Body Length"]
[null,"Outside Diameter","M","M","M",null,null,"Liquid/Vapor, and Sample Valves",null,"M","Body Diameter"]
[null,"Thickness","M","M"," M",null,null,"Liquid/Vapor, and Sample Valves",null,"D","Port Opening Size"]
["Heat and Pressure Sensors","AAR Device Approval ","D","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,"D","Body Material",null,null,null,null,null,{"$f":"A152","v":"Heat and Pressure Sensors"}]
[null,"Model","I","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,"I","Lining Material (If Applicable)"]
[null,"Manufacturing Facility","D","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,"D","Seal/O-Ring Dimensions"]
[null,"Connection – Flange Dimensions","M","D","M",null,null,"Liquid/Vapor, and Sample Valves",null,"D","Seal/O-Ring Material"]
[null,"Connection – Thread Specification","M","D","D & M",null,null,"Liquid/Vapor, and Sample Valves",null,"D","OEM test certificate"]
[null,"OEM test certificate","D","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,0,"Each Valve with a port flow diameter greater than 0.75 inchEs = net free-flow area of more than 1/2 in.2 (323 mm2) must be marked to indicate the following:\n"]
["Liquid/Vapor, and Sample Valves","AAR Device Approval ","D","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,"I","•Manufacturer marking",null,null,null,null,null,{"$f":"A158","v":"Liquid/Vapor, and Sample Valves"}]
[null,"Model","I","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,"I","• Manufacturer’s design or type number"]
[null,"Manufacturing Facility","D","D","D",null,null,"Liquid/Vapor, and Sample Valves",null,"I","• Serial number"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Liquid/Vapor, and Sample Valves",null,"I","• Type of trim"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Liquid/Vapor, and Sample Valves",null,"I","• Pressure-temperature limitations"]
[null,"Body Length","M","D","M",null,null,"Liquid/Vapor, and Sample Valves",null,"I","Note:  All pressure-retaining valve body castings shall be marked in accordance with the appropriate ASTM specification, including material identification with the grade symbols (e.g., WCB, WC9, CF8M, etc.), heat numbers, or a lot number traceable to either a heat number or month poured."]
[null,"Body Diameter","M","D","M",null,null,"Liquid/Vapor, and Sample Valves",null,0,"For valve bodies constructed with more than one pressure-retaining casting, each casting must comply with the applicable ASTM marking requirement. This does not apply to bonnets, yokes, or body inserts."]
[null,"Port Opening Size","M","D","D",null,null,"Nut",null,"D","Material Specification"]
[null,"Body Material","D","D","D",null,null,"Nut",null,"I","Marking"]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Nut",null,"D","Thread Specification"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Nut",null,"M","Length across flats"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Nut",null,"M","Thickness"]
[null,"OEM test certificate","D","D","D",null,null,"Nut",null,"I","Style (Square or Hex)"]
[null,"Each Valve with a port flow diameter greater than 0.75 inchEs = net free-flow area of more than 1/2 in.2 (323 mm2) must be marked to indicate the following:\n",null,null,null,null,null,"Pipe Plugs",null,"D","Material Specification"]
[null,"•Manufacturer marking","I","I","I",null,null,"Pipe Plugs",null,"D & M","Thread Specification "]
[null,"• Manufacturer’s design or type number","I","I","I",null,null,"Pipe Plugs",null,"M","Diameter"]
[null,"• Serial number","I","I","I",null,null,"Pressure Regulator Valves",null,"D","AAR Device Approval "]
[null,"• Type of trim","I","I","I",null,null,"Pressure Regulator Valves",null,"D","Model"]
[null,"• Pressure-temperature limitations","I","I","I",null,null,"Pressure Regulator Valves",null,"D","Manufacturing Facility"]
[null,"Note:  All pressure-retaining valve body castings shall be marked in accordance with the appropriate ASTM specification, including material identification with the grade symbols (e.g., WCB, WC9, CF8M, etc.), heat numbers, or a lot number traceable to either a heat number or month poured.","I","I","I",null,null,"Pressure Regulator Valves",null,"I","Connection – Flange Dimensions"]
[null,"For valve bodies constructed with more than one pressure-retaining casting, each casting must comply with the applicable ASTM marking requirement. This does not apply to bonnets, yokes, or body inserts.",null,null,null,null,null,"Pressure Regulator Valves",null,"I","Connection – Thread Specification"]
["Pressure Regulator Valves","AAR Device Approval ","D","D","D",null,null,"Pressure Regulator Valves",null,"M","Body Length",null,null,null,null,null,{"$f":"A179","v":"Pressure Regulator Valves"}]
[null,"Model","I","D","D",null,null,"Pressure Regulator Valves",null,"M","Body Diameter"]
[null,"Manufacturing Facility","D","D","D",null,null,"Pressure Regulator Valves",null,"D","Port Opening Size"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Pressure Regulator Valves",null,"D","Body Material"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Pressure Regulator Valves",null,"I","Lining Material (If Applicable)"]
[null,"Body Length","M","D","M",null,null,"Pressure Regulator Valves",null,"D","Seal/O-Ring Dimensions"]
[null,"Body Diameter","M","D","M",null,null,"Pressure Regulator Valves",null,"D","Seal/O-Ring Material"]
[null,"Port Opening Size","M","D","D",null,null,"Pressure Regulator Valves",null,"D","OEM test certificate "]
[null,"Body Material","D","D","D",null,null,"Pressure Regulator Valves",null,0,"Pressure Regulator Valves must be marked to indicate the following:"]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Pressure Regulator Valves",null,"I","• Manufacturer marking"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Pressure Regulator Valves",null,"I","• Manufacturer’s design or type number"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Pressure Regulator Valves",null,"I","• Nominal standard set pressure"]
[null,"OEM test certificate ","D","D","D",null,null,"Pressure Regulator Valves",null,"I","• Serial number"]
[null,"Pressure Regulator Valves must be marked to indicate the following:",null,null,null,null,null,"Pressure Regulator Valves",null,"I","• AAR-approval number as of the date of manufacture"]
[null,"• Manufacturer marking","I","I","I",null,null,"Pressure Relief Valves",null,"D","AAR Device Approval "]
[null,"• Manufacturer’s design or type number","I","I","I",null,null,"Pressure Relief Valves",null,"D","Model"]
[null,"• Nominal standard set pressure","I","I","I",null,null,"Pressure Relief Valves",null,"D","Manufacturing Facility"]
[null,"• Serial number","I","I","I",null,null,"Pressure Relief Valves",null,"I","Connection – Flange Dimensions"]
[null,"• AAR-approval number as of the date of manufacture","I","I","I",null,null,"Pressure Relief Valves",null,"I","Connection – Thread Specification"]
["Rupture Discs","Model","I","D","D",null,null,"Pressure Relief Valves",null,"M","Length",null,null,null,null,null,{"$f":"A198","v":"Rupture Discs"}]
[null,"Burst Rating","D","D","D",null,null,"Pressure Relief Valves",null,"M","Body Diameter"]
[null,"Structural Integrity","M","M","I",null,null,"Pressure Relief Valves",null,"D","Body Material"]
[null,"Certificate of Test (Per Lot)","D","D","D",null,null,"Pressure Relief Valves",null,"I","Lining Material (If Applicable)"]
[null,"Mark “TOP” on discharge side.","I","I","I",null,null,"Pressure Relief Valves",null,"D","Seal/O-Ring Dimensions"]
["Rupture Disc Housing/Devices","AAR Device Approval","D","D","D",null,null,"Pressure Relief Valves",null,"D","Seal/O-Ring Material",null,null,null,null,null,{"$f":"A203","v":"Rupture Disc Housing/Devices"}]
[null,"Model","I","D","D",null,null,"Pressure Relief Valves",null,"D","Start to Discharge Pressure"]
[null,"Manufacturing Facility","D","D","D",null,null,"Pressure Relief Valves",null,"D","Vapor Tight Pressure"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Pressure Relief Valves",null,"D","Flow Rated Capacity"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Pressure Relief Valves",null,"D","OEM Test Certificate"]
[null,"Body Length","M","D","M",null,null,"Pressure Relief Valves",null,"D","AAR Certificate of Test"]
[null,"Body Diameter","M","D","M",null,null,"Pressure Relief Valves",null,0,"Pressure Relief Valves must be marked as follows:"]
[null,"Port Opening Size","M","D","D",null,null,"Pressure Relief Valves",null,"I","• Manufacturer marking"]
[null,"Body Material","D","D","D",null,null,"Pressure Relief Valves",null,"I","• Manufacturer’s design or type number"]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Pressure Relief Valves",null,"I","• Serial number"]
[null,"Vapor Tight Pressure","D","D","D",null,null,"Pressure Relief Valves",null,"I","• Set pressure, psi (or psi and kPa)"]
[null,"OEM Test Certificate","D","D","D",null,null,"Pressure Relief Valves",null,"I","• Official flow capacity,"]
[null,"AAR Certificate of Test","D","D","D",null,null,"Pressure Relief Valves",null,"I","• Flow rating pressure, psi (or psi and kPa)"]
[null,"Marked on the flange or on a nameplate:",null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"D","Certified Mill Test Report"]
[null,"• Manufacturer marking;","I","I","I",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"D","Material Specification and Grade"]
[null,"• Manufacturer’s design or type number and serial number; and","I","I","I",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"M","Thickness"]
[null,"• Flow rating pressure, (PSI and/or kPa)","I","I","I",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"M","Radius (If Applicable)"]
["Excess Flow Valves, (Includes Spring Loaded)","AAR Device Approval ","D","D","D",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"I","Rolling Direction (If Applicable)",null,null,null,null,null,{"$f":"A220","v":"Excess Flow Valves, (Includes Spring Loaded)"}]
[null,"Model","I","D","D",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"M","Inside Diameter (If Applicable)"]
[null,"Manufacturing Facility","D","D","D ",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"M","Outside Diameter (If Applicable)"]
[null,"Connection – Flange Dimensions","M","D","M",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"I","Material Marking"]
[null,"Connection – Thread Specification","M","D","D & M",null,null,"Rupture Disc Housing/Devices",null,"D","AAR Device Approval"]
[null,"Flow Rated Capacity","D","D","D",null,null,"Rupture Disc Housing/Devices",null,"D","Model"]
[null,"OEM test certificate","D","D","D",null,null,"Rupture Disc Housing/Devices",null,"D","Manufacturing Facility"]
[null,"Each device must be marked to indicate as following:",null,null,null,null,null,"Rupture Disc Housing/Devices",null,"I","Connection – Flange Dimensions"]
[null,"• Manufacturer marking","I","I","I",null,null,"Rupture Disc Housing/Devices",null,"I","Connection – Thread Specification"]
[null,"• Manufacturer’s design or type number","I","I","I",null,null,"Rupture Disc Housing/Devices",null,"M","Body Length"]
[null,"• Serial number for threaded device (not welded to manway cover)","I","I","I",null,null,"Rupture Disc Housing/Devices",null,"M","Body Diameter"]
["Thermowell","Material Specification","D","D","D",null,null,"Rupture Disc Housing/Devices",null,"D","Port Opening Size",null,null,null,null,null,{"$f":"A231","v":"Thermowell"}]
[null,"AAR Device Approval ","D","D","D",null,null,"Rupture Disc Housing/Devices",null,"D","Body Material"]
[null,"Length Overall","M","M","M",null,null,"Rupture Disc Housing/Devices",null,"I","Lining Material (If Applicable)"]
[null,"Thread Specification","M","M","D & M",null,null,"Rupture Disc Housing/Devices",null,"D","Vapor Tight Pressure"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I",null,null,"Rupture Disc Housing/Devices",null,"D","OEM Test Certificate"]
["Pressure Relief Valves","AAR Device Approval ","D","D","D",null,null,"Rupture Disc Housing/Devices",null,"D","AAR Certificate of Test",null,null,null,null,null,{"$f":"A236","v":"Pressure Relief Valves"}]
[null,"Model","I","D","D",null,null,"Rupture Disc Housing/Devices",null,0,"Marked on the flange or on a nameplate:"]
[null,"Manufacturing Facility","D","D","D",null,null,"Rupture Disc Housing/Devices",null,"I","• Manufacturer marking;"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Rupture Disc Housing/Devices",null,"I","• Manufacturer’s design or type number and serial number; and"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Rupture Disc Housing/Devices",null,"I","• Flow rating pressure, (PSI and/or kPa)"]
[null,"Length","M","D","M",null,null,"Rupture Discs",null,"D","Model"]
[null,"Body Diameter","M","D","M",null,null,"Rupture Discs",null,"D","Burst Rating"]
[null,"Body Material","D","D","D",null,null,"Rupture Discs",null,"I","Structural Integrity"]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Rupture Discs",null,"D","Certificate of Test (Per Lot)"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Rupture Discs",null,"I","Mark “TOP” on discharge side."]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Socket Head Cap Screws",null,"D","Material Specification"]
[null,"Start to Discharge Pressure","D","D","D",null,null,"Socket Head Cap Screws",null,"I","Finish (plain, zinc, other)"]
[null,"Vapor Tight Pressure","D","D","D",null,null,"Socket Head Cap Screws",null,"I ","Marking (if specified)"]
[null,"Flow Rated Capacity","D","D","D",null,null,"Socket Head Cap Screws",null,"D","Thread Specification"]
[null,"OEM Test Certificate","D","D","D",null,null,"Socket Head Cap Screws",null,"M","Overall Length"]
[null,"AAR Certificate of Test","D","D","D",null,null,"Socket Head Cap Screws",null,"M","Minimum Thread Length"]
[null,"Pressure Relief Valves must be marked as follows:",null,null,null,null,null,"Socket Head Cap Screws",null,"M","Head Diameter"]
[null,"• Manufacturer marking","I","I","I",null,null,"Socket Head Cap Screws",null,"M","Screw Diameter"]
[null,"• Manufacturer’s design or type number","I","I","I",null,null,"Socket Head Cap Screws",null,"I","Head Type (plain, knurled)"]
[null,"• Serial number","I","I","I",null,null,"Socket Head Cap Screws",null,"M","Head Chamfer angle (30 or 45 degrees)"]
[null,"• Set pressure, psi (or psi and kPa)","I","I","I",null,null,"Socket Head Cap Screws",null,"M","Nominal Hex Socket Size"]
[null,"• Official flow capacity,","I","I","I",null,null,"Socket Head Cap Screws",null,"M","Nominal Hex Socket Depth"]
[null,"• Flow rating pressure, psi (or psi and kPa)","I","I","I",null,null,"Spool",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Vacuum Relief Valves","AAR Device Approval ","D","D","D",null,null,"Spool",null,"D","Material Specification",null,null,null,null,null,{"$f":"A259","v":"Vacuum Relief Valves"}]
[null,"Model","I","D","D",null,null,"Spool",null," M","Length Overall"]
[null,"Manufacturing Facility","D","D","D",null,null,"Spool",null,"M","Flange Dimensions"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Spool",null,"I","Mounting Style (Bolted or Threaded)"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Spool",null,"M","Pipe Dimensions"]
[null,"Length","M","D","M",null,null,"Stud Bolts",null,"D","Material Specification"]
[null,"Body Diameter","M","D","M",null,null,"Stud Bolts",null,"I","Marking"]
[null,"Body Material","D","D","D",null,null,"Stud Bolts",null,"D","Thread Specification"]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Stud Bolts",null,"M","Overall Length"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Stud Bolts",null,"M","Length of Threads"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Stud Bolts",null,"M","Length of Shoulder"]
[null,"OEM Test Certificate","D","D","D",null,null,"Stud Bolts",null,"D","Stud end chamfer and radius configuration"]
[null,"Vacuum Relief Valves must be marked as following:",null,null,null,null,null,"Stud Bolts",null,"M","Diameter"]
[null,"• Manufacturer marking","I","I","I",null,null,"Tank Shell and Manway Nozzles ",null,"D","Certified Mill Test Report"]
[null,"• Manufacturer’s design or type number","I","I","I",null,null,"Tank Shell and Manway Nozzles ",null,"D","Material Specification and Grade"]
[null,"• Serial number","I","I","I",null,null,"Tank Shell and Manway Nozzles ",null,"M","Thickness "]
[null,"• Type of trim and body material","I","I","I",null,null,"Tank Shell and Manway Nozzles ",null,"M","Radius (If Applicable)"]
[null,"• Vacuum set pressure","I","I","I",null,null,"Tank Shell and Manway Nozzles ",null,"I","Rolling Direction (If Applicable)"]
["Liquid Level and Gauging Devices","AAR Device Approval ","D","D","D",null,null,"Tank Shell and Manway Nozzles ",null,"I","Material Marking",null,null,null,null,null,{"$f":"A277","v":"Liquid Level and Gauging Devices"}]
[null,"Model","I","D","D",null,null,"Thermowell",null,"D","Material Specification"]
[null,"Manufacturing Facility","D","D","D ",null,null,"Thermowell",null,"D","AAR Device Approval "]
[null,"Connection – Flange Dimensions & Bolt Circle","M","D","M",null,null,"Thermowell",null,"M","Length Overall"]
[null,"Gage Rod Housing Length","M","D","M",null,null,"Thermowell",null,"D & M","Thread Specification"]
[null,"Gage Rod Assembly","D","D","I",null,null,"Thermowell",null,"I","Mounting Style (Bolted or Threaded)"]
[null,"Float Assembly","D","D","I",null,null,"Vacuum Relief Valves",null,"D","AAR Device Approval "]
[null,"Body Assembly","D","D","I",null,null,"Vacuum Relief Valves",null,"D","Model"]
[null,"Bottom Spring","D","D","I",null,null,"Vacuum Relief Valves",null,"D","Manufacturing Facility"]
[null,"Guide Tube Assembly","D","D","I",null,null,"Vacuum Relief Valves",null,"I","Connection – Flange Dimensions"]
[null,"Installation Correction Nut","D","D","I",null,null,"Vacuum Relief Valves",null,"I","Connection – Thread Specification"]
[null,"Specific Gravity Adjustment Bushing (as applicable)","D","D","I",null,null,"Vacuum Relief Valves",null,"M","Length"]
[null,"Cover with Chain","D","D","I",null,null,"Vacuum Relief Valves",null,"M","Body Diameter"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Vacuum Relief Valves",null,"D","Body Material"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Vacuum Relief Valves",null,"I","Lining Material (If Applicable)"]
[null,"Magnetic Strength per OEM Specifications","M","D","D",null,null,"Vacuum Relief Valves",null,"D","Seal/O-Ring Dimensions"]
[null,"Commodity(s)","I","D","D",null,null,"Vacuum Relief Valves",null,"D","Seal/O-Ring Material"]
[null,"Specific Gravity(s)","I","D","D",null,null,"Vacuum Relief Valves",null,"D","OEM Test Certificate"]
[null,"Each device must be marked as follows:",null,null,null,null,null,"Vacuum Relief Valves",null,0,"Vacuum Relief Valves must be marked as following:"]
[null,"• Manufacturer marking","I","I","I",null,null,"Vacuum Relief Valves",null,"I","• Manufacturer marking"]
[null,"• Manufacturer’s design or type number","I","I","I",null,null,"Vacuum Relief Valves",null,"I","• Manufacturer’s design or type number"]
[null,"• Serial number","I","I","I",null,null,"Vacuum Relief Valves",null,"I","• Serial number"]
[null,"• Pressure-temperature limitations","I","I","I",null,null,"Vacuum Relief Valves",null,"I","• Type of trim and body material"]
["Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material","Certified Mill Test Report","I","D","D",null,null,"Vacuum Relief Valves",null,"I","• Vacuum set pressure",null,null,null,null,null,{"$f":"A300","v":"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material"}]
[null,"Material Specification and Grade","D","D","D",null,null,"Washer",null,"D","Material Specification"]
[null,"Thickness","M","M","M",null,null,"Washer",null,"I","Marking"]
[null,"Radius (If Applicable)","M","M","M",null,null,"Washer",null,"M","Inside Diameter"]
[null,"Rolling Direction (If Applicable)","M","I","I",null,null,"Washer",null,"M","Outside Diameter"]
[null,"Inside Diameter (If Applicable)","M","M","M",null,null,"Washer",null,"M","Thickness"]
[null,"Outside Diameter (If Applicable)","M","M","M",null,null,"Washer",null,"M","Flatness"]
[null,"Material Marking","I","I","I",null,null,"Washer",null,"I","Style (Flat or Spring or Lock)"]

{"sheet":"MAIN LIST APP A","index":3,"n_rows":207,"n_cols":7,"rows_kept":207,"cut":false,"hidden":true,"merged":[[185,0,188,0],[189,0,195,0],[196,0,201,0],[202,0,206,0],[9,2,20,3],[9,0,20,0],[99,1,100,1],[108,1,109,1],[114,1,115,1],[116,1,117,1],[169,0,184,0],[47,2,52,3],[53,2,59,3],[53,0,59,0],[108,2,109,2],[108,3,109,3],[0,0,0,4],[1,0,1,4],[3,0,8,0],[21,2,28,3],[39,2,46,3],[21,0,28,0],[29,0,38,0],[39,0,46,0],[99,4,100,4],[67,0,74,0],[78,0,81,0],[82,0,86,0],[87,0,92,0],[93,0,103,0],[75,0,77,0],[99,2,100,2],[99,3,100,3],[101,2,102,2],[101,3,102,3],[101,4,102,4],[101,1,102,1],[47,0,52,0],[60,0,66,0],[133,3,134,3],[133,4,134,4],[129,0,135,0],[133,1,134,1],[116,2,117,2],[116,3,117,3],[116,4,117,4],[104,0,117,0],[118,0,122,0],[123,0,128,0],[108,4,109,4],[114,2,115,2],[114,3,115,3],[114,4,115,4],[136,0,142,0],[143,0,150,0],[151,0,155,0],[156,0,168,0],[133,2,134,2]]}
["Tank Car Containment Parts and Materials - CTQ Inspection Criteria"]
["D – Document Verification (certificates); I – Inspection Verification (Marking); M – Measurement Verification Criteria",null,null,null,null,null,"JULY 9TH 2020"]
["Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material","Certified Mill Test Report","I","D","D"]
[null,"Material Specification and Grade","D","D","D"]
[null,"Thickness Readings","M","M","M"]
[null,"Radius (If Applicable)","M","M","M"]
[null,"Rolling Direction (If Applicable)","M","I","I"]
[null,"Material Marking","I","I","I"]
["Socket Head Cap Screws","Material Specification","Per ASME B18.18 &\nASTM F1470\n",null,"D"]
[null,"Finish (plain, zinc, other)",null,null,"I"]
[null,"Marking (if specified)",null,null,"I or D"]
[null,"Thread Specification",null,null,"D"]
[null,"Overall Length",null,null,"M"]
[null,"Minimum Thread Length",null,null,"M"]
[null,"Head Diameter",null,null,"M"]
[null,"Screw Diameter",null,null,"M"]
[null,"Head Type (plain, knurled)",null,null,"I"]
[null,"Head Chamfer angle (30 or 45 degrees)",null,null,"M"]
[null,"Nominal Hex Socket Size",null,null,"M"]
[null,"Nominal Hex Socket Depth",null,null,"M"]
["Bolts","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Thread Specification",null,null,"D"]
[null,"Overall Length",null,null,"M"]
[null,"Length of Threads",null,null,"M"]
[null,"Length of Shoulder",null,null,"M"]
[null,"Diameter",null,null,"M"]
[null,"Head size across flats",null,null,"M"]
["Eyebolts","Material Specification","D","D","D"]
[null,"Marking","I","I","I"]
[null,"Thread Specification","M","M","D"]
[null,"Overall Length","M","M","M"]
[null,"Length of Threads","M","M","M"]
[null,"Length of Shoulder","M","M","M"]
[null,"Diameter","M","M","M"]
[null,"Nut length across flats and thickness","M","M","M"]
[null,"Nut style square/hex","M","M","M"]
[null,"Eyelet ID/OD","M","M","M"]
["Stud Bolts","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Thread Specification",null,null,"D"]
[null,"Overall Length",null,null,"M"]
[null,"Length of Threads",null,null,"M"]
[null,"Length of Shoulder",null,null,"M"]
[null,"Stud end chamfer and radius configuration",null,null,"D"]
[null,"Diameter",null,null,"M"]
["Nut","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Thread Specification",null,null,"D"]
[null,"Length across flats",null,null,"M"]
[null,"Thickness",null,null,"M"]
[null,"Style (Square or Hex)",null,null,"I"]
["Washer","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Inside Diameter",null,null,"M"]
[null,"Outside Diameter",null,null,"M"]
[null,"Thickness",null,null,"M"]
[null,"Flatness",null,null,"M"]
[null,"Style (Flat or Spring or Lock)",null,null,"I"]
["Flanges","Material Specification","D","D","D"]
[null,"Inside Diameter (if required)","M","M","M"]
[null,"Outside Diameter","M","M","M"]
[null,"Thickness","M","M","M"]
[null,"Mounting Style (Flat Face, Raised, or Tongue and"]
[null,"Groove)","M","M","D"]
[null,"Machined Characteristics /Gasket Surface","M","M","I"]
["Fittings Plate with no nozzles","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Thickness","M","M","D"]
[null,"Mounting Style (Opening Style, Flat Face, Raised,"]
[null,"or Tongue and Groove)","M","M","D"]
[null,"Gauge tapped threads","M","M","M"]
[null,"Machined Characteristics / Gasket Surface /","M","M","D"]
[null,"fitting holes/bolt holes"]
["Pipe Plugs","Material Specification","D","D","D"]
[null,"Thread Specification gauge threads","M","M","D"]
[null,"Diameter","M","M","D"]
["Bottom Outlet Valve Sump – No Opening","Material Specification","D","D","D"]
[null,"Marking","I","I","I"]
[null,"Dimensional","M","M","D"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Bottom Outlet Valve Saddle – Drain Opening","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Marking","I","I","I"]
[null,"Dimensional","M","M","D"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Spool","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Flange Dimensions","M","M","D"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I"]
[null,"Pipe Dimensions","M","M","M"]
["Fittings Plate with Welded Nozzle(s)","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Inside Diameter","M","M","D"]
[null,"Outside Diameter","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Nozzle Dimensions","M","M","D"]
[null,"Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)","I","I","I"]
[]
[null,"Machined Characteristics / Gasket Surface /fitting holes/bolt holes/bolt pattern","M","M","I"]
[]
[null,"Weld Size and Type","I","I","I"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Nozzle Dimensions","M","M","D"]
[null,"Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)","I","I","I"]
[]
[null,"Bolt Pattern","M","M","D"]
[null,"Weld Size and Type","I","I","I"]
[null,"Hinge Position","M","M","D"]
[null,"Bolt Slot Opening Dimensions","M","M","D"]
[null,"Gasket Groove Dimensions (I.D., O.D., Finish,and Profile)","M","M","D"]
[]
[null,"Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)","M","M","D"]
[]
["Thermowell","Material Specification","D","D","D"]
[null,"AAR Device Approval","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Thread Specification","M","M","D"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I"]
["Hinged and Bolted Nozzle Assembly","Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Weld Size and Type","I","I","I"]
[null,"Hinge Position","M","M","D"]
[null,"Eyebolt Lug Position","M","M","D"]
["Flanged Nozzle","Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Diameter","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Machined Characteristics / Gasket Surface /fitting holes/bolt holes/ bolt pattern","M","M","I"]
[]
[null,"Weld Size and Type (Forged or Cast)","I","I","I"]
["Eduction Pipe Assembly","Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Thread Specification (If Applicable)","M","M","D"]
[null,"Diameter","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Machined Characteristics","M","M","I"]
[null,"Weld Size and Type","I","I","I"]
["Hinged and Bolted Manway Covers","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Structural Integrity – Pressure Test","M","M","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Bolt Pattern","M","M","D"]
[null,"Hinge Position","M","M","D"]
[null,"Bolt Slot Opening Dimensions","M","M","D"]
[null,"Gasket Groove Dimensions","M","M","D"]
["Eduction Pipe Sump","Material Specification","D","D","D"]
[null,"Marking (If Required)","I","I","I"]
[null,"Dimensions (O.D. and Depth)","M","M","D"]
[null,"Structural Integrity – Pressure Test","M","M","D"]
[null,"Thickness","M","M","M"]
["Loading/Unloading, and Sample Valves","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","I"]
[null,"Connection – Thread Specification","M","D","I"]
[null,"Body Length","M","D","D"]
[null,"Body Diameter","M","D","D"]
[null,"Port Opening Size","M","D","D"]
[null,"Body Material","D","D","D"]
[null,"Lining Material (If Applicable)","D","D","I"]
[null,"Seal/O-Ring Dimensions","M","D","D"]
[null,"Seal/O-Ring Material","D","D","D"]
[null,"OEM test certificate","D","D","D"]
["Vent, Vacuum Relief, and Pressure Relief Valves","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","I"]
[null,"Connection – Thread Specification","M","D","I"]
[null,"Length","M","D","D"]
[null,"Body Diameter","M","D","D"]
[null,"Body Material","D","D","D"]
[null,"Lining Material (If Applicable)","D","D","I"]
[null,"Seal/O-Ring Dimensions","M","D","D"]
[null,"Seal/O-Ring Material","D","D","D"]
[null,"Start to Discharge Pressure","D","D","D"]
[null,"Vapor Tight Pressure","D","D","D"]
[null,"Flow Rated Capacity","D","D","D"]
[null,"OEM Test Certificate","D","D","D"]
[null,"AAR Certificate of Test","D","D","D"]
["Rupture Disks","Model","I","D","D"]
[null,"Burst Rating","D","D","D"]
[null,"Structural Integrity","M","M","I"]
[null,"Certificate of Test (Per Lot)","D","D","D"]
["Spring Loaded Check Valves","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","D"]
[null,"Connection – Thread Specification","M","D","D"]
[null,"Flow Rated Capacity","D","D","D"]
[null,"OEM test certificate","D","D","D"]
["Heat and Pressure Sensors","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","D"]
[null,"Connection – Thread Specification","M","D","D"]
[null,"OEM test certificate","D","D","D"]
["Gaskets and O-Rings","Material Specification","D","D","D"]
[null,"Marking (if applicable)","D","D","I"]
[null,"Inside Diameter","M","M","D"]
[null,"Outside Diameter","M","M","D"]
[null,"Thickness","M","M","D"]

{"sheet":"latest table 9","index":4,"n_rows":225,"n_cols":19,"rows_kept":225,"cut":false,"hidden":true,"merged":[[202,2,210,3],[210,7,218,7],[212,11,213,11],[210,8,218,8],[211,0,216,0],[219,7,224,7],[219,8,224,8],[1,0,1,4],[2,0,2,4],[3,0,3,4],[4,0,4,4],[6,0,10,0],[11,0,14,0],[61,0,70,0],[61,8,70,8],[111,0,115,0],[6,8,10,8],[71,0,76,0],[60,2,60,3],[50,0,52,0],[58,2,58,3],[104,0,110,0],[104,8,110,8],[111,8,115,8],[11,14,14,14],[50,14,52,14],[53,14,53,18],[53,2,53,3],[39,0,49,0],[39,8,49,8],[50,8,52,8],[53,8,60,8],[54,14,54,18],[55,14,55,18],[56,14,56,18],[54,2,54,3],[55,2,55,3],[56,2,56,3],[57,2,57,3],[59,2,59,3],[11,8,14,8],[15,0,20,0],[15,8,20,8],[21,0,29,0],[21,8,29,8],[30,0,38,0],[30,8,38,8],[53,0,60,0],[63,16,63,17],[64,16,64,17],[65,16,65,17],[64,15,65,15],[64,18,65,18],[76,16,76,17],[58,16,58,17],[59,16,59,17],[60,16,60,17],[61,16,61,17],[62,16,62,17],[83,16,83,17],[84,16,84,17],[85,16,85,17],[86,16,86,17],[87,16,87,17],[88,16,88,17],[77,16,77,17],[78,16,78,17],[79,16,79,17],[80,16,80,17],[81,16,81,17],[82,16,82,17],[191,14,197,14],[6,14,10,14],[4,14,4,18],[154,14,154,18],[155,14,155,18],[156,14,156,18],[158,14,162,14],[163,14,163,18],[164,14,164,18],[139,15,140,15],[139,16,140,16],[139,17,140,17],[139,18,140,18],[147,14,152,14],[153,14,153,18],[107,16,107,17],[108,16,108,17],[109,14,109,18],[110,14,110,18],[111,14,111,18],[112,14,112,18],[101,16,101,17],[102,16,102,17],[103,16,103,17],[0,0,0,4],[0,7,0,10],[3,14,3,18],[2,14,2,18],[1,14,1,18],[2,7,3,10],[165,14,165,18],[166,14,166,18],[168,14,173,14],[104,16,104,17],[105,16,105,17],[106,16,106,17],[95,16,95,17],[96,16,96,17],[97,16,97,17],[98,16,98,17],[99,16,99,17],[100,16,100,17],[89,16,89,17],[90,16,90,17],[91,16,91,17],[92,16,92,17],[93,16,93,17],[94,16,94,17],[77,2,88,3],[89,2,96,3],[97,2,103,3],[71,2,71,3],[72,2,72,3],[116,8,121,8],[122,0,127,0],[122,8,127,8],[71,8,76,8],[77,0,88,0],[77,8,88,8],[89,0,96,0],[89,8,96,8],[97,0,103,0],[97,8,103,8],[73,2,73,3],[74,2,74,3],[75,2,75,3],[76,2,76,3],[116,0,121,0],[202,8,209,8],[170,0,173,0],[170,8,173,8],[174,8,180,8],[181,0,185,0],[181,8,185,8],[186,0,201,0],[186,8,201,8],[128,8,133,8],[134,8,139,8],[140,8,145,8],[146,8,150,8],[151,8,156,8],[157,0,169,0],[157,8,169,8],[128,0,133,0],[134,0,139,0],[174,0,180,0],[140,0,145,0],[146,0,150,0],[151,0,156,0],[204,1,205,1],[204,4,205,4],[202,0,210,0]]}
["COPY & PASTER NEW TABEL 9 HERE",null,null,null,null,null,null,"ADJUST , EDIT THEN COPY AND PASTE \nTHIS TO FORMTAB"]
["CLOSURES - CTQ INSPECTION CRITERIA",null,null,null,null,null,null,null,null,null,null,null,null,null,"CLOSURES - CTQ INSPECTION CRITERIA"]
["D – Document Verification (certificates); I – Inspection Verification (Marking); and ",null,null,null,null,null,null,null,null,null,null,null,null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
["M – Measurement Verification Criteria",null,null,null,null,null,null,null,null,null,null,null,null,null,"M – Measurement Verification Criteria"]
[]
["Item","Inspection Criteria","Manufacturer","Distributor","Facility",">>>>>>",null,"seelct","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
["Bottom Outlet Valve Saddle – Drain Opening","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Bottom Outlet Valve Saddle – Drain Opening","Bottom Outlet Valve Saddle – Drain Opening",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,"Bottom Outlet Valve Saddle – Drain Opening","AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null,"D","Material Specification",null,null,null,"Material Specification","D","D","D"]
[null,"Marking","I","I","I",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Marking",null,null,null,"Marking","I","I","I"]
[null,"Dimensional","M","M"," M",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null," M","Dimensional",null,null,null,"Dimensional","M","M"," M"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)",null,null,null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Bottom Outlet Valve Sump – No Opening","Material Specification","D","D","D ",null,null,"Bottom Outlet Valve Sump – No Opening","Bottom Outlet Valve Sump – No Opening",null,"D ","Material Specification",null,null,"Bottom Outlet Valve Sump – No Opening","Material Specification","D","D","D "]
[null,"Marking","I","I","I",null,null,"Bottom Outlet Valve Sump – No Opening",null,null,"I","Marking",null,null,null,"Marking","I","I","I"]
[null,"Dimensional","M","M"," M",null,null,"Bottom Outlet Valve Sump – No Opening",null,null," M","Dimensional",null,null,null,"Dimensional","M","M"," M"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I",null,null,"Bottom Outlet Valve Sump – No Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)",null,null,null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Fittings Plate with no nozzles","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Fittings Plate with no nozzles","Fittings Plate with no nozzles",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Fittings Plate with no nozzles",null,null,"D","Material Specification",null,null,"Fittings Plate with no nozzles","Material Specification","D","D","D"]
[null,"Thickness","M","M","D",null,null,"Fittings Plate with no nozzles",null,null,"D","Thickness",null,null,null,"Thickness","M","M","D"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","M","M","D",null,null,"Fittings Plate with no nozzles",null,null,"D","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)",null,null,null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","M","M","D"]
[null,"Gauge tapped threads ","M","M","M",null,null,"Fittings Plate with no nozzles",null,null,"M","Gauge tapped threads ",null,null,null,"Gauge tapped threads ","M","M","M"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes","M","M","I &M",null,null,"Fittings Plate with no nozzles",null,null,"I &M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes",null,null,null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes","M","M","I &M"]
["Fittings Plate with Welded Nozzle(s)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Fittings Plate with Welded Nozzle(s)","Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D ",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"D ","Material Specification",null,null,"Fittings Plate with Welded Nozzle(s)","Material Specification","D","D","D "]
[null,"Inside Diameter","M","M"," M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null," M","Inside Diameter",null,null,null,"Inside Diameter","M","M"," M"]
[null,"Outside Diameter","M","M"," M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null," M","Outside Diameter",null,null,null,"Outside Diameter","M","M"," M"]
[null,"Thickness","M","M","M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"M","Thickness",null,null,null,"Thickness","M","M","M"]
[null,"Nozzle Dimensions","M","M","M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"M","Nozzle Dimensions",null,null,null,"Nozzle Dimensions","M","M","M"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)",null,null,null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern","M","M","I & M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern",null,null,null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern","M","M","I & M"]
[null,"Weld Size and Type","I","I","I",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"I","Weld Size and Type",null,null,null,"Weld Size and Type","I","I","I"]
["Hinged and Bolted Manway Covers (Cast)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Hinged and Bolted Manway Covers (Cast)","Hinged and Bolted Manway Covers (Cast)",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"D","Material Specification",null,null,"Hinged and Bolted Manway Covers","Material Specification","D","D","D"]
[null,"Structural Integrity – Pressure Test ","M","M","D ",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"D ","Structural Integrity – Pressure Test ",null,null,"(Cast)","Structural Integrity – Pressure Test ","M","M","D "]
[null,"Casting Quality","I","D","D",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"D","Casting Quality",null,null,null,"Casting Quality","I","D","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"I","Thickness (Dished, Flanged, or Grooved)",null,null,null,"Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Bolt Pattern","M","M","I",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"I","Bolt Pattern",null,null,null,"Bolt Pattern","M","M","I"]
[null,"Hinge Position","M","M","I",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"I","Hinge Position",null,null,null,"Hinge Position","M","M","I"]
[null,"Bolt Slot Opening Dimensions","M","M","M",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"M","Bolt Slot Opening Dimensions",null,null,null,"Bolt Slot Opening Dimensions","M","M","M"]
[null,"Gasket Groove Dimensions","M","M","M",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"M","Gasket Groove Dimensions",null,null,null,"Gasket Groove Dimensions","M","M","M"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Material Specification",null,null,null,"Material Specification","D","D","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Thickness (Dished, Flanged, or Grooved)",null,null,"Hinged and Bolted Manway or Fill Hole Cover ","Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Nozzle Dimensions","M","M"," M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Nozzle Dimensions",null,null,"(Fabricated)","Nozzle Dimensions","M","M"," M"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)",null,null,null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I"]
[null,"Bolt Pattern","M","M","D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Bolt Pattern",null,null,null,"Bolt Pattern","M","M","D"]
[null,"Weld Size and Type","I","I","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Weld Size and Type",null,null,null,"Weld Size and Type","I","I","I"]
[null,"Hinge Position","M","M","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Hinge Position",null,null,null,"Hinge Position","M","M","I"]
[null,"Bolt Slot Opening Dimensions","M","M"," M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Bolt Slot Opening Dimensions",null,null,null,"Bolt Slot Opening Dimensions","M","M"," M"]
[null,"Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)","M","M"," M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)",null,null,null,"Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)","M","M"," M"]
[null,"Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)","M","M"," I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," I","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)",null,null,null,"Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)","M","M"," I"]
["Pipe Plugs","Material Specification","D","D","D",null,null,"Pipe Plugs","Pipe Plugs",null,"D","Material Specification",null,null,"Pipe Plugs","Material Specification","D","D","D"]
[null,"Thread Specification ","M","M","D & M",null,null,"Pipe Plugs",null,null,"D & M","Thread Specification ",null,null,null,"Thread Specification ","M","M","D & M"]
[null,"Diameter","M","M","M",null,null,"Pipe Plugs",null,null,"M","Diameter",null,null,null,"Diameter","M","M","M"]
["Bolts","Material Specification",null,null,"D",null,null,"Bolts","Bolts",null,"D","Material Specification",null,null,"FASTENERS - CTQ INSPECTION CRITERIA"]
[null,"Marking","Per ASME B18.18 &",null,"I",null,null,"Bolts",null,null,"I","Marking",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
[null,"Thread Specification","ASTM F1470",null,"D",null,null,"Bolts",null,null,"D","Thread Specification",null,null,"M – Measurement Verification Criteria"]
[null,"Overall Length",null,null,"M",null,null,"Bolts",null,null,"M","Overall Length"]
[null,"Length of Threads",null,null,"M",null,null,"Bolts",null,null,"M","Length of Threads",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Length of Shoulder",null,null,"M",null,null,"Bolts",null,null,"M","Length of Shoulder",null,null,null,"Material Specification",null,null,"D"]
[null,"Diameter",null,null,"M",null,null,"Bolts",null,null,"M","Diameter",null,null,null,"Marking","Per ASME B18.18 &",null,"I"]
[null,"Head size across flats",null,null,"M",null,null,"Bolts",null,null,"M","Head size across flats",null,null,"Bolts","Thread Specification","ASTM F1470",null,"D"]
["Eyebolts","Material Specification","D","D","D",null,null,"Eyebolts","Eyebolts",null,"D","Material Specification",null,null,null,"Length of Threads",null,null,"M"]
[null,"Marking","I","I","I",null,null,"Eyebolts",null,null,"I","Marking",null,null,null,"Length of Shoulder",null,null,"M"]
[null,"Thread Specification","M","M","D",null,null,"Eyebolts",null,null,"D","Thread Specification",null,null,null,"Diameter",null,null,"M"]
[null,"Overall Length","M","M","M",null,null,"Eyebolts",null,null,"M","Overall Length",null,null,null,"Head size across flats",null,null,"M"]
[null,"Length of Threads","M","M","M",null,null,"Eyebolts",null,null,"M","Length of Threads"]
[null,"Length of Shoulder","M","M","M",null,null,"Eyebolts",null,null,"M","Length of Shoulder",null,null,null,"Material Specification","D","D","D"]
[null,"Diameter","M","M","M",null,null,"Eyebolts",null,null,"M","Diameter",null,null,null,"Marking","I","I","I"]
[null,"Nut length across flats and thickness","M","M","M",null,null,"Eyebolts",null,null,"M","Nut length across flats and thickness",null,null,"Eyebolts","Thread Specification","M","M","D"]
[null,"Nut style square/hex","M","M","M",null,null,"Eyebolts",null,null,"M","Nut style square/hex",null,null,null,"Overall Length","M","M","M"]
[null,"Eyelet ID/OD","M","M","M",null,null,"Eyebolts",null,null,"M","Eyelet ID/OD",null,null,null,"Length of Threads","M","M","M"]
["Nut","Material Specification","Per ASME B18.18 &",null,"D",null,null,"Nut","Nut",null,"D","Material Specification",null,null,null,"Length of Shoulder","M","M","M"]
[null,"Marking","ASTM F1470",null,"I",null,null,"Nut",null,null,"I","Marking",null,null,null,"Diameter","M","M","M"]
[null,"Thread Specification",null,null,"D",null,null,"Nut",null,null,"D","Thread Specification",null,null,null,"Nut length across flats and thickness","M","M","M"]
[null,"Length across flats",null,null,"M",null,null,"Nut",null,null,"M","Length across flats",null,null,null,"Nut style square/hex","M","M","M"]
[null,"Thickness",null,null,"M",null,null,"Nut",null,null,"M","Thickness",null,null,null,"Eyelet ID/OD","M","M","M"]
[null,"Style (Square or Hex)",null,null,"I",null,null,"Nut",null,null,"I","Style (Square or Hex)",null,null,null,"Material Specification","Per ASME B18.18 &",null,"D"]
["Socket Head Cap Screws","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D",null,null,"Socket Head Cap Screws","Socket Head Cap Screws",null,"D","Material Specification",null,null,"Nut","Marking","ASTM F1470",null,"I"]
[null,"Finish (plain, zinc, other)",null,null,"I",null,null,"Socket Head Cap Screws",null,null,"I","Finish (plain, zinc, other)",null,null,null,"Thread Specification",null,null,"D"]
[null,"Marking (if specified)",null,null,"I ",null,null,"Socket Head Cap Screws",null,null,"I ","Marking (if specified)",null,null,null,"Length across flats",null,null,"M"]
[null,"Thread Specification",null,null,"D",null,null,"Socket Head Cap Screws",null,null,"D","Thread Specification",null,null,null,"Thickness",null,null,"M"]
[null,"Overall Length",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Overall Length",null,null,null,"Style (Square or Hex)",null,null,"I"]
[null,"Minimum Thread Length",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Minimum Thread Length",null,null,null,"Material Specification",null,null,"D"]
[null,"Head Diameter",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Head Diameter",null,null,null,"Finish (plain, zinc, other)","Per ASME B18.18 &",null,"I"]
[null,"Screw Diameter",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Screw Diameter",null,null,"Socket Head Cap Screws","Marking (if specified)","ASTM F1470",null,"I "]
[null,"Head Type (plain, knurled)",null,null,"I",null,null,"Socket Head Cap Screws",null,null,"I","Head Type (plain, knurled)",null,null,null,"Thread Specification",null,null,"D"]
[null,"Head Chamfer angle (30 or 45 degrees)",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Head Chamfer angle (30 or 45 degrees)",null,null,null,"Overall Length",null,null,"M"]
[null,"Nominal Hex Socket Size",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Size",null,null,null,"Minimum Thread Length",null,null,"M"]
[null,"Nominal Hex Socket Depth",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Depth",null,null,null,"Head Diameter",null,null,"M"]
["Stud Bolts","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D",null,null,"Stud Bolts","Stud Bolts",null,"D","Material Specification",null,null,null,"Screw Diameter",null,null,"M"]
[null,"Marking",null,null,"I",null,null,"Stud Bolts",null,null,"I","Marking",null,null,null,"Head Type (plain, knurled)",null,null,"I"]
[null,"Thread Specification",null,null,"D",null,null,"Stud Bolts",null,null,"D","Thread Specification",null,null,null,"Head Chamfer angle (30 or 45 degrees)",null,null,"M"]
[null,"Overall Length",null,null,"M",null,null,"Stud Bolts",null,null,"M","Overall Length",null,null,null,"Nominal Hex Socket Size",null,null,"M"]
[null,"Length of Threads",null,null,"M",null,null,"Stud Bolts",null,null,"M","Length of Threads",null,null,null,"Nominal Hex Socket Depth",null,null,"M"]
[null,"Length of Shoulder",null,null,"M",null,null,"Stud Bolts",null,null,"M","Length of Shoulder",null,null,null,"Material Specification",null,null,"D"]
[null,"Stud end chamfer and radius configuration",null,null,"D",null,null,"Stud Bolts",null,null,"D","Stud end chamfer and radius configuration",null,null,"Stud Bolts","Marking","Per ASME B18.18 &",null,"I"]
[null,"Diameter",null,null,"M",null,null,"Stud Bolts",null,null,"M","Diameter",null,null,null,"Thread Specification","ASTM F1470",null,"D"]
["Washer","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D",null,null,"Washer","Washer",null,"D","Material Specification",null,null,null,"Overall Length",null,null,"M"]
[null,"Marking",null,null,"I",null,null,"Washer",null,null,"I","Marking",null,null,null,"Length of Threads",null,null,"M"]
[null,"Inside Diameter",null,null,"M",null,null,"Washer",null,null,"M","Inside Diameter",null,null,null,"Length of Shoulder",null,null,"M"]
[null,"Outside Diameter",null,null,"M",null,null,"Washer",null,null,"M","Outside Diameter",null,null,null,"Stud end chamfer and radius configuration",null,null,"D"]
[null,"Thickness",null,null,"M",null,null,"Washer",null,null,"M","Thickness",null,null,null,"Diameter",null,null,"M"]
[null,"Flatness",null,null,"M",null,null,"Washer",null,null,"M","Flatness",null,null,null,"Material Specification","Per ASME B18.18 &",null,"D"]
[null,"Style (Flat or Spring or Lock)",null,null,"I",null,null,"Washer",null,null,"I","Style (Flat or Spring or Lock)",null,null,"Washer","Marking","ASTM F1470",null,"I"]
["Eduction Pipe Assembly","Material Specification","D","D","D",null,null,"Eduction Pipe Assembly","Eduction Pipe Assembly",null,"D","Material Specification",null,null,null,"Inside Diameter",null,null,"M"]
[null,"Length Overall","M","M","     M",null,null,"Eduction Pipe Assembly",null,null,"     M","Length Overall",null,null,null,"Outside Diameter",null,null,"M"]
[null,"Thread Specification (If Applicable)","M","M","D & M",null,null,"Eduction Pipe Assembly",null,null,"D & M","Thread Specification (If Applicable)",null,null,null,"Thickness",null,null,"M"]
[null,"Diameter","M","M"," M",null,null,"Eduction Pipe Assembly",null,null," M","Diameter",null,null,null,"Flatness",null,null,"M"]
[null,"Thickness","M","M","M",null,null,"Eduction Pipe Assembly",null,null,"M","Thickness",null,null,null,"Style (Flat or Spring or Lock)",null,null,"I"]
[null,"Machined Characteristics","M","M","I & M",null,null,"Eduction Pipe Assembly",null,null,"I & M","Machined Characteristics",null,null,"PRESSURE CONTAINING TANK CAR TANK COMPONENTS - CTQ INSPECTION CRITERIA"]
[null,"Weld Size and Type","I","I","I",null,null,"Eduction Pipe Assembly",null,null,"I","Weld Size and Type",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
["Eduction Pipe Sump","Material Specification","D","D","D",null,null,"Eduction Pipe Sump","Eduction Pipe Sump",null,"D","Material Specification",null,null,"M – Measurement Verification Criteria"]
[null,"Marking (If Required)","I","I","I",null,null,"Eduction Pipe Sump",null,null,"I","Marking (If Required)"]
[null,"Dimensions (O.D. and Depth)","M","M","M",null,null,"Eduction Pipe Sump",null,null,"M","Dimensions (O.D. and Depth)",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Structural Integrity – Pressure Test","M","M","D ",null,null,"Eduction Pipe Sump",null,null,"D ","Structural Integrity – Pressure Test",null,null,null,"Diameter","M","M"," M"]
[null,"Thickness","M","M","M",null,null,"Eduction Pipe Sump",null,null,"M","Thickness",null,null,null,"Thickness","M","M","M"]
["Flanged Nozzle","Material Specification","D","D","D",null,null,"Flanged Nozzle","Flanged Nozzle",null,"D","Material Specification",null,null,null,"Machined Characteristics","M","M","I & M"]
[null,"Length Overall","M","M"," M",null,null,"Flanged Nozzle",null,null," M","Length Overall",null,null,null,"Weld Size and Type","I","I","I"]
[null,"Diameter","M","M","M",null,null,"Flanged Nozzle",null,null,"M","Diameter",null,null,null,"Material Specification","D","D","D"]
[null,"Thickness","M","M","M",null,null,"Flanged Nozzle",null,null,"M","Thickness",null,null,"Eduction Pipe Sump","Marking (If Required)","I","I","I"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern","M","M","I & M",null,null,"Flanged Nozzle",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern",null,null,null,"Dimensions (O.D. and Depth)","M","M","M"]
[null,"Weld Size and Type (Forged or Cast)","I","I","I",null,null,"Flanged Nozzle",null,null,"I","Weld Size and Type (Forged or Cast)",null,null,null,"Structural Integrity – Pressure Test","M","M","D "]
["Flanges","Material Specification","D","D","D",null,null,"Flanges","Flanges",null,"D","Material Specification",null,null,null,"Thickness","M","M","M"]
[null,"Inside Diameter (if required)","M","M","M",null,null,"Flanges",null,null,"M","Inside Diameter (if required)",null,null,null,"Material Specification","D","D","D"]
[null,"Outside Diameter","M","M","M",null,null,"Flanges",null,null,"M","Outside Diameter",null,null,"Flanged Nozzle","Length Overall","M","M"," M"]
[null,"Thickness","M","M","M",null,null,"Flanges",null,null,"M","Thickness",null,null,null,"Diameter","M","M","M"]
[null,"Sealing Style (Flat Face, Raised, or Tongue and Groove)","M","M","I",null,null,"Flanges",null,null,"I","Sealing Style (Flat Face, Raised, or Tongue and Groove)",null,null,null,"Thickness","M","M","M"]
[null,"Machined Characteristics /Gasket Surface","M","M","I",null,null,"Flanges",null,null,"I","Machined Characteristics /Gasket Surface",null,null,null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern","M","M","I & M"]
["Hinged and Bolted Nozzle Assembly","Material Specification","D","D","D",null,null,"Hinged and Bolted Nozzle Assembly","Hinged and Bolted Nozzle Assembly",null,"D","Material Specification",null,null,null,"Weld Size and Type (Forged or Cast)","I","I","I"]
[null,"Length Overall","M","M","M",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"M","Length Overall",null,null,null,"Material Specification","D","D","D"]
[null,"Thickness","M","M","M",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"M","Thickness",null,null,"Flanges","Inside Diameter (if required)","M","M","M"]
[null,"Weld Size and Type","I","I","I",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"I","Weld Size and Type",null,null,null,"Outside Diameter","M","M","M"]
[null,"Hinge Position","M","M","I",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"I","Hinge Position",null,null,null,"Thickness","M","M","M"]
[null,"Eyebolt Lug Position","M","M","M",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"M","Eyebolt Lug Position",null,null,null,"Sealing Style (Flat Face, Raised, or Tongue and Groove)","M","M","I"]
["Spool","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Spool","Spool",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"Material Specification","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Spool",null,null,"D","Material Specification",null,null,"Hinged and Bolted Nozzle Assembly","Length Overall","M","M","M"]
[null,"Length Overall","M","M"," M",null,null,"Spool",null,null," M","Length Overall",null,null,null,"Thickness","M","M","M"]
[null,"Flange Dimensions","M","M","M",null,null,"Spool",null,null,"M","Flange Dimensions",null,null,null,"Weld Size and Type","I","I","I"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I",null,null,"Spool",null,null,"I","Mounting Style (Bolted or Threaded)",null,null,null,"Hinge Position","M","M","I"]
[null,"Pipe Dimensions","M","M","M",null,null,"Spool",null,null,"M","Pipe Dimensions",null,null,null,"Eyebolt Lug Position","M","M","M"]
["Tank Shell and Manway Nozzles ","Certified Mill Test Report","I","D","D",null,null,"Tank Shell and Manway Nozzles ","Tank Shell and Manway Nozzles ",null,"D","Certified Mill Test Report"]
[null,"Material Specification and Grade","D","D","D",null,null,"Tank Shell and Manway Nozzles ",null,null,"D","Material Specification and Grade",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Thickness ","M","M","M",null,null,"Tank Shell and Manway Nozzles ",null,null,"M","Thickness ",null,null,"Spool","Material Specification","D","D","D"]
[null,"Radius (If Applicable)","M","M","M",null,null,"Tank Shell and Manway Nozzles ",null,null,"M","Radius (If Applicable)",null,null,null,"Length Overall","M","M"," M"]
[null,"Rolling Direction (If Applicable)","M","I","I",null,null,"Tank Shell and Manway Nozzles ",null,null,"I","Rolling Direction (If Applicable)",null,null,null,"Flange Dimensions","M","M","M"]
[null,"Material Marking","I","I","I",null,null,"Tank Shell and Manway Nozzles ",null,null,"I","Material Marking",null,null,null,"Mounting Style (Bolted or Threaded)","M","M","I"]
["Gaskets and O-Rings","Material Specification","D","D","D",null,null,"Gaskets and O-Rings","Gaskets and O-Rings",null,"D","Material Specification",null,null,null,"Pipe Dimensions","M","M","M"]
[null,"Marking (if applicable)","D","D","I",null,null,"Gaskets and O-Rings",null,null,"I","Marking (if applicable)",null,null,"Tank Shell and Manway Nozzles ","Certified Mill Test Report","I","D","D"]
[null,"Inside Diameter","M","M","M",null,null,"Gaskets and O-Rings",null,null,"M","Inside Diameter",null,null,null,"Material Specification and Grade","D","D","D"]
[null,"Outside Diameter","M","M","M",null,null,"Gaskets and O-Rings",null,null,"M","Outside Diameter",null,null,null,"Thickness ","M","M","M"]
[null,"Thickness","M","M"," M",null,null,"Gaskets and O-Rings",null,null," M","Thickness",null,null,null,"Radius (If Applicable)","M","M","M"]
["Heat and Pressure Sensors","AAR Device Approval ","D","D","D",null,null,"Heat and Pressure Sensors","Heat and Pressure Sensors",null,"D","AAR Device Approval ",null,null,null,"Rolling Direction (If Applicable)","M","I","I"]
[null,"Model","I","D","D",null,null,"Heat and Pressure Sensors",null,null,"D","Model",null,null,null,"Material Marking","I","I","I"]
[null,"Manufacturing Facility","D","D","D",null,null,"Heat and Pressure Sensors",null,null,"D","Manufacturing Facility",null,null,"GASKETS AND O-RINGS - CTQ INSPECTION CRITERIA"]
[null,"Connection – Flange Dimensions","M","D","M",null,null,"Heat and Pressure Sensors",null,null,"M","Connection – Flange Dimensions",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
[null,"Connection – Thread Specification","M","D","D & M",null,null,"Heat and Pressure Sensors",null,null,"D & M","Connection – Thread Specification",null,null,"M – Measurement Verification Criteria"]
[null,"OEM test certificate","D","D","D",null,null,"Heat and Pressure Sensors",null,null,"D","OEM test certificate"]
["Loading/Unloading, and Sample Valves","AAR Device Approval ","D","D","D",null,null,"Loading/Unloading, and Sample Valves","Loading/Unloading, and Sample Valves",null,"D","AAR Device Approval ",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Model","I","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Model",null,null,"Gaskets and O-Rings","Material Specification","D","D","D"]
[null,"Manufacturing Facility","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Manufacturing Facility",null,null,null,"Marking (if applicable)","D","D","I"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Loading/Unloading, and Sample Valves",null,null,"I","Connection – Flange Dimensions",null,null,null,"Inside Diameter","M","M","M"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Loading/Unloading, and Sample Valves",null,null,"I","Connection – Thread Specification",null,null,null,"Outside Diameter","M","M","M"]
[null,"Body Length","M","D","M",null,null,"Loading/Unloading, and Sample Valves",null,null,"M","Body Length",null,null,null,"Thickness","M","M"," M"]
[null,"Body Diameter","M","D","      M",null,null,"Loading/Unloading, and Sample Valves",null,null,"      M","Body Diameter",null,null,"VALVES AND INSTRUMENTS - CTQ INSPECTION CRITERIA"]
[null,"Port Opening Size","M","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Port Opening Size",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
[null,"Body Material","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Body Material",null,null,"M – Measurement Verification Criteria"]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Loading/Unloading, and Sample Valves",null,null,"I","Lining Material (If Applicable)"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Dimensions",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Material",null,null,"Heat and Pressure Sensors","AAR Device Approval ","D","D","D"]
[null,"OEM test certificate","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","OEM test certificate",null,null,null,"Model","I","D","D"]
["Rupture Disks","Model","I","D","D",null,null,"Rupture Disks","Rupture Disks",null,"D","Model",null,null,null,"Manufacturing Facility","D","D","D"]
[null,"Burst Rating","D","D","D",null,null,"Rupture Disks",null,null,"D","Burst Rating",null,null,null,"Connection – Flange Dimensions","M","D","M"]
[null,"Structural Integrity","M","M","I",null,null,"Rupture Disks",null,null,"I","Structural Integrity",null,null,null,"Connection – Thread Specification","M","D","D & M"]
[null,"Certificate of Test (Per Lot)","D","D","D",null,null,"Rupture Disks",null,null,"D","Certificate of Test (Per Lot)",null,null,null,"OEM test certificate","D","D","D"]
["Spring Loaded Check Valves","AAR Device Approval ","D","D","D",null,null,"Spring Loaded Check Valves","Spring Loaded Check Valves",null,"D","AAR Device Approval ",null,null,null,"AAR Device Approval ","D","D","D"]
[null,"Model","I","D","D",null,null,"Spring Loaded Check Valves",null,null,"D","Model",null,null,null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D ",null,null,"Spring Loaded Check Valves",null,null,"D ","Manufacturing Facility",null,null,"Loading/Unloading, and Sample Valves","Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","M",null,null,"Spring Loaded Check Valves",null,null,"M","Connection – Flange Dimensions",null,null,null,"Connection – Flange Dimensions","M","D","I"]
[null,"Connection – Thread Specification","M","D","D & M",null,null,"Spring Loaded Check Valves",null,null,"D & M","Connection – Thread Specification",null,null,null,"Connection – Thread Specification","M","D","I"]
[null,"Flow Rated Capacity","D","D","D",null,null,"Spring Loaded Check Valves",null,null,"D","Flow Rated Capacity",null,null,null,"Body Length","M","D","M"]
[null,"OEM test certificate","D","D","D",null,null,"Spring Loaded Check Valves",null,null,"D","OEM test certificate",null,null,null,"Body Diameter","M","D","      M"]
["Thermowell","Material Specification","D","D","D",null,null,"Thermowell","Thermowell",null,"D","Material Specification",null,null,null,"Port Opening Size","M","D","D"]
[null,"AAR Device Approval ","D","D","D",null,null,"Thermowell",null,null,"D","AAR Device Approval ",null,null,null,"Body Material","D","D","D"]
[null,"Length Overall","M","M","M",null,null,"Thermowell",null,null,"M","Length Overall",null,null,null,"Lining Material (If Applicable)","D","D","I"]
[null,"Thread Specification","M","M","D & M",null,null,"Thermowell",null,null,"D & M","Thread Specification",null,null,null,"Seal/O-Ring Dimensions","M","D","D"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I",null,null,"Thermowell",null,null,"I","Mounting Style (Bolted or Threaded)",null,null,null,"Seal/O-Ring Material","D","D","D"]
["Vent, Vacuum Relief, and Pressure Relief Valves","AAR Device Approval ","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves","Vent, Vacuum Relief, and Pressure Relief Valves",null,"D","AAR Device Approval ",null,null,null,"OEM test certificate","D","D","D"]
[null,"Model","I","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Model",null,null,null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Manufacturing Facility",null,null,"Rupture Disks","Burst Rating","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Flange Dimensions",null,null,null,"Structural Integrity","M","M","I"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Thread Specification",null,null,null,"Certificate of Test (Per Lot)","D","D","D"]
[null,"Length","M","D","M",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"M","Length",null,null,"Spring Loaded Check Valves","AAR Device Approval ","D","D","D"]
[null,"Body Diameter","M","D","M",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"M","Body Diameter",null,null,null,"Model","I","D","D"]
[null,"Body Material","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Body Material",null,null,null,"Manufacturing Facility","D","D","D "]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Lining Material (If Applicable)",null,null,null,"Connection – Flange Dimensions","M","D","M"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Dimensions",null,null,null,"Connection – Thread Specification","M","D","D & M"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Material",null,null,null,"Flow Rated Capacity","D","D","D"]
[null,"Start to Discharge Pressure","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Start to Discharge Pressure",null,null,null,"OEM test certificate","D","D","D"]
[null,"Vapor Tight Pressure","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Vapor Tight Pressure",null,null,null,"Material Specification","D","D","D"]
[null,"Flow Rated Capacity","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Flow Rated Capacity",null,null,"Thermowell","AAR Device Approval ","D","D","D"]
[null,"OEM Test Certificate","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","OEM Test Certificate",null,null,null,"Length Overall","M","M","M"]
[null,"AAR Certificate of Test","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","AAR Certificate of Test",null,null,null,"Thread Specification","M","M","D & M"]
["Segment Washer\n\n(used on rubber lined fittings)\nPCP 7","Material Specification","Per ASME B18.18,\nCategory 2. ASTM F1470",null,"D",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material","Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"D","Certified Mill Test Report",null,null,null,"Mounting Style (Bolted or Threaded)","M","M","I"]
[null,"Marking (if required)",null,null,"I",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"D","Material Specification and Grade",null,null,null,"AAR Device Approval ","D","D","D"]
[null,"Inside Radius",null,null,"M",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Thickness",null,null,null,"Model","I","D","D"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Radius (If Applicable)",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves","Manufacturing Facility","D","D","D"]
[null,"Outside Radius",null,null,"M",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Rolling Direction (If Applicable)",null,null,null,"Connection – Flange Dimensions","M","D","I"]
[null,"Thickness",null,null,"M",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Inside Diameter (If Applicable)",null,null,null,"Connection – Thread Specification","M","D","I"]
[null,"Flatness",null,null,"M",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Outside Diameter (If Applicable)",null,null,null,"Length","M","D","M"]
[null,"Bolt Circle",null,null,"M",null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Material Marking",null,null,null,"Body Diameter","M","D","M"]
[null,"Bolt Hole Diameter",null,null,"M",null,null,"Segment Washer\n\n(used on rubber lined fittings)\nPCP 7","Segment\nWasher\n(used on rubber lined cars)",null,"D","Material Specification",null,null,null,"Body Material","D","D","D"]
["Secondary Closures - Caps with w/o Camlocks \nPCP 1 \n(3 if requried)","Material Specification","D","D","D",null,null,null,null,null,"I","Marking (if required)",null,null,null,"Lining Material (If Applicable)","D","D","I"]
[null,"Thread Specification","M","M","D & M",null,null,null,null,null,"M","Inside Radius",null,null,null,"Seal/O-Ring Dimensions","M","D","D"]
[null,"Thread Depth","M","M","M",null,null,null,null,null,null,null,null,null,null,"Seal/O-Ring Material","D","D","D"]
[null,"Diameter","M","M","M",null,null,null,null,null,"M","Outside Radius",null,null,null,"Start to Discharge Pressure","D","D","D"]
[null,"Casting Quality (if required)","I","D","D",null,null,null,null,null,"M","Thickness",null,null,null,"Vapor Tight Pressure","D","D","D"]
[null,"Overall Height","M","M","M",null,null,null,null,null,"M","Flatness",null,null,null,"Flow Rated Capacity","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,"M","Bolt Circle",null,null,null,"OEM Test Certificate","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,"M","Bolt Hole Diameter",null,null,null,"AAR Certificate of Test","D","D","D"]
[null,null,null,null,null,null,null,"Secondary Closures - Caps with w/o Camlocks \nPCP 1 \n(3 if requried)","Secondary Closures - Caps with w/o Camlocks ",null,"D","Material Specification"]
[null,null,null,null,null,null,null,null,null,null,"D & M","Thread Specification"]
[null,null,null,null,null,null,null,null,null,null,"M","Thread Depth"]
[null,null,null,null,null,null,null,null,null,null,"M","Diameter"]
[null,null,null,null,null,null,null,null,null,null,"D","Casting Quality (if required)"]
[null,null,null,null,null,null,null,null,null,null,"M","Overall Height"]

{"sheet":"INSP FORM V4","index":5,"n_rows":233,"n_cols":9,"rows_kept":233,"cut":false,"hidden":true,"merged":[[10,0,16,8],[23,1,23,8],[26,1,31,1],[26,2,31,2],[32,1,39,1],[32,2,39,2],[40,1,51,1],[40,2,51,2],[52,1,61,1],[52,2,61,2],[62,1,69,1],[62,2,69,2],[70,1,75,1],[70,2,75,2],[76,1,82,1],[76,2,82,2],[83,1,88,1],[83,2,88,2],[89,1,94,1],[89,2,94,2],[95,1,97,1],[95,2,97,2],[98,1,101,1],[98,2,101,2],[102,1,106,1],[102,2,106,2],[107,1,112,1],[107,2,112,2],[113,1,123,1],[113,2,123,2],[119,3,120,3],[119,4,120,4],[121,3,122,3],[121,4,122,4],[124,1,137,1],[124,2,137,2],[128,3,129,3],[128,4,129,4],[134,3,135,3],[134,4,135,4],[136,3,137,3],[136,4,137,4],[138,1,142,1],[138,2,142,2],[143,1,148,1],[143,2,148,2],[153,7,154,7],[153,8,154,8],[156,1,162,1],[156,2,162,2],[163,1,170,1],[163,2,170,2],[149,1,155,1],[149,2,155,2],[153,3,154,3],[153,4,154,4],[153,5,154,5],[153,6,154,6],[171,1,175,1],[171,2,175,2],[176,1,188,1],[176,2,188,2],[189,1,204,1],[189,2,204,2],[222,1,226,1],[233,1,233,4],[205,1,208,1],[205,2,208,2],[209,1,215,1],[209,2,215,2],[216,1,221,1],[216,2,221,2]]}
[]
[null,null,null,null,null,null,"Form",null,"RSI-100-05"]
[null,null,null,null,null,null,"Original Date"]
[null,null,null,null,null,null,"Revision Level",null,"VER 7-28-20"]
[null,null,null,null,"Incoming Inspection"]
[null,null,null,null,"Checklist",null,"Revision Date"]
[null,null,null,null,null,null,"Revised By"]
[null,null,null,null,null,null,"Approved By "]
[]
[]
["The tank car facility receiving parts, materials, or components must ensure that the manufactures or distributor provides any requested certificates of conformance, compliance (measurement, testing or mill test reports) required by the purchasing documents that provides the objective evidence that the required inspection points noted in Appendix A of RSI-100 were in fact performed. Each facility is responsible to address the CTC characteristics/requirements identified in Appendix A."]
[]
[]
[]
[]
[]
[]
["Purchasing Document(s): "]
[]
["Brand and Model number:"]
[]
["Facility Part Number: "]
[]
[null,"Inspection Method\nD – Document Verification (certificates)\nI – Inspection Verification (Marking)\nM – Measurement Verification Criteria"]
[]
["SELECT","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria","Certificate \nProvided\nY/N","Inspection\nPerfromed\nY/N","Pass\nFail\nP/F","Measurement \nEquipment\nID#"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material","Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,"D","Certified Mill Test Report"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"D","Material Specification and Grade"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"M","Thickness Readings"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"M","Radius (If Applicable)"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"I","Rolling Direction (If Applicable)",null,"`"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"I","Material Marking"]
["BOLTS","Bolts",null,"D","Material Specification"]
["BOLTS",null,null,"I","Marking"]
["BOLTS",null,null,"D","Thread Specification"]
["BOLTS",null,null,"M","Overall Length"]
["BOLTS",null,null,"M","Length of Threads"]
["BOLTS",null,null,"M","Length of Shoulder"]
["BOLTS",null,null,"M","Diameter"]
["BOLTS",null,null,"M","Head size across flats"]
["Socket Head Cap Screws","Socket Head Cap Screws",null,"D","Material Specification"]
["Socket Head Cap Screws",null,null,"I","Finish (plain, zinc, other)"]
["Socket Head Cap Screws",null,null,"I or D","Marking (if specified)"]
["Socket Head Cap Screws",null,null,"D","Thread Specification"]
["Socket Head Cap Screws",null,null,"M","Overall Length"]
["Socket Head Cap Screws",null,null,"M","Minimum Thread Length"]
["Socket Head Cap Screws",null,null,"M","Head Diameter"]
["Socket Head Cap Screws",null,null,"M","Screw Diameter"]
["Socket Head Cap Screws",null,null,"I","Head Type (plain, knurled)"]
["Socket Head Cap Screws",null,null,"M","Head Chamfer angle (30 or 45 degrees)"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Size"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Depth"]
["Eyebolts","Eyebolts",null,"D","Material Specification"]
["Eyebolts",null,null,"I","Marking"]
["Eyebolts",null,null,"D","Thread Specification"]
["Eyebolts",null,null,"M","Overall Length"]
["Eyebolts",null,null,"M","Length of Threads"]
["Eyebolts",null,null,"M","Length of Shoulder"]
["Eyebolts",null,null,"M","Diameter"]
["Eyebolts",null,null,"M","Nut length across flats and thickness"]
["Eyebolts",null,null,"M","Nut style square/hex"]
["Eyebolts",null,null,"M","Eyelet ID/OD"]
["Stud Bolts","Stud Bolts",null,"D","Material Specification"]
["Stud Bolts",null,null,"I","Marking"]
["Stud Bolts",null,null,"D","Thread Specification"]
["Stud Bolts",null,null,"M","Overall Length"]
["Stud Bolts",null,null,"M","Length of Threads"]
["Stud Bolts",null,null,"M","Length of Shoulder"]
["Stud Bolts",null,null,"D","Stud end chamfer and radius configuration"]
["Stud Bolts",null,null,"M","Diameter"]
["Nut","Nut",null,"D","Material Specification"]
["Nut",null,null,"I","Marking"]
["Nut",null,null,"D","Thread Specification"]
["Nut",null,null,"M","Length across flats"]
["Nut",null,null,"M","Thickness"]
["Nut",null,null,"I","Style (Square or Hex)"]
["Washer","Washer",null,"D","Material Specification"]
["Washer",null,null,"I","Marking"]
["Washer",null,null,"M","Inside Diameter"]
["Washer",null,null,"M","Outside Diameter"]
["Washer",null,null,"M","Thickness"]
["Washer",null,null,"M","Flatness"]
["Washer",null,null,"I","Style (Flat or Spring or Lock)"]
["Flanges","Flanges",null,"D","Material Specification"]
["Flanges",null,null,"M","Inside Diameter (if required)"]
["Flanges",null,null,"M","Outside Diameter"]
["Flanges",null,null,"M","Thickness"]
["Flanges",null,null,"D","Mounting Style (Flat Face, Raised, or Tongue and Groove)"]
["Flanges",null,null,"I","Machined Characteristics /Gasket Surface"]
["Fittings Plate with no nozzles","Fittings Plate with no nozzles",null,"D","AAR Device Approval (If Contractually Specified)"]
["Fittings Plate with no nozzles",null,null,"D","Material Specification"]
["Fittings Plate with no nozzles",null,null,"D","Thickness"]
["Fittings Plate with no nozzles",null,null,"D","Mounting Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with no nozzles",null,null,"M","Gauge tapped threads"]
["Fittings Plate with no nozzles",null,null,"D","Machined Characteristics / Gasket Surface /fitting holes/bolt holes"]
["Pipe Plugs","Pipe Plugs",null,"D","Material Specification"]
["Pipe Plugs",null,null,"D","Thread Specification gauge threads"]
["Pipe Plugs",null,null,"D","Diameter"]
["Bottom Outlet Valve Sump – No Opening","Bottom Outlet Valve Sump – No Opening",null,"D","Material Specification"]
["Bottom Outlet Valve Sump – No Opening",null,null,"I","Marking"]
["Bottom Outlet Valve Sump – No Opening",null,null,"D","Dimensional"]
["Bottom Outlet Valve Sump – No Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Bottom Outlet Valve Saddle – Drain Opening","Bottom Outlet Valve Saddle – Drain Opening",null,"D","AAR Device Approval (If Contractually Specified)"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"D","Material Specification"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Marking"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"D","Dimensional"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Spool","Spool",null,"D","AAR Device Approval (If Contractually Specified)"]
["Spool",null,null,"D","Material Specification"]
["Spool",null,null,"D","Length Overall"]
["Spool",null,null,"D","Flange Dimensions"]
["Spool",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Spool",null,null,"M","Pipe Dimensions"]
["Fittings Plate with Welded Nozzle(s)","Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval (If Contractually Specified)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Material Specification"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Inside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Outside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Thickness"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Nozzle Dimensions"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)"]
["Fittings Plate with Welded Nozzle(s)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Machined Characteristics / Gasket Surface /fitting holes/bolt holes/bolt pattern"]
["Fittings Plate with Welded Nozzle(s)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Weld Size and Type"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover","Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,"D","AAR Device Approval (If Contractually Specified)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Material Specification"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Nozzle Dimensions"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"I","Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Bolt Pattern"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"I","Weld Size and Type"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Hinge Position"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Bolt Slot Opening Dimensions"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Gasket Groove Dimensions (I.D., O.D., Finish,and Profile)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover"]
["Thermowell","Thermowell",null,"D","Material Specification"]
["Thermowell",null,null,"D","AAR Device Approval"]
["Thermowell",null,null,"D","Length Overall"]
["Thermowell",null,null,"D","Thread Specification"]
["Thermowell",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Hinged and Bolted Nozzle Assembly","Hinged and Bolted Nozzle Assembly",null,"D","Material Specification"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Length Overall"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Thickness"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Hinge Position"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Eyebolt Lug Position"]
["Flanged Nozzle","Flanged Nozzle",null,"D","Material Specification"]
["Flanged Nozzle",null,null,"D","Length Overall"]
["Flanged Nozzle",null,null,"D","Diameter"]
["Flanged Nozzle",null,null,"D","Thickness"]
["Flanged Nozzle",null,null,"I","Machined Characteristics / Gasket Surface /fitting holes/bolt holes/ bolt pattern"]
["Flanged Nozzle"]
["Flanged Nozzle",null,null,"I","Weld Size and Type (Forged or Cast)"]
["Eduction Pipe Assembly","Eduction Pipe Assembly",null,"D","Material Specification"]
["Eduction Pipe Assembly",null,null,"D","Length Overall"]
["Eduction Pipe Assembly",null,null,"D","Thread Specification (If Applicable)"]
["Eduction Pipe Assembly",null,null,"D","Diameter"]
["Eduction Pipe Assembly",null,null,"D","Thickness"]
["Eduction Pipe Assembly",null,null,"I","Machined Characteristics"]
["Eduction Pipe Assembly",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Manway Cover","Hinged and Bolted Manway Covers",null,"D","AAR Device Approval (If Contractually Specified)"]
["Hinged and Bolted Manway Cover",null,null,"D","Material Specification"]
["Hinged and Bolted Manway Cover",null,null,"D","Structural Integrity – Pressure Test"]
["Hinged and Bolted Manway Cover",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted Manway Cover",null,null,"D","Bolt Pattern"]
["Hinged and Bolted Manway Cover",null,null,"D","Hinge Position"]
["Hinged and Bolted Manway Cover",null,null,"D","Bolt Slot Opening Dimensions"]
["Hinged and Bolted Manway Cover",null,null,"D","Gasket Groove Dimensions"]
["Eduction Pipe Sump","Eduction Pipe Sump",null,"D","Material Specification"]
["Eduction Pipe Sump",null,null,"I","Marking (If Required)"]
["Eduction Pipe Sump",null,null,"D","Dimensions (O.D. and Depth)"]
["Eduction Pipe Sump",null,null,"D","Structural Integrity – Pressure Test"]
["Eduction Pipe Sump",null,null,"M","Thickness"]
["Loading/Unloading, and Sample Valves","Loading/Unloading, and Sample Valves",null,"D","AAR Device Approval"]
["Loading/Unloading, and Sample Valves",null,null,"D","Model"]
["Loading/Unloading, and Sample Valves",null,null,"D","Manufacturing Facility"]
["Loading/Unloading, and Sample Valves",null,null,"I","Connection – Flange Dimensions"]
["Loading/Unloading, and Sample Valves",null,null,"I","Connection – Thread Specification"]
["Loading/Unloading, and Sample Valves",null,null,"D","Body Length"]
["Loading/Unloading, and Sample Valves",null,null,"D","Body Diameter"]
["Loading/Unloading, and Sample Valves",null,null,"D","Port Opening Size"]
["Loading/Unloading, and Sample Valves",null,null,"D","Body Material"]
["Loading/Unloading, and Sample Valves",null,null,"I","Lining Material (If Applicable)"]
["Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Material"]
["Loading/Unloading, and Sample Valves",null,null,"D","OEM test certificate"]
["Vent, Vacuum Relief, and Pressure Relief Valves","Vent, Vacuum Relief, and Pressure Relief Valves",null,"D","AAR Device Approval"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Model"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Manufacturing Facility"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Flange Dimensions"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Thread Specification"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Length"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Body Diameter"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Body Material"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Lining Material (If Applicable)"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Material"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Start to Discharge Pressure"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Vapor Tight Pressure"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Flow Rated Capacity"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","OEM Test Certificate"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","AAR Certificate of Test"]
["Rupture Disks","Rupture Disks",null,"D","Model"]
["Rupture Disks",null,null,"D","Burst Rating"]
["Rupture Disks",null,null,"I","Structural Integrity"]
["Rupture Disks",null,null,"D","Certificate of Test (Per Lot)"]
["Spring Loaded Check Valves","Spring Loaded Check Valves",null,"D","AAR Device Approval"]
["Spring Loaded Check Valves",null,null,"D","Model"]
["Spring Loaded Check Valves",null,null,"D","Manufacturing Facility"]
["Spring Loaded Check Valves",null,null,"D","Connection – Flange Dimensions"]
["Spring Loaded Check Valves",null,null,"D","Connection – Thread Specification"]
["Spring Loaded Check Valves",null,null,"D","Flow Rated Capacity"]
["Spring Loaded Check Valves",null,null,"D","OEM test certificate"]
["Heat and Pressure Sensors","Heat and Pressure Sensors",null,"D","AAR Device Approval"]
["Heat and Pressure Sensors",null,null,"D","Model"]
["Heat and Pressure Sensors",null,null,"D","Manufacturing Facility"]
["Heat and Pressure Sensors",null,null,"D","Connection – Flange Dimensions"]
["Heat and Pressure Sensors",null,null,"D","Connection – Thread Specification"]
["Heat and Pressure Sensors",null,null,"D","OEM test certificate"]
["Gaskets and O-Rings","Gaskets and O-Rings",null,"D","Material Specification"]
["Gaskets and O-Rings",null,null,"I","Marking (if applicable)"]
["Gaskets and O-Rings",null,null,"D","Inside Diameter"]
["Gaskets and O-Rings",null,null,"D","Outside Diameter"]
["Gaskets and O-Rings",null,null,"D","Thickness"]
["A-No Entry"]
[]
[]
[]
[]
[null,"INPSECTOR NAME:",null,null,"SIGNATURE:",null,null,"DATE:"]

{"sheet":"INSP FORM V3","index":6,"n_rows":2,"n_cols":13,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"JULY 9TH 2020"]

{"sheet":"INSP FORM V2","index":7,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"ORIG INSP FORM","index":8,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}