{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["latest INSP FORM WITH DROP DOWN","MAIN LIST APP A","latest table 9","INSP FORM V4","INSP FORM V3","INSP FORM V2","ORIG INSP FORM"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"latest INSP FORM WITH DROP DOWN","index":0,"n_rows":234,"n_cols":9,"rows_kept":234,"cut":false,"hidden":false,"merged":[[77,1,87,1],[201,1,208,1],[201,2,208,2],[77,2,87,2],[88,1,93,1],[88,2,93,2],[94,1,96,1],[94,2,96,2],[177,2,189,2],[190,2,193,2],[194,2,200,2],[43,2,52,2],[53,2,58,2],[59,1,67,1],[59,2,67,2],[68,1,76,1],[68,2,76,2],[154,1,159,1],[142,2,147,2],[148,2,153,2],[154,2,159,2],[142,1,147,1],[148,1,153,1],[124,1,130,1],[131,1,135,1],[136,1,141,1],[124,2,130,2],[131,2,135,2],[136,2,141,2],[10,0,16,8],[23,1,23,8],[109,1,116,1],[117,1,123,1],[109,2,116,2],[117,2,123,2],[97,2,108,2],[97,1,108,1],[26,1,33,1],[34,1,38,1],[39,1,42,1],[43,1,52,1],[53,1,58,1],[26,2,33,2],[34,2,38,2],[39,2,42,2],[234,1,234,4],[160,1,165,1],[166,1,170,1],[171,1,176,1],[177,1,189,1],[160,2,165,2],[166,2,170,2],[171,2,176,2],[190,1,193,1],[194,1,200,1],[209,1,213,1],[214,1,229,1],[209,2,213,2],[214,2,229,2]]}
[]
[null,null,null,null,null,null,"Form",null,"RSI-100-05"]
[null,null,null,null,null,null,"Original Date"]
[null,null,null,null,"Incoming Material ",null,"Revision Level",null,"VER 9-21-20"]
[]
[null,null,null,null,"Inspection  Form",null,"Revision Date",null,"Original"]
[null,null,null,null,null,null,"Revised By"]
[null,null,null,null,null,null,"Approved By ",null,"J. Byrne"]
[]
[]
["The tank car facility receiving parts, materials, or components must ensure that the manufactures or distributor provides any requested certificates of conformance, compliance (measurement, testing or mill test reports) required by the purchasing documents that provides the objective evidence that the required inspection points noted in Appendix A of RSI-100 were in fact performed. Each facility is responsible to address the CTC characteristics/requirements identified in Appendix A."]
[]
[]
[]
[]
[]
[]
["Purchasing Document(s): "]
[]
["Brand and Model number:"]
[]
["Facility Part Number: "]
[]
[null,"Inspection Method\nD – Document Verification (certificates) , I – Inspection Verification (Marking),  M – Measurement Verification Criteria"]
[]
["SELECT","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria","Certificate \nProvided\nY/N","Inspection\nPerfromed\nY/N","Pass\nFail\nP/F","Measurement \nEquipment\nID#"]
["Bolts","Bolts",null,"D","Material Specification"]
["Bolts",null,null,"I","Marking"]
["Bolts",null,null,"D","Thread Specification"]
["Bolts",null,null,"M","Overall Length"]
["Bolts",null,null,"M","Length of Threads"]
["Bolts",null,null,"M","Length of Shoulder"]
["Bolts",null,null,"M","Diameter"]
["Bolts",null,null,"M","Head size across flats"]
["Bottom Outlet Valve Saddle – Drain Opening","Bottom Outlet Valve Saddle – Drain Opening",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"D","Material Specification"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Marking"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null," M","Dimensional"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Bottom Outlet Valve Sump – No Opening","Bottom Outlet Valve Sump – No Opening",null,"D ","Material Specification"]
["Bottom Outlet Valve Sump – No Opening",null,null,"I","Marking"]
["Bottom Outlet Valve Sump – No Opening",null,null," M","Dimensional"]
["Bottom Outlet Valve Sump – No Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Eyebolts","Eyebolts",null,"D","Material Specification"]
["Eyebolts",null,null,"I","Marking"]
["Eyebolts",null,null,"D","Thread Specification"]
["Eyebolts",null,null,"M","Overall Length"]
["Eyebolts",null,null,"M","Length of Threads"]
["Eyebolts",null,null,"M","Length of Shoulder"]
["Eyebolts",null,null,"M","Diameter"]
["Eyebolts",null,null,"M","Nut length across flats and thickness"]
["Eyebolts",null,null,"M","Nut style square/hex"]
["Eyebolts",null,null,"M","Eyelet ID/OD"]
["Fittings Plate with no nozzles","Fittings Plate with no nozzles",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Fittings Plate with no nozzles",null,null,"D","Material Specification"]
["Fittings Plate with no nozzles",null,null,"D","Thickness"]
["Fittings Plate with no nozzles",null,null,"D","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with no nozzles",null,null,"M","Gauge tapped threads "]
["Fittings Plate with no nozzles",null,null,"I &M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes"]
["Fittings Plate with Welded Nozzle(s)","Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D ","Material Specification"]
["Fittings Plate with Welded Nozzle(s)",null,null," M","Inside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null," M","Outside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null,"M","Thickness"]
["Fittings Plate with Welded Nozzle(s)",null,null,"M","Nozzle Dimensions"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Manway Covers (Cast)","Hinged and Bolted Manway Covers (Cast)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Hinged and Bolted Manway Covers (Cast)",null,null,"D","Material Specification"]
["Hinged and Bolted Manway Covers (Cast)",null,null,"D ","Structural Integrity – Pressure Test "]
["Hinged and Bolted Manway Covers (Cast)",null,null,"D","Casting Quality"]
["Hinged and Bolted Manway Covers (Cast)",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted Manway Covers (Cast)",null,null,"I","Bolt Pattern"]
["Hinged and Bolted Manway Covers (Cast)",null,null,"I","Hinge Position"]
["Hinged and Bolted Manway Covers (Cast)",null,null,"M","Bolt Slot Opening Dimensions"]
["Hinged and Bolted Manway Covers (Cast)",null,null,"M","Gasket Groove Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Material Specification"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Nozzle Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Bolt Pattern"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Hinge Position"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Bolt Slot Opening Dimensions"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," I","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)"]
["Nut","Nut",null,"D","Material Specification"]
["Nut",null,null,"I","Marking"]
["Nut",null,null,"D","Thread Specification"]
["Nut",null,null,"M","Length across flats"]
["Nut",null,null,"M","Thickness"]
["Nut",null,null,"I","Style (Square or Hex)"]
["Pipe Plugs","Pipe Plugs",null,"D","Material Specification"]
["Pipe Plugs",null,null,"D & M","Thread Specification "]
["Pipe Plugs",null,null,"M","Diameter"]
["Socket Head Cap Screws","Socket Head Cap Screws",null,"D","Material Specification"]
["Socket Head Cap Screws",null,null,"I","Finish (plain, zinc, other)"]
["Socket Head Cap Screws",null,null,"I ","Marking (if specified)"]
["Socket Head Cap Screws",null,null,"D","Thread Specification"]
["Socket Head Cap Screws",null,null,"M","Overall Length"]
["Socket Head Cap Screws",null,null,"M","Minimum Thread Length"]
["Socket Head Cap Screws",null,null,"M","Head Diameter"]
["Socket Head Cap Screws",null,null,"M","Screw Diameter"]
["Socket Head Cap Screws",null,null,"I","Head Type (plain, knurled)"]
["Socket Head Cap Screws",null,null,"M","Head Chamfer angle (30 or 45 degrees)"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Size"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Depth"]
["Stud Bolts","Stud Bolts",null,"D","Material Specification"]
["Stud Bolts",null,null,"I","Marking"]
["Stud Bolts",null,null,"D","Thread Specification"]
["Stud Bolts",null,null,"M","Overall Length"]
["Stud Bolts",null,null,"M","Length of Threads"]
["Stud Bolts",null,null,"M","Length of Shoulder"]
["Stud Bolts",null,null,"D","Stud end chamfer and radius configuration"]
["Stud Bolts",null,null,"M","Diameter"]
["Washer","Washer",null,"D","Material Specification"]
["Washer",null,null,"I","Marking"]
["Washer",null,null,"M","Inside Diameter"]
["Washer",null,null,"M","Outside Diameter"]
["Washer",null,null,"M","Thickness"]
["Washer",null,null,"M","Flatness"]
["Washer",null,null,"I","Style (Flat or Spring or Lock)"]
["Eduction Pipe Assembly","Eduction Pipe Assembly",null,"D","Material Specification"]
["Eduction Pipe Assembly",null,null,"     M","Length Overall"]
["Eduction Pipe Assembly",null,null,"D & M","Thread Specification (If Applicable)"]
["Eduction Pipe Assembly",null,null," M","Diameter"]
["Eduction Pipe Assembly",null,null,"M","Thickness"]
["Eduction Pipe Assembly",null,null,"I & M","Machined Characteristics"]
["Eduction Pipe Assembly",null,null,"I","Weld Size and Type"]
["Eduction Pipe Sump","Eduction Pipe Sump",null,"D","Material Specification"]
["Eduction Pipe Sump",null,null,"I","Marking (If Required)"]
["Eduction Pipe Sump",null,null,"M","Dimensions (O.D. and Depth)"]
["Eduction Pipe Sump",null,null,"D ","Structural Integrity – Pressure Test"]
["Eduction Pipe Sump",null,null,"M","Thickness"]
["Flanged Nozzle","Flanged Nozzle",null,"D","Material Specification"]
["Flanged Nozzle",null,null," M","Length Overall"]
["Flanged Nozzle",null,null,"M","Diameter"]
["Flanged Nozzle",null,null,"M","Thickness"]
["Flanged Nozzle",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern"]
["Flanged Nozzle",null,null,"I","Weld Size and Type (Forged or Cast)"]
["Flanges","Flanges",null,"D","Material Specification"]
["Flanges",null,null,"M","Inside Diameter (if required)"]
["Flanges",null,null,"M","Outside Diameter"]
["Flanges",null,null,"M","Thickness"]
["Flanges",null,null,"I","Sealing Style (Flat Face, Raised, or Tongue and Groove)"]
["Flanges",null,null,"I","Machined Characteristics /Gasket Surface"]
["Hinged and Bolted Nozzle Assembly","Hinged and Bolted Nozzle Assembly",null,"D","Material Specification"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Length Overall"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Thickness"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Hinge Position"]
["Hinged and Bolted Nozzle Assembly",null,null,"M","Eyebolt Lug Position"]
["Spool","Spool",null,"D","AAR Device Approval  (If Contractually Specified)"]
["Spool",null,null,"D","Material Specification"]
["Spool",null,null," M","Length Overall"]
["Spool",null,null,"M","Flange Dimensions"]
["Spool",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Spool",null,null,"M","Pipe Dimensions"]
["Tank Shell and Manway Nozzles ","Tank Shell and Manway Nozzles ",null,"D","Certified Mill Test Report"]
["Tank Shell and Manway Nozzles ",null,null,"D","Material Specification and Grade"]
["Tank Shell and Manway Nozzles ",null,null,"M","Thickness "]
["Tank Shell and Manway Nozzles ",null,null,"M","Radius (If Applicable)"]
["Tank Shell and Manway Nozzles ",null,null,"I","Rolling Direction (If Applicable)"]
["Tank Shell and Manway Nozzles ",null,null,"I","Material Marking"]
["Gaskets and O-Rings","Gaskets and O-Rings",null,"D","Material Specification"]
["Gaskets and O-Rings",null,null,"I","Marking (if applicable)"]
["Gaskets and O-Rings",null,null,"M","Inside Diameter"]
["Gaskets and O-Rings",null,null,"M","Outside Diameter"]
["Gaskets and O-Rings",null,null," M","Thickness"]
["Heat and Pressure Sensors","Heat and Pressure Sensors",null,"D","AAR Device Approval "]
["Heat and Pressure Sensors",null,null,"D","Model"]
["Heat and Pressure Sensors",null,null,"D","Manufacturing Facility"]
["Heat and Pressure Sensors",null,null,"M","Connection – Flange Dimensions"]
["Heat and Pressure Sensors",null,null,"D & M","Connection – Thread Specification"]
["Heat and Pressure Sensors",null,null,"D","OEM test certificate"]
["Loading/Unloading, and Sample Valves","Loading/Unloading, and Sample Valves",null,"D","AAR Device Approval "]
["Loading/Unloading, and Sample Valves",null,null,"D","Model"]
["Loading/Unloading, and Sample Valves",null,null,"D","Manufacturing Facility"]
["Loading/Unloading, and Sample Valves",null,null,"I","Connection – Flange Dimensions"]
["Loading/Unloading, and Sample Valves",null,null,"I","Connection – Thread Specification"]
["Loading/Unloading, and Sample Valves",null,null,"M","Body Length"]
["Loading/Unloading, and Sample Valves",null,null,"      M","Body Diameter"]
["Loading/Unloading, and Sample Valves",null,null,"D","Port Opening Size"]
["Loading/Unloading, and Sample Valves",null,null,"D","Body Material"]
["Loading/Unloading, and Sample Valves",null,null,"I","Lining Material (If Applicable)"]
["Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Material"]
["Loading/Unloading, and Sample Valves",null,null,"D","OEM test certificate"]
["Rupture Disks","Rupture Disks",null,"D","Model"]
["Rupture Disks",null,null,"D","Burst Rating"]
["Rupture Disks",null,null,"I","Structural Integrity"]
["Rupture Disks",null,null,"D","Certificate of Test (Per Lot)"]
["Spring Loaded Check Valves","Spring Loaded Check Valves",null,"D","AAR Device Approval "]
["Spring Loaded Check Valves",null,null,"D","Model"]
["Spring Loaded Check Valves",null,null,"D ","Manufacturing Facility"]
["Spring Loaded Check Valves",null,null,"M","Connection – Flange Dimensions"]
["Spring Loaded Check Valves",null,null,"D & M","Connection – Thread Specification"]
["Spring Loaded Check Valves",null,null,"D","Flow Rated Capacity"]
["Spring Loaded Check Valves",null,null,"D","OEM test certificate"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material","Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"D","Certified Mill Test Report"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"D","Material Specification and Grade"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Thickness"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Radius (If Applicable)"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Rolling Direction (If Applicable)"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Inside Diameter (If Applicable)"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Outside Diameter (If Applicable)"]
["Steel - Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Material Marking"]
["Thermowell","Thermowell",null,"D","Material Specification"]
["Thermowell",null,null,"D","AAR Device Approval "]
["Thermowell",null,null,"M","Length Overall"]
["Thermowell",null,null,"D & M","Thread Specification"]
["Thermowell",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Vent, Vacuum Relief, and Pressure Relief Valves","Vent, Vacuum Relief, and Pressure Relief Valves",null,"D","AAR Device Approval "]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Model"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Manufacturing Facility"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Flange Dimensions"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Thread Specification"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"M","Length"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"M","Body Diameter"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Body Material"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Lining Material (If Applicable)"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Material"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Start to Discharge Pressure"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Vapor Tight Pressure"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Flow Rated Capacity"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","OEM Test Certificate"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","AAR Certificate of Test"]
["A-No Entry"]
[]
[]
[null,"INPSECTOR NAME:",null,null,"   SIGNATURE:",null,null,"DATE:"]

{"sheet":"MAIN LIST APP A","index":1,"n_rows":207,"n_cols":7,"rows_kept":207,"cut":false,"hidden":true,"merged":[[136,0,142,0],[143,0,150,0],[151,0,155,0],[156,0,168,0],[133,2,134,2],[47,0,52,0],[60,0,66,0],[133,3,134,3],[133,4,134,4],[129,0,135,0],[133,1,134,1],[116,2,117,2],[116,3,117,3],[116,4,117,4],[104,0,117,0],[118,0,122,0],[123,0,128,0],[108,4,109,4],[114,2,115,2],[114,3,115,3],[114,4,115,4],[99,4,100,4],[67,0,74,0],[78,0,81,0],[82,0,86,0],[87,0,92,0],[93,0,103,0],[75,0,77,0],[99,2,100,2],[99,3,100,3],[101,2,102,2],[101,3,102,3],[101,4,102,4],[101,1,102,1],[0,0,0,4],[1,0,1,4],[3,0,8,0],[21,2,28,3],[39,2,46,3],[21,0,28,0],[29,0,38,0],[39,0,46,0],[185,0,188,0],[189,0,195,0],[196,0,201,0],[202,0,206,0],[9,2,20,3],[9,0,20,0],[99,1,100,1],[108,1,109,1],[114,1,115,1],[116,1,117,1],[169,0,184,0],[47,2,52,3],[53,2,59,3],[53,0,59,0],[108,2,109,2],[108,3,109,3]]}
["Tank Car Containment Parts and Materials - CTQ Inspection Criteria"]
["D – Document Verification (certificates); I – Inspection Verification (Marking); M – Measurement Verification Criteria",null,null,null,null,null,"JULY 9TH 2020"]
["Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material","Certified Mill Test Report","I","D","D"]
[null,"Material Specification and Grade","D","D","D"]
[null,"Thickness Readings","M","M","M"]
[null,"Radius (If Applicable)","M","M","M"]
[null,"Rolling Direction (If Applicable)","M","I","I"]
[null,"Material Marking","I","I","I"]
["Socket Head Cap Screws","Material Specification","Per ASME B18.18 &\nASTM F1470\n",null,"D"]
[null,"Finish (plain, zinc, other)",null,null,"I"]
[null,"Marking (if specified)",null,null,"I or D"]
[null,"Thread Specification",null,null,"D"]
[null,"Overall Length",null,null,"M"]
[null,"Minimum Thread Length",null,null,"M"]
[null,"Head Diameter",null,null,"M"]
[null,"Screw Diameter",null,null,"M"]
[null,"Head Type (plain, knurled)",null,null,"I"]
[null,"Head Chamfer angle (30 or 45 degrees)",null,null,"M"]
[null,"Nominal Hex Socket Size",null,null,"M"]
[null,"Nominal Hex Socket Depth",null,null,"M"]
["Bolts","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Thread Specification",null,null,"D"]
[null,"Overall Length",null,null,"M"]
[null,"Length of Threads",null,null,"M"]
[null,"Length of Shoulder",null,null,"M"]
[null,"Diameter",null,null,"M"]
[null,"Head size across flats",null,null,"M"]
["Eyebolts","Material Specification","D","D","D"]
[null,"Marking","I","I","I"]
[null,"Thread Specification","M","M","D"]
[null,"Overall Length","M","M","M"]
[null,"Length of Threads","M","M","M"]
[null,"Length of Shoulder","M","M","M"]
[null,"Diameter","M","M","M"]
[null,"Nut length across flats and thickness","M","M","M"]
[null,"Nut style square/hex","M","M","M"]
[null,"Eyelet ID/OD","M","M","M"]
["Stud Bolts","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Thread Specification",null,null,"D"]
[null,"Overall Length",null,null,"M"]
[null,"Length of Threads",null,null,"M"]
[null,"Length of Shoulder",null,null,"M"]
[null,"Stud end chamfer and radius configuration",null,null,"D"]
[null,"Diameter",null,null,"M"]
["Nut","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Thread Specification",null,null,"D"]
[null,"Length across flats",null,null,"M"]
[null,"Thickness",null,null,"M"]
[null,"Style (Square or Hex)",null,null,"I"]
["Washer","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D"]
[null,"Marking",null,null,"I"]
[null,"Inside Diameter",null,null,"M"]
[null,"Outside Diameter",null,null,"M"]
[null,"Thickness",null,null,"M"]
[null,"Flatness",null,null,"M"]
[null,"Style (Flat or Spring or Lock)",null,null,"I"]
["Flanges","Material Specification","D","D","D"]
[null,"Inside Diameter (if required)","M","M","M"]
[null,"Outside Diameter","M","M","M"]
[null,"Thickness","M","M","M"]
[null,"Mounting Style (Flat Face, Raised, or Tongue and"]
[null,"Groove)","M","M","D"]
[null,"Machined Characteristics /Gasket Surface","M","M","I"]
["Fittings Plate with no nozzles","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Thickness","M","M","D"]
[null,"Mounting Style (Opening Style, Flat Face, Raised,"]
[null,"or Tongue and Groove)","M","M","D"]
[null,"Gauge tapped threads","M","M","M"]
[null,"Machined Characteristics / Gasket Surface /","M","M","D"]
[null,"fitting holes/bolt holes"]
["Pipe Plugs","Material Specification","D","D","D"]
[null,"Thread Specification gauge threads","M","M","D"]
[null,"Diameter","M","M","D"]
["Bottom Outlet Valve Sump – No Opening","Material Specification","D","D","D"]
[null,"Marking","I","I","I"]
[null,"Dimensional","M","M","D"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Bottom Outlet Valve Saddle – Drain Opening","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Marking","I","I","I"]
[null,"Dimensional","M","M","D"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Spool","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Flange Dimensions","M","M","D"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I"]
[null,"Pipe Dimensions","M","M","M"]
["Fittings Plate with Welded Nozzle(s)","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Inside Diameter","M","M","D"]
[null,"Outside Diameter","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Nozzle Dimensions","M","M","D"]
[null,"Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)","I","I","I"]
[]
[null,"Machined Characteristics / Gasket Surface /fitting holes/bolt holes/bolt pattern","M","M","I"]
[]
[null,"Weld Size and Type","I","I","I"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Nozzle Dimensions","M","M","D"]
[null,"Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)","I","I","I"]
[]
[null,"Bolt Pattern","M","M","D"]
[null,"Weld Size and Type","I","I","I"]
[null,"Hinge Position","M","M","D"]
[null,"Bolt Slot Opening Dimensions","M","M","D"]
[null,"Gasket Groove Dimensions (I.D., O.D., Finish,and Profile)","M","M","D"]
[]
[null,"Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)","M","M","D"]
[]
["Thermowell","Material Specification","D","D","D"]
[null,"AAR Device Approval","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Thread Specification","M","M","D"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I"]
["Hinged and Bolted Nozzle Assembly","Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Weld Size and Type","I","I","I"]
[null,"Hinge Position","M","M","D"]
[null,"Eyebolt Lug Position","M","M","D"]
["Flanged Nozzle","Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Diameter","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Machined Characteristics / Gasket Surface /fitting holes/bolt holes/ bolt pattern","M","M","I"]
[]
[null,"Weld Size and Type (Forged or Cast)","I","I","I"]
["Eduction Pipe Assembly","Material Specification","D","D","D"]
[null,"Length Overall","M","M","D"]
[null,"Thread Specification (If Applicable)","M","M","D"]
[null,"Diameter","M","M","D"]
[null,"Thickness","M","M","D"]
[null,"Machined Characteristics","M","M","I"]
[null,"Weld Size and Type","I","I","I"]
["Hinged and Bolted Manway Covers","AAR Device Approval (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D"]
[null,"Structural Integrity – Pressure Test","M","M","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Bolt Pattern","M","M","D"]
[null,"Hinge Position","M","M","D"]
[null,"Bolt Slot Opening Dimensions","M","M","D"]
[null,"Gasket Groove Dimensions","M","M","D"]
["Eduction Pipe Sump","Material Specification","D","D","D"]
[null,"Marking (If Required)","I","I","I"]
[null,"Dimensions (O.D. and Depth)","M","M","D"]
[null,"Structural Integrity – Pressure Test","M","M","D"]
[null,"Thickness","M","M","M"]
["Loading/Unloading, and Sample Valves","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","I"]
[null,"Connection – Thread Specification","M","D","I"]
[null,"Body Length","M","D","D"]
[null,"Body Diameter","M","D","D"]
[null,"Port Opening Size","M","D","D"]
[null,"Body Material","D","D","D"]
[null,"Lining Material (If Applicable)","D","D","I"]
[null,"Seal/O-Ring Dimensions","M","D","D"]
[null,"Seal/O-Ring Material","D","D","D"]
[null,"OEM test certificate","D","D","D"]
["Vent, Vacuum Relief, and Pressure Relief Valves","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","I"]
[null,"Connection – Thread Specification","M","D","I"]
[null,"Length","M","D","D"]
[null,"Body Diameter","M","D","D"]
[null,"Body Material","D","D","D"]
[null,"Lining Material (If Applicable)","D","D","I"]
[null,"Seal/O-Ring Dimensions","M","D","D"]
[null,"Seal/O-Ring Material","D","D","D"]
[null,"Start to Discharge Pressure","D","D","D"]
[null,"Vapor Tight Pressure","D","D","D"]
[null,"Flow Rated Capacity","D","D","D"]
[null,"OEM Test Certificate","D","D","D"]
[null,"AAR Certificate of Test","D","D","D"]
["Rupture Disks","Model","I","D","D"]
[null,"Burst Rating","D","D","D"]
[null,"Structural Integrity","M","M","I"]
[null,"Certificate of Test (Per Lot)","D","D","D"]
["Spring Loaded Check Valves","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","D"]
[null,"Connection – Thread Specification","M","D","D"]
[null,"Flow Rated Capacity","D","D","D"]
[null,"OEM test certificate","D","D","D"]
["Heat and Pressure Sensors","AAR Device Approval","D","D","D"]
[null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","D"]
[null,"Connection – Thread Specification","M","D","D"]
[null,"OEM test certificate","D","D","D"]
["Gaskets and O-Rings","Material Specification","D","D","D"]
[null,"Marking (if applicable)","D","D","I"]
[null,"Inside Diameter","M","M","D"]
[null,"Outside Diameter","M","M","D"]
[null,"Thickness","M","M","D"]

{"sheet":"latest table 9","index":2,"n_rows":219,"n_cols":19,"rows_kept":219,"cut":false,"hidden":true,"merged":[[202,8,209,8],[170,0,173,0],[170,8,173,8],[174,8,180,8],[181,0,185,0],[181,8,185,8],[186,0,201,0],[186,8,201,8],[128,8,133,8],[134,8,139,8],[140,8,145,8],[146,8,150,8],[151,8,156,8],[157,0,169,0],[157,8,169,8],[128,0,133,0],[134,0,139,0],[174,0,180,0],[116,8,121,8],[122,0,127,0],[122,8,127,8],[71,8,76,8],[77,0,88,0],[77,8,88,8],[89,0,96,0],[89,8,96,8],[97,0,103,0],[97,8,103,8],[61,0,70,0],[61,8,70,8],[111,0,115,0],[6,8,10,8],[11,8,14,8],[15,0,20,0],[15,8,20,8],[21,0,29,0],[21,8,29,8],[30,0,38,0],[30,8,38,8],[53,0,60,0],[71,0,76,0],[60,2,60,3],[50,0,52,0],[58,2,58,3],[104,0,110,0],[104,8,110,8],[111,8,115,8],[0,0,0,4],[0,7,0,10],[3,14,3,18],[2,14,2,18],[1,14,1,18],[2,7,3,10],[165,14,165,18],[166,14,166,18],[168,14,173,14],[104,16,104,17],[105,16,105,17],[106,16,106,17],[95,16,95,17],[96,16,96,17],[97,16,97,17],[98,16,98,17],[99,16,99,17],[100,16,100,17],[89,16,89,17],[90,16,90,17],[91,16,91,17],[92,16,92,17],[93,16,93,17],[94,16,94,17],[191,14,197,14],[6,14,10,14],[4,14,4,18],[154,14,154,18],[155,14,155,18],[156,14,156,18],[158,14,162,14],[163,14,163,18],[164,14,164,18],[139,15,140,15],[139,16,140,16],[139,17,140,17],[139,18,140,18],[147,14,152,14],[153,14,153,18],[107,16,107,17],[108,16,108,17],[109,14,109,18],[110,14,110,18],[111,14,111,18],[112,14,112,18],[101,16,101,17],[102,16,102,17],[103,16,103,17],[83,16,83,17],[84,16,84,17],[85,16,85,17],[86,16,86,17],[87,16,87,17],[88,16,88,17],[77,16,77,17],[78,16,78,17],[79,16,79,17],[80,16,80,17],[81,16,81,17],[82,16,82,17],[63,16,63,17],[64,16,64,17],[65,16,65,17],[64,15,65,15],[64,18,65,18],[76,16,76,17],[58,16,58,17],[59,16,59,17],[60,16,60,17],[61,16,61,17],[62,16,62,17],[140,0,145,0],[146,0,150,0],[151,0,156,0],[77,2,88,3],[89,2,96,3],[97,2,103,3],[71,2,71,3],[72,2,72,3],[73,2,73,3],[74,2,74,3],[75,2,75,3],[76,2,76,3],[116,0,121,0],[1,0,1,4],[2,0,2,4],[3,0,3,4],[4,0,4,4],[6,0,10,0],[11,0,14,0],[11,14,14,14],[50,14,52,14],[53,14,53,18],[53,2,53,3],[39,0,49,0],[39,8,49,8],[50,8,52,8],[53,8,60,8],[54,14,54,18],[55,14,55,18],[56,14,56,18],[54,2,54,3],[55,2,55,3],[56,2,56,3],[57,2,57,3],[59,2,59,3]]}
["COPY & PASTER NEW TABEL 9 HERE",null,null,null,null,null,null,"ADJUST , EDIT THEN COPY AND PASTE \nTHIS TO FORMTAB"]
["CLOSURES - CTQ INSPECTION CRITERIA",null,null,null,null,null,null,null,null,null,null,null,null,null,"CLOSURES - CTQ INSPECTION CRITERIA"]
["D – Document Verification (certificates); I – Inspection Verification (Marking); and ",null,null,null,null,null,null,null,null,null,null,null,null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
["M – Measurement Verification Criteria",null,null,null,null,null,null,null,null,null,null,null,null,null,"M – Measurement Verification Criteria"]
[]
["Item","Inspection Criteria","Manufacturer","Distributor","Facility",">>>>>>",null,"seelct","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
["Bottom Outlet Valve Saddle – Drain Opening","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Bottom Outlet Valve Saddle – Drain Opening","Bottom Outlet Valve Saddle – Drain Opening",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,"Bottom Outlet Valve Saddle – Drain Opening","AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null,"D","Material Specification",null,null,null,"Material Specification","D","D","D"]
[null,"Marking","I","I","I",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Marking",null,null,null,"Marking","I","I","I"]
[null,"Dimensional","M","M"," M",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null," M","Dimensional",null,null,null,"Dimensional","M","M"," M"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I",null,null,"Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)",null,null,null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Bottom Outlet Valve Sump – No Opening","Material Specification","D","D","D ",null,null,"Bottom Outlet Valve Sump – No Opening","Bottom Outlet Valve Sump – No Opening",null,"D ","Material Specification",null,null,"Bottom Outlet Valve Sump – No Opening","Material Specification","D","D","D "]
[null,"Marking","I","I","I",null,null,"Bottom Outlet Valve Sump – No Opening",null,null,"I","Marking",null,null,null,"Marking","I","I","I"]
[null,"Dimensional","M","M"," M",null,null,"Bottom Outlet Valve Sump – No Opening",null,null," M","Dimensional",null,null,null,"Dimensional","M","M"," M"]
[null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I",null,null,"Bottom Outlet Valve Sump – No Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)",null,null,null,"Structural Integrity (Cracks or Excessive Porosity)","I","I","I"]
["Fittings Plate with no nozzles","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Fittings Plate with no nozzles","Fittings Plate with no nozzles",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Fittings Plate with no nozzles",null,null,"D","Material Specification",null,null,"Fittings Plate with no nozzles","Material Specification","D","D","D"]
[null,"Thickness","M","M","D",null,null,"Fittings Plate with no nozzles",null,null,"D","Thickness",null,null,null,"Thickness","M","M","D"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","M","M","D",null,null,"Fittings Plate with no nozzles",null,null,"D","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)",null,null,null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","M","M","D"]
[null,"Gauge tapped threads ","M","M","M",null,null,"Fittings Plate with no nozzles",null,null,"M","Gauge tapped threads ",null,null,null,"Gauge tapped threads ","M","M","M"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes","M","M","I &M",null,null,"Fittings Plate with no nozzles",null,null,"I &M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes",null,null,null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes","M","M","I &M"]
["Fittings Plate with Welded Nozzle(s)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Fittings Plate with Welded Nozzle(s)","Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D ",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"D ","Material Specification",null,null,"Fittings Plate with Welded Nozzle(s)","Material Specification","D","D","D "]
[null,"Inside Diameter","M","M"," M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null," M","Inside Diameter",null,null,null,"Inside Diameter","M","M"," M"]
[null,"Outside Diameter","M","M"," M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null," M","Outside Diameter",null,null,null,"Outside Diameter","M","M"," M"]
[null,"Thickness","M","M","M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"M","Thickness",null,null,null,"Thickness","M","M","M"]
[null,"Nozzle Dimensions","M","M","M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"M","Nozzle Dimensions",null,null,null,"Nozzle Dimensions","M","M","M"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)",null,null,null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern","M","M","I & M",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern",null,null,null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/bolt pattern","M","M","I & M"]
[null,"Weld Size and Type","I","I","I",null,null,"Fittings Plate with Welded Nozzle(s)",null,null,"I","Weld Size and Type",null,null,null,"Weld Size and Type","I","I","I"]
["Hinged and Bolted Manway Covers (Cast)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Hinged and Bolted Manway Covers (Cast)","Hinged and Bolted Manway Covers (Cast)",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"D","Material Specification",null,null,"Hinged and Bolted Manway Covers","Material Specification","D","D","D"]
[null,"Structural Integrity – Pressure Test ","M","M","D ",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"D ","Structural Integrity – Pressure Test ",null,null,"(Cast)","Structural Integrity – Pressure Test ","M","M","D "]
[null,"Casting Quality","I","D","D",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"D","Casting Quality",null,null,null,"Casting Quality","I","D","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"I","Thickness (Dished, Flanged, or Grooved)",null,null,null,"Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Bolt Pattern","M","M","I",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"I","Bolt Pattern",null,null,null,"Bolt Pattern","M","M","I"]
[null,"Hinge Position","M","M","I",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"I","Hinge Position",null,null,null,"Hinge Position","M","M","I"]
[null,"Bolt Slot Opening Dimensions","M","M","M",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"M","Bolt Slot Opening Dimensions",null,null,null,"Bolt Slot Opening Dimensions","M","M","M"]
[null,"Gasket Groove Dimensions","M","M","M",null,null,"Hinged and Bolted Manway Covers (Cast)",null,null,"M","Gasket Groove Dimensions",null,null,null,"Gasket Groove Dimensions","M","M","M"]
["Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)","Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Material Specification",null,null,null,"Material Specification","D","D","D"]
[null,"Thickness (Dished, Flanged, or Grooved)","M","M","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Thickness (Dished, Flanged, or Grooved)",null,null,"Hinged and Bolted Manway or Fill Hole Cover ","Thickness (Dished, Flanged, or Grooved)","M","M","I"]
[null,"Nozzle Dimensions","M","M"," M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Nozzle Dimensions",null,null,"(Fabricated)","Nozzle Dimensions","M","M"," M"]
[null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)",null,null,null,"Sealing Style (Opening Style, Flat Face, Raised, or Tongue and Groove)","I","I","I"]
[null,"Bolt Pattern","M","M","D",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"D","Bolt Pattern",null,null,null,"Bolt Pattern","M","M","D"]
[null,"Weld Size and Type","I","I","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Weld Size and Type",null,null,null,"Weld Size and Type","I","I","I"]
[null,"Hinge Position","M","M","I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null,"I","Hinge Position",null,null,null,"Hinge Position","M","M","I"]
[null,"Bolt Slot Opening Dimensions","M","M"," M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Bolt Slot Opening Dimensions",null,null,null,"Bolt Slot Opening Dimensions","M","M"," M"]
[null,"Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)","M","M"," M",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," M","Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)",null,null,null,"Gasket Groove Dimensions (I.D., O.D., Finish, and Profile)","M","M"," M"]
[null,"Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)","M","M"," I",null,null,"Hinged and Bolted Manway or Fill Hole Cover (Fabricated)",null,null," I","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)",null,null,null,"Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)","M","M"," I"]
["Pipe Plugs","Material Specification","D","D","D",null,null,"Pipe Plugs","Pipe Plugs",null,"D","Material Specification",null,null,"Pipe Plugs","Material Specification","D","D","D"]
[null,"Thread Specification ","M","M","D & M",null,null,"Pipe Plugs",null,null,"D & M","Thread Specification ",null,null,null,"Thread Specification ","M","M","D & M"]
[null,"Diameter","M","M","M",null,null,"Pipe Plugs",null,null,"M","Diameter",null,null,null,"Diameter","M","M","M"]
["Bolts","Material Specification",null,null,"D",null,null,"Bolts","Bolts",null,"D","Material Specification",null,null,"FASTENERS - CTQ INSPECTION CRITERIA"]
[null,"Marking","Per ASME B18.18 &",null,"I",null,null,"Bolts",null,null,"I","Marking",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
[null,"Thread Specification","ASTM F1470",null,"D",null,null,"Bolts",null,null,"D","Thread Specification",null,null,"M – Measurement Verification Criteria"]
[null,"Overall Length",null,null,"M",null,null,"Bolts",null,null,"M","Overall Length"]
[null,"Length of Threads",null,null,"M",null,null,"Bolts",null,null,"M","Length of Threads",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Length of Shoulder",null,null,"M",null,null,"Bolts",null,null,"M","Length of Shoulder",null,null,null,"Material Specification",null,null,"D"]
[null,"Diameter",null,null,"M",null,null,"Bolts",null,null,"M","Diameter",null,null,null,"Marking","Per ASME B18.18 &",null,"I"]
[null,"Head size across flats",null,null,"M",null,null,"Bolts",null,null,"M","Head size across flats",null,null,"Bolts","Thread Specification","ASTM F1470",null,"D"]
["Eyebolts","Material Specification","D","D","D",null,null,"Eyebolts","Eyebolts",null,"D","Material Specification",null,null,null,"Length of Threads",null,null,"M"]
[null,"Marking","I","I","I",null,null,"Eyebolts",null,null,"I","Marking",null,null,null,"Length of Shoulder",null,null,"M"]
[null,"Thread Specification","M","M","D",null,null,"Eyebolts",null,null,"D","Thread Specification",null,null,null,"Diameter",null,null,"M"]
[null,"Overall Length","M","M","M",null,null,"Eyebolts",null,null,"M","Overall Length",null,null,null,"Head size across flats",null,null,"M"]
[null,"Length of Threads","M","M","M",null,null,"Eyebolts",null,null,"M","Length of Threads"]
[null,"Length of Shoulder","M","M","M",null,null,"Eyebolts",null,null,"M","Length of Shoulder",null,null,null,"Material Specification","D","D","D"]
[null,"Diameter","M","M","M",null,null,"Eyebolts",null,null,"M","Diameter",null,null,null,"Marking","I","I","I"]
[null,"Nut length across flats and thickness","M","M","M",null,null,"Eyebolts",null,null,"M","Nut length across flats and thickness",null,null,"Eyebolts","Thread Specification","M","M","D"]
[null,"Nut style square/hex","M","M","M",null,null,"Eyebolts",null,null,"M","Nut style square/hex",null,null,null,"Overall Length","M","M","M"]
[null,"Eyelet ID/OD","M","M","M",null,null,"Eyebolts",null,null,"M","Eyelet ID/OD",null,null,null,"Length of Threads","M","M","M"]
["Nut","Material Specification","Per ASME B18.18 &",null,"D",null,null,"Nut","Nut",null,"D","Material Specification",null,null,null,"Length of Shoulder","M","M","M"]
[null,"Marking","ASTM F1470",null,"I",null,null,"Nut",null,null,"I","Marking",null,null,null,"Diameter","M","M","M"]
[null,"Thread Specification",null,null,"D",null,null,"Nut",null,null,"D","Thread Specification",null,null,null,"Nut length across flats and thickness","M","M","M"]
[null,"Length across flats",null,null,"M",null,null,"Nut",null,null,"M","Length across flats",null,null,null,"Nut style square/hex","M","M","M"]
[null,"Thickness",null,null,"M",null,null,"Nut",null,null,"M","Thickness",null,null,null,"Eyelet ID/OD","M","M","M"]
[null,"Style (Square or Hex)",null,null,"I",null,null,"Nut",null,null,"I","Style (Square or Hex)",null,null,null,"Material Specification","Per ASME B18.18 &",null,"D"]
["Socket Head Cap Screws","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D",null,null,"Socket Head Cap Screws","Socket Head Cap Screws",null,"D","Material Specification",null,null,"Nut","Marking","ASTM F1470",null,"I"]
[null,"Finish (plain, zinc, other)",null,null,"I",null,null,"Socket Head Cap Screws",null,null,"I","Finish (plain, zinc, other)",null,null,null,"Thread Specification",null,null,"D"]
[null,"Marking (if specified)",null,null,"I ",null,null,"Socket Head Cap Screws",null,null,"I ","Marking (if specified)",null,null,null,"Length across flats",null,null,"M"]
[null,"Thread Specification",null,null,"D",null,null,"Socket Head Cap Screws",null,null,"D","Thread Specification",null,null,null,"Thickness",null,null,"M"]
[null,"Overall Length",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Overall Length",null,null,null,"Style (Square or Hex)",null,null,"I"]
[null,"Minimum Thread Length",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Minimum Thread Length",null,null,null,"Material Specification",null,null,"D"]
[null,"Head Diameter",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Head Diameter",null,null,null,"Finish (plain, zinc, other)","Per ASME B18.18 &",null,"I"]
[null,"Screw Diameter",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Screw Diameter",null,null,"Socket Head Cap Screws","Marking (if specified)","ASTM F1470",null,"I "]
[null,"Head Type (plain, knurled)",null,null,"I",null,null,"Socket Head Cap Screws",null,null,"I","Head Type (plain, knurled)",null,null,null,"Thread Specification",null,null,"D"]
[null,"Head Chamfer angle (30 or 45 degrees)",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Head Chamfer angle (30 or 45 degrees)",null,null,null,"Overall Length",null,null,"M"]
[null,"Nominal Hex Socket Size",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Size",null,null,null,"Minimum Thread Length",null,null,"M"]
[null,"Nominal Hex Socket Depth",null,null,"M",null,null,"Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Depth",null,null,null,"Head Diameter",null,null,"M"]
["Stud Bolts","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D",null,null,"Stud Bolts","Stud Bolts",null,"D","Material Specification",null,null,null,"Screw Diameter",null,null,"M"]
[null,"Marking",null,null,"I",null,null,"Stud Bolts",null,null,"I","Marking",null,null,null,"Head Type (plain, knurled)",null,null,"I"]
[null,"Thread Specification",null,null,"D",null,null,"Stud Bolts",null,null,"D","Thread Specification",null,null,null,"Head Chamfer angle (30 or 45 degrees)",null,null,"M"]
[null,"Overall Length",null,null,"M",null,null,"Stud Bolts",null,null,"M","Overall Length",null,null,null,"Nominal Hex Socket Size",null,null,"M"]
[null,"Length of Threads",null,null,"M",null,null,"Stud Bolts",null,null,"M","Length of Threads",null,null,null,"Nominal Hex Socket Depth",null,null,"M"]
[null,"Length of Shoulder",null,null,"M",null,null,"Stud Bolts",null,null,"M","Length of Shoulder",null,null,null,"Material Specification",null,null,"D"]
[null,"Stud end chamfer and radius configuration",null,null,"D",null,null,"Stud Bolts",null,null,"D","Stud end chamfer and radius configuration",null,null,"Stud Bolts","Marking","Per ASME B18.18 &",null,"I"]
[null,"Diameter",null,null,"M",null,null,"Stud Bolts",null,null,"M","Diameter",null,null,null,"Thread Specification","ASTM F1470",null,"D"]
["Washer","Material Specification","Per ASME B18.18 & ASTM F1470",null,"D",null,null,"Washer","Washer",null,"D","Material Specification",null,null,null,"Overall Length",null,null,"M"]
[null,"Marking",null,null,"I",null,null,"Washer",null,null,"I","Marking",null,null,null,"Length of Threads",null,null,"M"]
[null,"Inside Diameter",null,null,"M",null,null,"Washer",null,null,"M","Inside Diameter",null,null,null,"Length of Shoulder",null,null,"M"]
[null,"Outside Diameter",null,null,"M",null,null,"Washer",null,null,"M","Outside Diameter",null,null,null,"Stud end chamfer and radius configuration",null,null,"D"]
[null,"Thickness",null,null,"M",null,null,"Washer",null,null,"M","Thickness",null,null,null,"Diameter",null,null,"M"]
[null,"Flatness",null,null,"M",null,null,"Washer",null,null,"M","Flatness",null,null,null,"Material Specification","Per ASME B18.18 &",null,"D"]
[null,"Style (Flat or Spring or Lock)",null,null,"I",null,null,"Washer",null,null,"I","Style (Flat or Spring or Lock)",null,null,"Washer","Marking","ASTM F1470",null,"I"]
["Eduction Pipe Assembly","Material Specification","D","D","D",null,null,"Eduction Pipe Assembly","Eduction Pipe Assembly",null,"D","Material Specification",null,null,null,"Inside Diameter",null,null,"M"]
[null,"Length Overall","M","M","     M",null,null,"Eduction Pipe Assembly",null,null,"     M","Length Overall",null,null,null,"Outside Diameter",null,null,"M"]
[null,"Thread Specification (If Applicable)","M","M","D & M",null,null,"Eduction Pipe Assembly",null,null,"D & M","Thread Specification (If Applicable)",null,null,null,"Thickness",null,null,"M"]
[null,"Diameter","M","M"," M",null,null,"Eduction Pipe Assembly",null,null," M","Diameter",null,null,null,"Flatness",null,null,"M"]
[null,"Thickness","M","M","M",null,null,"Eduction Pipe Assembly",null,null,"M","Thickness",null,null,null,"Style (Flat or Spring or Lock)",null,null,"I"]
[null,"Machined Characteristics","M","M","I & M",null,null,"Eduction Pipe Assembly",null,null,"I & M","Machined Characteristics",null,null,"PRESSURE CONTAINING TANK CAR TANK COMPONENTS - CTQ INSPECTION CRITERIA"]
[null,"Weld Size and Type","I","I","I",null,null,"Eduction Pipe Assembly",null,null,"I","Weld Size and Type",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
["Eduction Pipe Sump","Material Specification","D","D","D",null,null,"Eduction Pipe Sump","Eduction Pipe Sump",null,"D","Material Specification",null,null,"M – Measurement Verification Criteria"]
[null,"Marking (If Required)","I","I","I",null,null,"Eduction Pipe Sump",null,null,"I","Marking (If Required)"]
[null,"Dimensions (O.D. and Depth)","M","M","M",null,null,"Eduction Pipe Sump",null,null,"M","Dimensions (O.D. and Depth)",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Structural Integrity – Pressure Test","M","M","D ",null,null,"Eduction Pipe Sump",null,null,"D ","Structural Integrity – Pressure Test",null,null,null,"Diameter","M","M"," M"]
[null,"Thickness","M","M","M",null,null,"Eduction Pipe Sump",null,null,"M","Thickness",null,null,null,"Thickness","M","M","M"]
["Flanged Nozzle","Material Specification","D","D","D",null,null,"Flanged Nozzle","Flanged Nozzle",null,"D","Material Specification",null,null,null,"Machined Characteristics","M","M","I & M"]
[null,"Length Overall","M","M"," M",null,null,"Flanged Nozzle",null,null," M","Length Overall",null,null,null,"Weld Size and Type","I","I","I"]
[null,"Diameter","M","M","M",null,null,"Flanged Nozzle",null,null,"M","Diameter",null,null,null,"Material Specification","D","D","D"]
[null,"Thickness","M","M","M",null,null,"Flanged Nozzle",null,null,"M","Thickness",null,null,"Eduction Pipe Sump","Marking (If Required)","I","I","I"]
[null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern","M","M","I & M",null,null,"Flanged Nozzle",null,null,"I & M","Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern",null,null,null,"Dimensions (O.D. and Depth)","M","M","M"]
[null,"Weld Size and Type (Forged or Cast)","I","I","I",null,null,"Flanged Nozzle",null,null,"I","Weld Size and Type (Forged or Cast)",null,null,null,"Structural Integrity – Pressure Test","M","M","D "]
["Flanges","Material Specification","D","D","D",null,null,"Flanges","Flanges",null,"D","Material Specification",null,null,null,"Thickness","M","M","M"]
[null,"Inside Diameter (if required)","M","M","M",null,null,"Flanges",null,null,"M","Inside Diameter (if required)",null,null,null,"Material Specification","D","D","D"]
[null,"Outside Diameter","M","M","M",null,null,"Flanges",null,null,"M","Outside Diameter",null,null,"Flanged Nozzle","Length Overall","M","M"," M"]
[null,"Thickness","M","M","M",null,null,"Flanges",null,null,"M","Thickness",null,null,null,"Diameter","M","M","M"]
[null,"Sealing Style (Flat Face, Raised, or Tongue and Groove)","M","M","I",null,null,"Flanges",null,null,"I","Sealing Style (Flat Face, Raised, or Tongue and Groove)",null,null,null,"Thickness","M","M","M"]
[null,"Machined Characteristics /Gasket Surface","M","M","I",null,null,"Flanges",null,null,"I","Machined Characteristics /Gasket Surface",null,null,null,"Machined Characteristics / Gasket Surface / fitting holes/bolt holes/ bolt pattern","M","M","I & M"]
["Hinged and Bolted Nozzle Assembly","Material Specification","D","D","D",null,null,"Hinged and Bolted Nozzle Assembly","Hinged and Bolted Nozzle Assembly",null,"D","Material Specification",null,null,null,"Weld Size and Type (Forged or Cast)","I","I","I"]
[null,"Length Overall","M","M","M",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"M","Length Overall",null,null,null,"Material Specification","D","D","D"]
[null,"Thickness","M","M","M",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"M","Thickness",null,null,"Flanges","Inside Diameter (if required)","M","M","M"]
[null,"Weld Size and Type","I","I","I",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"I","Weld Size and Type",null,null,null,"Outside Diameter","M","M","M"]
[null,"Hinge Position","M","M","I",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"I","Hinge Position",null,null,null,"Thickness","M","M","M"]
[null,"Eyebolt Lug Position","M","M","M",null,null,"Hinged and Bolted Nozzle Assembly",null,null,"M","Eyebolt Lug Position",null,null,null,"Sealing Style (Flat Face, Raised, or Tongue and Groove)","M","M","I"]
["Spool","AAR Device Approval  (If Contractually Specified)","D","D","D",null,null,"Spool","Spool",null,"D","AAR Device Approval  (If Contractually Specified)",null,null,null,"Material Specification","D","D","D"]
[null,"Material Specification","D","D","D",null,null,"Spool",null,null,"D","Material Specification",null,null,"Hinged and Bolted Nozzle Assembly","Length Overall","M","M","M"]
[null,"Length Overall","M","M"," M",null,null,"Spool",null,null," M","Length Overall",null,null,null,"Thickness","M","M","M"]
[null,"Flange Dimensions","M","M","M",null,null,"Spool",null,null,"M","Flange Dimensions",null,null,null,"Weld Size and Type","I","I","I"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I",null,null,"Spool",null,null,"I","Mounting Style (Bolted or Threaded)",null,null,null,"Hinge Position","M","M","I"]
[null,"Pipe Dimensions","M","M","M",null,null,"Spool",null,null,"M","Pipe Dimensions",null,null,null,"Eyebolt Lug Position","M","M","M"]
["Tank Shell and Manway Nozzles ","Certified Mill Test Report","I","D","D",null,null,"Tank Shell and Manway Nozzles ","Tank Shell and Manway Nozzles ",null,"D","Certified Mill Test Report"]
[null,"Material Specification and Grade","D","D","D",null,null,"Tank Shell and Manway Nozzles ",null,null,"D","Material Specification and Grade",null,null,null,"AAR Device Approval  (If Contractually Specified)","D","D","D"]
[null,"Thickness ","M","M","M",null,null,"Tank Shell and Manway Nozzles ",null,null,"M","Thickness ",null,null,"Spool","Material Specification","D","D","D"]
[null,"Radius (If Applicable)","M","M","M",null,null,"Tank Shell and Manway Nozzles ",null,null,"M","Radius (If Applicable)",null,null,null,"Length Overall","M","M"," M"]
[null,"Rolling Direction (If Applicable)","M","I","I",null,null,"Tank Shell and Manway Nozzles ",null,null,"I","Rolling Direction (If Applicable)",null,null,null,"Flange Dimensions","M","M","M"]
[null,"Material Marking","I","I","I",null,null,"Tank Shell and Manway Nozzles ",null,null,"I","Material Marking",null,null,null,"Mounting Style (Bolted or Threaded)","M","M","I"]
["Gaskets and O-Rings","Material Specification","D","D","D",null,null,"Gaskets and O-Rings","Gaskets and O-Rings",null,"D","Material Specification",null,null,null,"Pipe Dimensions","M","M","M"]
[null,"Marking (if applicable)","D","D","I",null,null,"Gaskets and O-Rings",null,null,"I","Marking (if applicable)",null,null,"Tank Shell and Manway Nozzles ","Certified Mill Test Report","I","D","D"]
[null,"Inside Diameter","M","M","M",null,null,"Gaskets and O-Rings",null,null,"M","Inside Diameter",null,null,null,"Material Specification and Grade","D","D","D"]
[null,"Outside Diameter","M","M","M",null,null,"Gaskets and O-Rings",null,null,"M","Outside Diameter",null,null,null,"Thickness ","M","M","M"]
[null,"Thickness","M","M"," M",null,null,"Gaskets and O-Rings",null,null," M","Thickness",null,null,null,"Radius (If Applicable)","M","M","M"]
["Heat and Pressure Sensors","AAR Device Approval ","D","D","D",null,null,"Heat and Pressure Sensors","Heat and Pressure Sensors",null,"D","AAR Device Approval ",null,null,null,"Rolling Direction (If Applicable)","M","I","I"]
[null,"Model","I","D","D",null,null,"Heat and Pressure Sensors",null,null,"D","Model",null,null,null,"Material Marking","I","I","I"]
[null,"Manufacturing Facility","D","D","D",null,null,"Heat and Pressure Sensors",null,null,"D","Manufacturing Facility",null,null,"GASKETS AND O-RINGS - CTQ INSPECTION CRITERIA"]
[null,"Connection – Flange Dimensions","M","D","M",null,null,"Heat and Pressure Sensors",null,null,"M","Connection – Flange Dimensions",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
[null,"Connection – Thread Specification","M","D","D & M",null,null,"Heat and Pressure Sensors",null,null,"D & M","Connection – Thread Specification",null,null,"M – Measurement Verification Criteria"]
[null,"OEM test certificate","D","D","D",null,null,"Heat and Pressure Sensors",null,null,"D","OEM test certificate"]
["Loading/Unloading, and Sample Valves","AAR Device Approval ","D","D","D",null,null,"Loading/Unloading, and Sample Valves","Loading/Unloading, and Sample Valves",null,"D","AAR Device Approval ",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Model","I","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Model",null,null,"Gaskets and O-Rings","Material Specification","D","D","D"]
[null,"Manufacturing Facility","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Manufacturing Facility",null,null,null,"Marking (if applicable)","D","D","I"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Loading/Unloading, and Sample Valves",null,null,"I","Connection – Flange Dimensions",null,null,null,"Inside Diameter","M","M","M"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Loading/Unloading, and Sample Valves",null,null,"I","Connection – Thread Specification",null,null,null,"Outside Diameter","M","M","M"]
[null,"Body Length","M","D","M",null,null,"Loading/Unloading, and Sample Valves",null,null,"M","Body Length",null,null,null,"Thickness","M","M"," M"]
[null,"Body Diameter","M","D","      M",null,null,"Loading/Unloading, and Sample Valves",null,null,"      M","Body Diameter",null,null,"VALVES AND INSTRUMENTS - CTQ INSPECTION CRITERIA"]
[null,"Port Opening Size","M","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Port Opening Size",null,null,"D – Document Verification (certificates); I – Inspection Verification (Marking); and "]
[null,"Body Material","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Body Material",null,null,"M – Measurement Verification Criteria"]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Loading/Unloading, and Sample Valves",null,null,"I","Lining Material (If Applicable)"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Dimensions",null,null,"Item","Inspection Criteria","Manufacturer","Distributor","Facility"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Material",null,null,"Heat and Pressure Sensors","AAR Device Approval ","D","D","D"]
[null,"OEM test certificate","D","D","D",null,null,"Loading/Unloading, and Sample Valves",null,null,"D","OEM test certificate",null,null,null,"Model","I","D","D"]
["Rupture Disks","Model","I","D","D",null,null,"Rupture Disks","Rupture Disks",null,"D","Model",null,null,null,"Manufacturing Facility","D","D","D"]
[null,"Burst Rating","D","D","D",null,null,"Rupture Disks",null,null,"D","Burst Rating",null,null,null,"Connection – Flange Dimensions","M","D","M"]
[null,"Structural Integrity","M","M","I",null,null,"Rupture Disks",null,null,"I","Structural Integrity",null,null,null,"Connection – Thread Specification","M","D","D & M"]
[null,"Certificate of Test (Per Lot)","D","D","D",null,null,"Rupture Disks",null,null,"D","Certificate of Test (Per Lot)",null,null,null,"OEM test certificate","D","D","D"]
["Spring Loaded Check Valves","AAR Device Approval ","D","D","D",null,null,"Spring Loaded Check Valves","Spring Loaded Check Valves",null,"D","AAR Device Approval ",null,null,null,"AAR Device Approval ","D","D","D"]
[null,"Model","I","D","D",null,null,"Spring Loaded Check Valves",null,null,"D","Model",null,null,null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D ",null,null,"Spring Loaded Check Valves",null,null,"D ","Manufacturing Facility",null,null,"Loading/Unloading, and Sample Valves","Manufacturing Facility","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","M",null,null,"Spring Loaded Check Valves",null,null,"M","Connection – Flange Dimensions",null,null,null,"Connection – Flange Dimensions","M","D","I"]
[null,"Connection – Thread Specification","M","D","D & M",null,null,"Spring Loaded Check Valves",null,null,"D & M","Connection – Thread Specification",null,null,null,"Connection – Thread Specification","M","D","I"]
[null,"Flow Rated Capacity","D","D","D",null,null,"Spring Loaded Check Valves",null,null,"D","Flow Rated Capacity",null,null,null,"Body Length","M","D","M"]
[null,"OEM test certificate","D","D","D",null,null,"Spring Loaded Check Valves",null,null,"D","OEM test certificate",null,null,null,"Body Diameter","M","D","      M"]
["Thermowell","Material Specification","D","D","D",null,null,"Thermowell","Thermowell",null,"D","Material Specification",null,null,null,"Port Opening Size","M","D","D"]
[null,"AAR Device Approval ","D","D","D",null,null,"Thermowell",null,null,"D","AAR Device Approval ",null,null,null,"Body Material","D","D","D"]
[null,"Length Overall","M","M","M",null,null,"Thermowell",null,null,"M","Length Overall",null,null,null,"Lining Material (If Applicable)","D","D","I"]
[null,"Thread Specification","M","M","D & M",null,null,"Thermowell",null,null,"D & M","Thread Specification",null,null,null,"Seal/O-Ring Dimensions","M","D","D"]
[null,"Mounting Style (Bolted or Threaded)","M","M","I",null,null,"Thermowell",null,null,"I","Mounting Style (Bolted or Threaded)",null,null,null,"Seal/O-Ring Material","D","D","D"]
["Vent, Vacuum Relief, and Pressure Relief Valves","AAR Device Approval ","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves","Vent, Vacuum Relief, and Pressure Relief Valves",null,"D","AAR Device Approval ",null,null,null,"OEM test certificate","D","D","D"]
[null,"Model","I","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Model",null,null,null,"Model","I","D","D"]
[null,"Manufacturing Facility","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Manufacturing Facility",null,null,"Rupture Disks","Burst Rating","D","D","D"]
[null,"Connection – Flange Dimensions","M","D","I",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Flange Dimensions",null,null,null,"Structural Integrity","M","M","I"]
[null,"Connection – Thread Specification","M","D","I",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Thread Specification",null,null,null,"Certificate of Test (Per Lot)","D","D","D"]
[null,"Length","M","D","M",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"M","Length",null,null,"Spring Loaded Check Valves","AAR Device Approval ","D","D","D"]
[null,"Body Diameter","M","D","M",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"M","Body Diameter",null,null,null,"Model","I","D","D"]
[null,"Body Material","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Body Material",null,null,null,"Manufacturing Facility","D","D","D "]
[null,"Lining Material (If Applicable)","D","D","I",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Lining Material (If Applicable)",null,null,null,"Connection – Flange Dimensions","M","D","M"]
[null,"Seal/O-Ring Dimensions","M","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Dimensions",null,null,null,"Connection – Thread Specification","M","D","D & M"]
[null,"Seal/O-Ring Material","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Material",null,null,null,"Flow Rated Capacity","D","D","D"]
[null,"Start to Discharge Pressure","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Start to Discharge Pressure",null,null,null,"OEM test certificate","D","D","D"]
[null,"Vapor Tight Pressure","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Vapor Tight Pressure",null,null,null,"Material Specification","D","D","D"]
[null,"Flow Rated Capacity","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Flow Rated Capacity",null,null,"Thermowell","AAR Device Approval ","D","D","D"]
[null,"OEM Test Certificate","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","OEM Test Certificate",null,null,null,"Length Overall","M","M","M"]
[null,"AAR Certificate of Test","D","D","D",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","AAR Certificate of Test",null,null,null,"Thread Specification","M","M","D & M"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material","Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,"D","Certified Mill Test Report",null,null,null,"Mounting Style (Bolted or Threaded)","M","M","I"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"D","Material Specification and Grade",null,null,null,"AAR Device Approval ","D","D","D"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Thickness",null,null,null,"Model","I","D","D"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Radius (If Applicable)",null,null,"Vent, Vacuum Relief, and Pressure Relief Valves","Manufacturing Facility","D","D","D"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Rolling Direction (If Applicable)",null,null,null,"Connection – Flange Dimensions","M","D","I"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Inside Diameter (If Applicable)",null,null,null,"Connection – Thread Specification","M","D","I"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"M","Outside Diameter (If Applicable)",null,null,null,"Length","M","D","M"]
[null,null,null,null,null,null,null,"Reinforcement Pads, Steel Plate, Bar, Tubes and Stub Sill Material",null,null,"I","Material Marking",null,null,null,"Body Diameter","M","D","M"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Body Material","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lining Material (If Applicable)","D","D","I"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Seal/O-Ring Dimensions","M","D","D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Seal/O-Ring Material","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Start to Discharge Pressure","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Vapor Tight Pressure","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Flow Rated Capacity","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OEM Test Certificate","D","D","D"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"AAR Certificate of Test","D","D","D"]

{"sheet":"INSP FORM V4","index":3,"n_rows":233,"n_cols":9,"rows_kept":233,"cut":false,"hidden":true,"merged":[[222,1,226,1],[233,1,233,4],[205,1,208,1],[205,2,208,2],[209,1,215,1],[209,2,215,2],[216,1,221,1],[216,2,221,2],[171,1,175,1],[171,2,175,2],[176,1,188,1],[176,2,188,2],[189,1,204,1],[189,2,204,2],[153,8,154,8],[156,1,162,1],[156,2,162,2],[163,1,170,1],[163,2,170,2],[149,1,155,1],[149,2,155,2],[153,3,154,3],[153,4,154,4],[153,5,154,5],[153,6,154,6],[138,1,142,1],[138,2,142,2],[143,1,148,1],[143,2,148,2],[153,7,154,7],[119,3,120,3],[119,4,120,4],[121,3,122,3],[121,4,122,4],[124,1,137,1],[124,2,137,2],[128,3,129,3],[128,4,129,4],[134,3,135,3],[134,4,135,4],[136,3,137,3],[136,4,137,4],[102,1,106,1],[102,2,106,2],[107,1,112,1],[107,2,112,2],[113,1,123,1],[113,2,123,2],[89,1,94,1],[89,2,94,2],[95,1,97,1],[95,2,97,2],[98,1,101,1],[98,2,101,2],[70,1,75,1],[70,2,75,2],[76,1,82,1],[76,2,82,2],[83,1,88,1],[83,2,88,2],[40,1,51,1],[40,2,51,2],[52,1,61,1],[52,2,61,2],[62,1,69,1],[62,2,69,2],[10,0,16,8],[23,1,23,8],[26,1,31,1],[26,2,31,2],[32,1,39,1],[32,2,39,2]]}
[]
[null,null,null,null,null,null,"Form",null,"RSI-100-05"]
[null,null,null,null,null,null,"Original Date"]
[null,null,null,null,null,null,"Revision Level",null,"VER 7-28-20"]
[null,null,null,null,"Incoming Inspection"]
[null,null,null,null,"Checklist",null,"Revision Date"]
[null,null,null,null,null,null,"Revised By"]
[null,null,null,null,null,null,"Approved By "]
[]
[]
["The tank car facility receiving parts, materials, or components must ensure that the manufactures or distributor provides any requested certificates of conformance, compliance (measurement, testing or mill test reports) required by the purchasing documents that provides the objective evidence that the required inspection points noted in Appendix A of RSI-100 were in fact performed. Each facility is responsible to address the CTC characteristics/requirements identified in Appendix A."]
[]
[]
[]
[]
[]
[]
["Purchasing Document(s): "]
[]
["Brand and Model number:"]
[]
["Facility Part Number: "]
[]
[null,"Inspection Method\nD – Document Verification (certificates)\nI – Inspection Verification (Marking)\nM – Measurement Verification Criteria"]
[]
["SELECT","Item\nInspected","Quantity\nInspected","Insp.\nMethod\n(D, I or M)","Inspection Criteria","Certificate \nProvided\nY/N","Inspection\nPerfromed\nY/N","Pass\nFail\nP/F","Measurement \nEquipment\nID#"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material","Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,"D","Certified Mill Test Report"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"D","Material Specification and Grade"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"M","Thickness Readings"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"M","Radius (If Applicable)"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"I","Rolling Direction (If Applicable)",null,"`"]
["Tank Car Steel Plate, Reinforcement Pads, Bar and Stub Sill Material",null,null,"I","Material Marking"]
["BOLTS","Bolts",null,"D","Material Specification"]
["BOLTS",null,null,"I","Marking"]
["BOLTS",null,null,"D","Thread Specification"]
["BOLTS",null,null,"M","Overall Length"]
["BOLTS",null,null,"M","Length of Threads"]
["BOLTS",null,null,"M","Length of Shoulder"]
["BOLTS",null,null,"M","Diameter"]
["BOLTS",null,null,"M","Head size across flats"]
["Socket Head Cap Screws","Socket Head Cap Screws",null,"D","Material Specification"]
["Socket Head Cap Screws",null,null,"I","Finish (plain, zinc, other)"]
["Socket Head Cap Screws",null,null,"I or D","Marking (if specified)"]
["Socket Head Cap Screws",null,null,"D","Thread Specification"]
["Socket Head Cap Screws",null,null,"M","Overall Length"]
["Socket Head Cap Screws",null,null,"M","Minimum Thread Length"]
["Socket Head Cap Screws",null,null,"M","Head Diameter"]
["Socket Head Cap Screws",null,null,"M","Screw Diameter"]
["Socket Head Cap Screws",null,null,"I","Head Type (plain, knurled)"]
["Socket Head Cap Screws",null,null,"M","Head Chamfer angle (30 or 45 degrees)"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Size"]
["Socket Head Cap Screws",null,null,"M","Nominal Hex Socket Depth"]
["Eyebolts","Eyebolts",null,"D","Material Specification"]
["Eyebolts",null,null,"I","Marking"]
["Eyebolts",null,null,"D","Thread Specification"]
["Eyebolts",null,null,"M","Overall Length"]
["Eyebolts",null,null,"M","Length of Threads"]
["Eyebolts",null,null,"M","Length of Shoulder"]
["Eyebolts",null,null,"M","Diameter"]
["Eyebolts",null,null,"M","Nut length across flats and thickness"]
["Eyebolts",null,null,"M","Nut style square/hex"]
["Eyebolts",null,null,"M","Eyelet ID/OD"]
["Stud Bolts","Stud Bolts",null,"D","Material Specification"]
["Stud Bolts",null,null,"I","Marking"]
["Stud Bolts",null,null,"D","Thread Specification"]
["Stud Bolts",null,null,"M","Overall Length"]
["Stud Bolts",null,null,"M","Length of Threads"]
["Stud Bolts",null,null,"M","Length of Shoulder"]
["Stud Bolts",null,null,"D","Stud end chamfer and radius configuration"]
["Stud Bolts",null,null,"M","Diameter"]
["Nut","Nut",null,"D","Material Specification"]
["Nut",null,null,"I","Marking"]
["Nut",null,null,"D","Thread Specification"]
["Nut",null,null,"M","Length across flats"]
["Nut",null,null,"M","Thickness"]
["Nut",null,null,"I","Style (Square or Hex)"]
["Washer","Washer",null,"D","Material Specification"]
["Washer",null,null,"I","Marking"]
["Washer",null,null,"M","Inside Diameter"]
["Washer",null,null,"M","Outside Diameter"]
["Washer",null,null,"M","Thickness"]
["Washer",null,null,"M","Flatness"]
["Washer",null,null,"I","Style (Flat or Spring or Lock)"]
["Flanges","Flanges",null,"D","Material Specification"]
["Flanges",null,null,"M","Inside Diameter (if required)"]
["Flanges",null,null,"M","Outside Diameter"]
["Flanges",null,null,"M","Thickness"]
["Flanges",null,null,"D","Mounting Style (Flat Face, Raised, or Tongue and Groove)"]
["Flanges",null,null,"I","Machined Characteristics /Gasket Surface"]
["Fittings Plate with no nozzles","Fittings Plate with no nozzles",null,"D","AAR Device Approval (If Contractually Specified)"]
["Fittings Plate with no nozzles",null,null,"D","Material Specification"]
["Fittings Plate with no nozzles",null,null,"D","Thickness"]
["Fittings Plate with no nozzles",null,null,"D","Mounting Style (Opening Style, Flat Face, Raised, or Tongue and Groove)"]
["Fittings Plate with no nozzles",null,null,"M","Gauge tapped threads"]
["Fittings Plate with no nozzles",null,null,"D","Machined Characteristics / Gasket Surface /fitting holes/bolt holes"]
["Pipe Plugs","Pipe Plugs",null,"D","Material Specification"]
["Pipe Plugs",null,null,"D","Thread Specification gauge threads"]
["Pipe Plugs",null,null,"D","Diameter"]
["Bottom Outlet Valve Sump – No Opening","Bottom Outlet Valve Sump – No Opening",null,"D","Material Specification"]
["Bottom Outlet Valve Sump – No Opening",null,null,"I","Marking"]
["Bottom Outlet Valve Sump – No Opening",null,null,"D","Dimensional"]
["Bottom Outlet Valve Sump – No Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Bottom Outlet Valve Saddle – Drain Opening","Bottom Outlet Valve Saddle – Drain Opening",null,"D","AAR Device Approval (If Contractually Specified)"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"D","Material Specification"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Marking"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"D","Dimensional"]
["Bottom Outlet Valve Saddle – Drain Opening",null,null,"I","Structural Integrity (Cracks or Excessive Porosity)"]
["Spool","Spool",null,"D","AAR Device Approval (If Contractually Specified)"]
["Spool",null,null,"D","Material Specification"]
["Spool",null,null,"D","Length Overall"]
["Spool",null,null,"D","Flange Dimensions"]
["Spool",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Spool",null,null,"M","Pipe Dimensions"]
["Fittings Plate with Welded Nozzle(s)","Fittings Plate with Welded Nozzle(s)",null,"D","AAR Device Approval (If Contractually Specified)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Material Specification"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Inside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Outside Diameter"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Thickness"]
["Fittings Plate with Welded Nozzle(s)",null,null,"D","Nozzle Dimensions"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)"]
["Fittings Plate with Welded Nozzle(s)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Machined Characteristics / Gasket Surface /fitting holes/bolt holes/bolt pattern"]
["Fittings Plate with Welded Nozzle(s)"]
["Fittings Plate with Welded Nozzle(s)",null,null,"I","Weld Size and Type"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover","Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,"D","AAR Device Approval (If Contractually Specified)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Material Specification"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Nozzle Dimensions"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"I","Mounting Style (Opening Style, Flat Face, Raised,or Tongue and Groove)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Bolt Pattern"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"I","Weld Size and Type"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Hinge Position"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Bolt Slot Opening Dimensions"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Gasket Groove Dimensions (I.D., O.D., Finish,and Profile)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover",null,null,"D","Special Features (Single Bolt “Kelso” or Submarine Style “Baier”)"]
["Fabricated Hinged and Bolted Manway or Fill Hole Cover"]
["Thermowell","Thermowell",null,"D","Material Specification"]
["Thermowell",null,null,"D","AAR Device Approval"]
["Thermowell",null,null,"D","Length Overall"]
["Thermowell",null,null,"D","Thread Specification"]
["Thermowell",null,null,"I","Mounting Style (Bolted or Threaded)"]
["Hinged and Bolted Nozzle Assembly","Hinged and Bolted Nozzle Assembly",null,"D","Material Specification"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Length Overall"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Thickness"]
["Hinged and Bolted Nozzle Assembly",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Hinge Position"]
["Hinged and Bolted Nozzle Assembly",null,null,"D","Eyebolt Lug Position"]
["Flanged Nozzle","Flanged Nozzle",null,"D","Material Specification"]
["Flanged Nozzle",null,null,"D","Length Overall"]
["Flanged Nozzle",null,null,"D","Diameter"]
["Flanged Nozzle",null,null,"D","Thickness"]
["Flanged Nozzle",null,null,"I","Machined Characteristics / Gasket Surface /fitting holes/bolt holes/ bolt pattern"]
["Flanged Nozzle"]
["Flanged Nozzle",null,null,"I","Weld Size and Type (Forged or Cast)"]
["Eduction Pipe Assembly","Eduction Pipe Assembly",null,"D","Material Specification"]
["Eduction Pipe Assembly",null,null,"D","Length Overall"]
["Eduction Pipe Assembly",null,null,"D","Thread Specification (If Applicable)"]
["Eduction Pipe Assembly",null,null,"D","Diameter"]
["Eduction Pipe Assembly",null,null,"D","Thickness"]
["Eduction Pipe Assembly",null,null,"I","Machined Characteristics"]
["Eduction Pipe Assembly",null,null,"I","Weld Size and Type"]
["Hinged and Bolted Manway Cover","Hinged and Bolted Manway Covers",null,"D","AAR Device Approval (If Contractually Specified)"]
["Hinged and Bolted Manway Cover",null,null,"D","Material Specification"]
["Hinged and Bolted Manway Cover",null,null,"D","Structural Integrity – Pressure Test"]
["Hinged and Bolted Manway Cover",null,null,"I","Thickness (Dished, Flanged, or Grooved)"]
["Hinged and Bolted Manway Cover",null,null,"D","Bolt Pattern"]
["Hinged and Bolted Manway Cover",null,null,"D","Hinge Position"]
["Hinged and Bolted Manway Cover",null,null,"D","Bolt Slot Opening Dimensions"]
["Hinged and Bolted Manway Cover",null,null,"D","Gasket Groove Dimensions"]
["Eduction Pipe Sump","Eduction Pipe Sump",null,"D","Material Specification"]
["Eduction Pipe Sump",null,null,"I","Marking (If Required)"]
["Eduction Pipe Sump",null,null,"D","Dimensions (O.D. and Depth)"]
["Eduction Pipe Sump",null,null,"D","Structural Integrity – Pressure Test"]
["Eduction Pipe Sump",null,null,"M","Thickness"]
["Loading/Unloading, and Sample Valves","Loading/Unloading, and Sample Valves",null,"D","AAR Device Approval"]
["Loading/Unloading, and Sample Valves",null,null,"D","Model"]
["Loading/Unloading, and Sample Valves",null,null,"D","Manufacturing Facility"]
["Loading/Unloading, and Sample Valves",null,null,"I","Connection – Flange Dimensions"]
["Loading/Unloading, and Sample Valves",null,null,"I","Connection – Thread Specification"]
["Loading/Unloading, and Sample Valves",null,null,"D","Body Length"]
["Loading/Unloading, and Sample Valves",null,null,"D","Body Diameter"]
["Loading/Unloading, and Sample Valves",null,null,"D","Port Opening Size"]
["Loading/Unloading, and Sample Valves",null,null,"D","Body Material"]
["Loading/Unloading, and Sample Valves",null,null,"I","Lining Material (If Applicable)"]
["Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Loading/Unloading, and Sample Valves",null,null,"D","Seal/O-Ring Material"]
["Loading/Unloading, and Sample Valves",null,null,"D","OEM test certificate"]
["Vent, Vacuum Relief, and Pressure Relief Valves","Vent, Vacuum Relief, and Pressure Relief Valves",null,"D","AAR Device Approval"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Model"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Manufacturing Facility"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Flange Dimensions"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Connection – Thread Specification"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Length"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Body Diameter"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Body Material"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"I","Lining Material (If Applicable)"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Dimensions"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Seal/O-Ring Material"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Start to Discharge Pressure"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Vapor Tight Pressure"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","Flow Rated Capacity"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","OEM Test Certificate"]
["Vent, Vacuum Relief, and Pressure Relief Valves",null,null,"D","AAR Certificate of Test"]
["Rupture Disks","Rupture Disks",null,"D","Model"]
["Rupture Disks",null,null,"D","Burst Rating"]
["Rupture Disks",null,null,"I","Structural Integrity"]
["Rupture Disks",null,null,"D","Certificate of Test (Per Lot)"]
["Spring Loaded Check Valves","Spring Loaded Check Valves",null,"D","AAR Device Approval"]
["Spring Loaded Check Valves",null,null,"D","Model"]
["Spring Loaded Check Valves",null,null,"D","Manufacturing Facility"]
["Spring Loaded Check Valves",null,null,"D","Connection – Flange Dimensions"]
["Spring Loaded Check Valves",null,null,"D","Connection – Thread Specification"]
["Spring Loaded Check Valves",null,null,"D","Flow Rated Capacity"]
["Spring Loaded Check Valves",null,null,"D","OEM test certificate"]
["Heat and Pressure Sensors","Heat and Pressure Sensors",null,"D","AAR Device Approval"]
["Heat and Pressure Sensors",null,null,"D","Model"]
["Heat and Pressure Sensors",null,null,"D","Manufacturing Facility"]
["Heat and Pressure Sensors",null,null,"D","Connection – Flange Dimensions"]
["Heat and Pressure Sensors",null,null,"D","Connection – Thread Specification"]
["Heat and Pressure Sensors",null,null,"D","OEM test certificate"]
["Gaskets and O-Rings","Gaskets and O-Rings",null,"D","Material Specification"]
["Gaskets and O-Rings",null,null,"I","Marking (if applicable)"]
["Gaskets and O-Rings",null,null,"D","Inside Diameter"]
["Gaskets and O-Rings",null,null,"D","Outside Diameter"]
["Gaskets and O-Rings",null,null,"D","Thickness"]
["A-No Entry"]
[]
[]
[]
[]
[null,"INPSECTOR NAME:",null,null,"SIGNATURE:",null,null,"DATE:"]

{"sheet":"INSP FORM V3","index":4,"n_rows":2,"n_cols":13,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"JULY 9TH 2020"]

{"sheet":"INSP FORM V2","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"ORIG INSP FORM","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}